{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["分部分项工程和单价措施项目清单与计价表","总价措施项目清单与计价表","其他项目清单与计价汇总","规费、税金项目计价表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"分部分项工程和单价措施项目清单与计价表","index":0,"n_rows":201,"n_cols":9,"rows_kept":201,"merged":[[0,0,0,8],[1,0,1,3],[1,4,1,5],[1,6,1,8],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,2,7],[2,8,3,8],[199,0,199,1],[200,0,200,8]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：铜山区城乡供水一体化工程区域供水完善工程施工03标段",{"$nulls":3},"标段：",null,"第 页 共 页"]
["序号","项目编码","项目名称","项目特征描述","计量\r\n单位","工程量","金额(元)",null,"备注"]
[{"$nulls":6},"单价","合价"]
["一"," 土石方工程"]
["1","040101003001","挖基坑土方","1.土壤类别:三类土\n2.挖土深度:2m 内","m3",85754]
[2,"040103002001","余方弃置","1.废弃料品种:余土\n2.运距:3Km内","m3",10266.609999999999]
[3,"040103001001","填方","1.密实度要求:93%\n2.填方材料品种:粘土\n3.回填方式:填土碾压","m3",76399.49]
[4,"040102002001","挖沟槽石方","1.岩石类别:普坚石\n2.开凿深度:2.5m","m3",1831.9]
[5,"040103002002","余方弃置","1.废弃料品种:石方\n2.运距:3Km内","m3",1831.9]
[6,"040103002003","余方弃置","1.废弃料品种:石渣\n2.运距:3Km内","m3",1831.9]
["二","管道敷设"]
[2.1,"开槽埋管"]
[1,"040501003001","铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN800\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",5792]
[2,"040501003001","铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN600\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",5805]
[3,"040501003001","铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN300\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",694]
[4,"040501003002","铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN200\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",10]
[5,"040501002007","钢管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:焊接钢管 D630*9\n3.接口方式:焊接接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",35.1]
[6,"040501002007","钢管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:焊接钢管 D820*10\n3.接口方式:焊接接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",18]
[7,"040501002001","双盘直管","1.名称:钢管\n2.垫层、基础材质及厚度:砂垫层200厚\n3.材质及规格:Q235B D219×6\n4.接口方式:焊接接口\n5.铺设深度:2m\n6.管道检验及试验要求:1.0MPa","m",34]
[8,"040501002008","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、D219*6  L=2000 P=1.0MPa 2根；法兰盘、DN200、4片\n3.接口形式:焊接；","m",10]
[9,"040501002001","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、D219*6  L=2000 P=1.0MPa 2根；法兰盘、DN100、4片\n3.接口形式:焊接；","m",4]
[10,"040501002009","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、D325*8  L=2000 P=1.0MPa 2根；法兰盘、DN300、4片\n3.接口形式:焊接；","m",4]
[11,"040501002005","单盘直管","1.名称:单盘直管\n2.垫层、基础材质及厚度:砂垫层200厚\n3.材质及规格:Q235B D219×6 L=2m 共1根\n4.接口方式:焊接接口\n5.铺设深度:2m\n6.管道检验及试验要求:0.8MPa\n7.法兰盘材质、规格、形式:Q235B、DN200、单盘平焊法兰\n8.连接方式:电弧焊","m",4]
[12,"031201001001","管道刷油","1.除锈级别:喷砂除锈sa2.5级\n2.油漆品种:CZ-2型新型高分子饮水防腐涂料\n3.管道内壁防腐（二底二面）:先刷GZ-2底漆一道，面漆一道，然后刷底漆一道，再涂面漆一道，2道底漆干膜厚度大于100μm，2道面漆干膜厚度大于120μm，总干膜厚度大于200μm。","m2",114.68]
[13,"031201001002","管道刷油","1.除锈级别:喷砂除锈sa2.5级\n2.油漆品种:CZ-2型新型高分子饮水防腐涂料\n3.管道外壁防腐（二布四油）:先刷GZ-2底漆一道，缠绕玻璃纤维布一层，再涂底漆一道，再缠绕玻璃纤维布一层，再涂面漆两道，干膜厚度大于420μm。\n4.玻璃纤维布:采用10*10中碱无蜡玻璃丝布","m2",114.68]
[2.2,"牵引管"]
[1,"040501008008","水平导向钻进","1.土壤类别:三类土\n2.材质及规格:PE100管 SDR11 De710\n3.一次成孔长度:132m","m",132]
[2,"040501008001","水平导向钻进","1.土壤类别:三类土\n2.材质及规格:PE100管 SDR11 dn355\n3.一次成孔长度:109m","m",109]
[2.3,"倒虹管、过河道包封、预留管过小沟\n"]
[1,"040305005001","护底","1.材料品种:C25混凝土\n2.结构形式:预拌\n3.厚度:20cm\n4.垫层材料、厚度:砂石混合料、10cm","m2",327.9]
[2,"040305005002","护坡","1.材料品种:C25混凝土\n2.结构形式:预拌\n3.厚度:15cm\n4.垫层材料、厚度:砂石混合料、10cm","m2",788.67]
[3,"040303016001","格梗","1.混凝土强度等级:C25","m3",101.58]
[4,"040503002003","管道包封","1.垫层材质、厚度:C25砼垫层、200mm\n2.混凝土强度等级:C25","m3",283.59000000000003]
[5,"040901001002","现浇构件钢筋","1.钢筋种类:HRB400\n2.钢筋规格:10以外","t",22.63]
[6,"041103001002","围堰","土方","m3",4062.92]
[7,"041103001003","围堰","编制袋土","m3",284.40999999999997]
["三","管道附属构筑物"]
[3.1,"混凝土支墩"]
[1,"040503002002","混凝土支墩","1.混凝土强度等级:C25","m3",281.46999999999997]
[2,"040305001001","垫层","1.材料品种、规格:碎石\n2.厚度:20cm","m3",27.63]
[3,"040901001001","现浇构件钢筋","1.钢筋种类:HRB400\n2.钢筋规格:10以内","t",1.9]
[3.2,"标识桩"]
[1,"040205018002","警示柱","1.类型:标识桩\n2.材料品种:C25砼\n3.规格、型号:170×170mm、高700mm\n4.基础材料、尺寸:C25砼、400×400mm、高200mm\n5.钢筋种类、规格:HPB30、HRB400；10以内、10以外","根",148]
[3.3,"管道包封"]
[1,"040503002004","管道包封","1.垫层材质、厚度:C15砼垫层、300mm\n2.混凝土强度等级:C25","m3",7.2]
[2,"040901001001","现浇构件钢筋","1.钢筋种类:HRB400\n2.钢筋规格:10以外","t",0.24]
["四","管件安装"]
[1,"040502007003","盲堵板制作、安装","1.名称：法兰盲板\n2.材质规格：球墨铸铁 DN800","个",1]
[2,"040502007003","盲堵板制作、安装","1.名称：法兰盲板\n2.材质规格：球墨铸铁 DN200","个",3]
[3,"040502001021","铸铁管管件","1.种类:盘承短管\n2.材质及规格:球墨铸铁 DN800\n3.接口形式:胶圈接口","个",1]
[4,"040502001035","铸铁管管件","1.种类:盘插短管\n2.材质及规格:球墨铸铁 DN800\n3.接口形式:胶圈接口","个",1]
[5,"040502001021","铸铁管管件","1.种类:盘承短管\n2.材质及规格:球墨铸铁 DN600\n3.接口形式:胶圈接口","个",8]
[6,"040502001035","铸铁管管件","1.种类:盘插短管\n2.材质及规格:球墨铸铁 DN600\n3.接口形式:胶圈接口","个",8]
[7,"040502001036","铸铁管管件","1.种类:45°弯头\n2.材质及规格:球墨铸铁、DN800\n3.接口形式:胶圈接口","个",1]
[8,"040502001036","铸铁管管件","1.种类:11.25°弯头\n2.材质及规格:球墨铸铁、DN600\n3.接口形式:胶圈接口","个",12]
[9,"040502001037","铸铁管管件","1.种类:22.5° 弯头\n2.材质及规格:球墨铸铁、DN600\n3.接口形式:胶圈接口","个",2]
[10,"040502001038","铸铁管管件","1.种类:90°弯头\n2.材质及规格:球墨铸铁、DN600\n3.接口形式:胶圈接口","个",1]
[11,"040502001002","铸铁管管件","1.种类:插堵\n2.材质及规格:球墨铸铁 DN300\n3.接口形式:胶圈接口","个",1]
[12,"040502001003","铸铁管管件","1.种类:盘插短管\n2.材质及规格:球墨铸铁 DN300\n3.接口形式:胶圈接口","个",1]
[13,"040502001013","铸铁管管件","1.种类:盘承短管\n2.材质及规格:球墨铸铁 DN300\n3.接口形式:胶圈接口","个",1]
[14,"040502001016","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN300*200\n3.接口形式:橡胶圈","个",1]
[15,"040502001014","铸铁管管件","1.种类:钢塑转换管件\n2.材质及规格:DN300","个",2]
[16,"040502001015","铸铁管管件","1.种类:闷板\n2.材质及规格:球墨铸铁 DN200","个",1]
[17,"040502004003","钢塑转换接头","1.材质及规格:PE100,dn630\n2.接口形式:热熔","个",2]
[18,"040502002004","钢管管件制作、安装","1.种类:30°弯头\n2.材质及规格:Q235B D820*10\n3.接口形式:焊接","个",4]
[19,"040502002004","钢管管件制作、安装","1.种类:30°弯头\n2.材质及规格:Q235B D630×8 La=170\n3.接口形式:焊接","个",10]
[20,"040502002008","钢管管件制作、安装","1.种类:60°弯头\n2.材质及规格:Q235B D630×8 La=170\n3.接口形式:焊接","个",2]
[21,"040502001030","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁、DN800XDN200\n3.接口形式:胶圈接口","个",1]
[22,"040502001037","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁、DN800XDN300\n3.接口形式:胶圈接口","个",1]
[23,"040502001030","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁、DN600XDN200\n3.接口形式:胶圈接口","个",3]
[24,"040502007004","盲堵板制作、安装","1.名称：法兰承堵\n2.材质规格：球墨铸铁 DN600","个",1]
[25,"040502007004","盲堵板制作、安装","1.名称：法兰闷板\n2.材质规格：球墨铸铁 DN200","个",1]
[26,"040502007005","盲堵板制作、安装","1.名称：法兰闷板\n2.材质规格：球墨铸铁 DN300","个",1]
[27,"040502002009","钢管管件制作、安装","1.种类:30°弯头\n2.材质及规格:Q235B D219*6\n3.接口形式:焊接","个",4]
["五","阀门井安装"]
[5.1,"DN250预留支管水表井"]
[1,"040502008008","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D=325、L=300","个",20]
[2,"040502009004","水表","1.规格:DN250\n2.安装方式:含蝶阀2个，止回阀1个，水表1个，伸缩节1个，压力表1个，法兰连接","组",10]
[5.2,"DN300预留支管水表井"]
[1,"040502008006","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D=377、L=300","个",2]
[2,"040502009002","水表","1.规格:DN300\n2.安装方式:含蝶阀2个，止回阀1个，水表1个，法兰连接","组",1]
[5.3,"DN200预留支管水表井"]
[1,"040502008006","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D=273、L=300","个",28]
[2,"040502009002","水表","1.规格:DN200\n2.安装方式:含蝶阀2个，止回阀1个，水表1个，法兰连接","组",14]
[5.4,"DN150预留支管水表井"]
[1,"040502008007","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D=209、L=300","个",22]
[2,"040502009003","水表","1.规格:DN150\n2.安装方式:含蝶阀2个，止回阀1个，水表1个，伸缩节1个，压力表1个，法兰连接","组",11]
[5.5,"DN800排泥阀井"]
[1,"040502001001","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN800*250\n3.接口形式:橡胶圈","个",4]
[2,"040502005001","阀门","1.种类:手动闸阀\n2.材质及规格:铸铁、DN250\n3.连接方式:法兰连接","个",4]
[3,"040502008001","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D=325、L=300\n2.管内填料材质:沥青麻丝","个",8]
[4,"040501002003","短管","1.种类:短管\n2.材质及规格:钢管、DN273*8  L=5000 1根 P=1.0MPa；\n3.接口形式:焊接；","m",20]
[5,"040501002005","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、D273*8  L=2000 P=1.0MPa；法兰盘、DN250、2片\n3.接口形式:焊接","m",8]
[6,"040501002006","单盘短管","1.种类:单盘短管\n2.材质及规格:钢管、D273*8  L=2000 P=1.0MPa；法兰盘、DN250、1片\n3.接口形式:焊接","m",8]
[5.6,"DN800排气阀井"]
[1,"040502001002","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁 DN800*100 P=1.0MPa；","个",14]
[2,"040502008002","套管制作、安装","1.形式、材质及规格:D880*10 防水套管、Q235B、D=880 L=300","个",28]
[3,"040502005002","阀门","1.种类:手动蝶阀\n2.材质及规格:DN100 L=127 P=1.0MPa\n3.连接方式:法兰连接","个",14]
[4,"040502005003","阀门","1.种类:复合排气阀\n2.材质及规格:铸铁、DN100\n3.连接方式:法兰连接","个",14]
[5,"040501002004","双盘短管","1.种类:双盘短管\n2.材质及规格:Q235B D108x6  L=200 1根；法兰盘、DN100、2片\n3.接口形式:焊接","m",2.8]
[5.7,"DN800排水井"]
[1,"040502001003","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN800*250\n3.接口形式:橡胶圈","个",2]
[2,"040502005008","阀门","1.种类:手动闸阀\n2.材质及规格:铸铁、DN250\n3.连接方式:法兰连接","个",2]
[3,"040502008007","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D=325、L=300\n2.管内填料材质:沥青麻丝","个",4]
[4,"040501002010","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、D273*8  L=2000 P=1.0MPa；法兰盘、DN250、2片\n3.接口形式:焊接","m",2]
[5,"040501002011","单盘短管","1.种类:单盘短管\n2.材质及规格:钢管、D273*8  L=2000 P=1.0MPa；法兰盘、DN250、1片\n3.接口形式:焊接","m",2]
[5.8,"DN800蝶阀井"]
[1,"040502008004","套管制作、安装","1.形式、材质及规格:D880*10 防水套管、Q235B、D=880 L=400","个",6]
[2,"040502005006","阀门","1.种类:手动卧式蝶阀\n2.材质及规格:DN800 L=318\n3.连接方式:法兰连接","个",3]
[3,"040502005007","阀门","1.种类:限位伸缩器\n2.材质及规格:DN800 L=600\n3.连接方式:法兰连接","个",3]
[4,"040501002008","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、D820*10  L=3000 P=1.0MPa；法兰盘、DN800、2片\n3.接口形式:焊接","m",18]
[5.9,"DN600排泥阀井"]
[1,"040502001001","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN600*200\n3.接口形式:橡胶圈","个",3]
[2,"040502005001","阀门","1.种类:手动闸阀\n2.材质及规格:铸铁、DN200\n3.连接方式:法兰连接","个",3]
[3,"040502008001","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D=273、L=300\n2.管内填料材质:沥青麻丝","个",6]
[4,"040501002003","短管","1.种类:短管\n2.材质及规格:钢管、D219*6  L=5000 1根 P=1.0MPa；\n3.接口形式:焊接；","m",15]
[5,"040501002005","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、DN219*6  L=2000 P=1.0MPa；法兰盘、DN200、2片\n3.接口形式:焊接","m",6]
[6,"040501002006","单盘短管","1.种类:单盘短管\n2.材质及规格:钢管、DN219*6  L=2000 P=1.0MPa；法兰盘、DN200、2片\n3.接口形式:焊接","m",6]
[7,"040501002007","短管","1.种类:短管\n2.材质及规格:钢管、DN219*6  P=1.0MPa；\n3.接口形式:焊接","m",15]
[{"v":5.1,"d":"5.10"},"DN600排气阀井"]
[1,"040502001002","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁 DN600×80 P=1.0MPa；","个",6]
[2,"040502008002","套管制作、安装","1.形式、材质及规格:D690×10 防水套管、Q235B、D =690 L=300","个",12]
[3,"040502005002","阀门","1.种类:手动蝶阀\n2.材质及规格:DN80 L=114 P=1.0MPa\n3.连接方式:法兰连接","个",6]
[4,"040501002004","双盘短管","1.种类:双盘短管\n2.材质及规格:Q235B D89x6  L=200 1根；法兰盘、DN80、2片\n3.接口形式:焊接","m",1.2]
[5,"040502005003","阀门","1.种类:复合排气阀\n2.材质及规格:铸铁、DN80\n3.连接方式:法兰连接","个",6]
[5.11,"DN600蝶阀井"]
[1,"040502008004","套管制作、安装","1.形式、材质及规格:D690*10防水套管、Q235B、D =690 L=300","个",6]
[2,"040502005006","阀门","1.种类:手动卧式蝶阀\n2.材质及规格:DN600 L=267\n3.连接方式:法兰连接","个",3]
[3,"040502005007","阀门","1.种类:限位伸缩器\n2.材质及规格:DN600 L=370\n3.连接方式:法兰连接","个",3]
[4,"040501002008","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、DN630*8  L=2000 P=1.0MPa；法兰盘、DN600、2片\n3.接口形式:焊接","m",12]
[5.12,"DN300排泥阀井"]
[1,"040502001001","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN300*100\n3.接口形式:橡胶圈","个",1]
[2,"040502005001","阀门","1.种类:手动闸阀\n2.材质及规格:铸铁、DN100\n3.连接方式:法兰连接","个",1]
[3,"040502008001","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D159×4.5、L=300\n2.管内填料材质:沥青麻丝","个",2]
[4,"040501002003","双盘短管","1.种类:双盘短管\n2.材质及规格:钢管、DN108×6  L=2000 P=1.0MPa；法兰盘、DN100、2片\n3.接口形式:焊接；","m",2]
[5,"040501002005","单盘短管","1.种类:单盘短管\n2.材质及规格:钢管、DN108×6  L=2000 P=1.0MPa；法兰盘、DN100、2片\n3.接口形式:焊接；","m",2]
[6,"040501002006","短管","1.种类:短管\n2.材质及规格:钢管、DN108×6  P=1.0MPa；\n3.接口形式:焊接；","m",10]
[5.13,"DN300排气阀井"]
[1,"040502001002","铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁 DN300*80 P=1.0MPa；","个",1]
[2,"040502008002","套管制作、安装","1.形式、材质及规格:D377*10 防水套管、Q235B、D377 L=300","个",2]
[3,"040502005002","阀门","1.种类:手动蝶阀\n2.材质及规格:DN80 L=114 P=1.0MPa\n3.连接方式:法兰连接","个",1]
[4,"040501002004","双盘短管","1.种类:双盘短管\n2.材质及规格:Q235B D89x6  L=200 1根；法兰盘、DN80、2片\n3.接口形式:焊接","m",0.2]
[5,"040502005003","阀门","1.种类:复合排气阀\n2.材质及规格:铸铁、DN80\n3.连接方式:法兰连接","个",1]
[5.14,"DN300闸阀井"]
[1,"040502008004","套管制作、安装","1.形式、材质及规格:D377*10 防水套管、Q235B、D =377 L=300","个",2]
[2,"040502005006","阀门","1.种类:手动闸阀\n2.材质及规格:DN300\n3.连接方式:法兰连接","个",1]
[3,"040501002007","双盘短管","1.种类:双盘短管\n2.材质及规格:Q235B DN325*8  L=2000 2根；法兰盘、DN80、4片\n3.接口形式:焊接","m",4]
[5.15,"DN200水表井"]
[1,"040502008005","套管制作、安装","1.形式、材质及规格:防水套管、Q235B、D159*4.5、L=300\n2.管内填料材质:沥青麻丝","个",2]
[2,"040502009001","水表","1.规格:DN200\n2.安装方式:含蝶阀2个，止回阀1个，水表1个，法兰连接","组",1]
["六","阀门井土建"]
[1,"040504002004","混凝土井","1.井名称及规格:预留支管井、2750×1300\n2.垫层、基础材质及厚度:砼垫层、C15、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷","座",25]
[2,"040504002005","混凝土井","1.井名称及规格:预留支管井、3200×1300\n2.垫层、基础材质及厚度:砼垫层、C15、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷","座",11]
[3,"040504002013","混凝土井","1.井名称及规格:蝶阀井2200*3000\n2.垫层、基础材质及厚度:砼垫层、C25、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖、防坠网\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷\n8.详见图纸设计","座",3]
[4,"040504002005","混凝土井","1.井名称及规格:排气阀井、1400*1400\n2.垫层、基础材质及厚度:砼垫层、C25、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖、防坠网\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷\n8.详见图纸设计","座",14]
[5,"040504002007","混凝土井","1.井名称及规格:排泥及泄水阀门井、1300×1300\n2.垫层、基础材质及厚度:砼垫层、C25、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖、防坠网\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷\n8.详见图纸设计","座",8]
[6,"040504001001","砌筑井","1.井名称及规格:砖砌排泥井 Φ1000\n2.垫层、基础材质及厚度:砼垫层、C25、10cm\n3.盖板材质、规格:钢筋砼\n4.井盖、井圈材质及规格:Φ700三防铸铁井盖、防坠网\n5.踏步材质、规格:塑钢\n6.防渗、防水要求:防水砂浆粉刷\n7.详见图纸设计","座",8]
[7,"040504002013","混凝土井","1.井名称及规格:蝶阀井1800*2600\n2.垫层、基础材质及厚度:砼垫层、C25、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖、防坠网\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷\n8.详见图纸设计","座",3]
[8,"040504002005","混凝土井","1.井名称及规格:排气阀井、1200*1200\n2.垫层、基础材质及厚度:砼垫层、C25、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖、防坠网\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷\n8.详见图纸设计","座",7]
[9,"040504002006","混凝土井","1.井名称及规格:排泥阀门井、1100*1100\n2.垫层、基础材质及厚度:砼垫层、C25、10cm\n3.混凝土强度等级:C25\n4.盖板材质、规格:钢筋砼\n5.井盖、井圈材质及规格:Φ700三防铸铁井盖、防坠网\n6.踏步材质、规格:塑钢\n7.防渗、防水要求:防水砂浆粉刷\n8.详见图纸设计","座",1]
["七","道路破坏与恢复"]
[1,"081201001001","拆除路面","1.材质:混凝土路面\n2.厚度:20cm","m3",930]
[2,"081201002001","拆除基层","1.材质:二灰结石\n2.厚度:40cm","m3",1860]
[3,"040202002001","路面基层恢复","1.含灰量:5%\n2.厚度:40cm","m2",4650]
[4,"040203007001","水泥混凝土","1.混凝土强度等级:C30\n2.厚度:20cm","m2",4650]
["八","管桥"]
[8.1,"毛庄南中沟管桥"]
[1,"040301004001","泥浆护壁成孔灌注桩","1.地层情况:砂砾\n2.空桩长度、桩长:H ≤ 20m\n3.桩径:Φ≤800\n4.成孔方法:回旋钻机钻孔\n5.混凝土种类、强度等级:C30","m",20.64]
[2,"040303002001","混凝土基础","1.混凝土强度等级:C30","m3",0.96]
[3,"040303005001","混凝土墩(台）身","1.部位:墩(台)身\n2.混凝土强度等级:C30","m3",3.39]
[4,"040501006001","管道架空跨越","1.管道架设高度:4.02\n2.管道材质及规格:Q235b、钢板卷管、D630×10\n3.接口方式:焊接接口\n4.固定及连接材料:固定工字钢10#、L=1.5m×4；连接角钢L50×6、L=0.97m×2；16厚钢板","m",35.4]
[5,"040502002002","钢管管件制作、安装","1.种类:30°弯头\n2.材质及规格:Q235B D630×8 La=170\n3.接口形式:焊接","个",4]
[6,"040502005003","阀门","1.种类:手动蝶阀\n2.材质及规格:DN80 L=114 P=1.0MPa\n3.连接方式:法兰连接","个",1]
[7,"040501002001","双盘短管","1.种类:双盘短管\n2.材质及规格:Q235B D89x6  L=200 1根；法兰盘、DN80、2片\n3.接口形式:焊接","m",0.2]
[8,"040502005004","阀门","1.种类:复合排气阀\n2.材质及规格:铸铁、DN80\n3.连接方式:法兰连接","个",1]
[9,"040901001003","现浇构件钢筋","1.钢筋种类:HRB400\n2.钢筋规格:10以外","t",1.816]
[10,"040901004001","钢筋笼","1.钢筋种类:Q235B、HPB300、HRB500\n2.钢筋规格:10以内、10以外","t",1.35]
[11,"040503002003","混凝土支墩","1.垫层材质、厚度:C20砼、10cm\n2.混凝土强度等级:C25","m3",5.66]
[12,"031201001001","管道刷油","1.除锈级别:喷砂除锈sa2.5级\n2.油漆品种:CZ-2型新型高分子饮水防腐涂料\n3.管道内壁防腐（二底二面）:先刷GZ-2底漆一道，面漆一道，然后刷底漆一道，再涂面漆一道，2道底漆干膜厚度大于100μm，2道面漆干膜厚度大于120μm，总干膜厚度大于200μm。","m2",69.31]
[13,"031201001002","管道刷油","1.除锈级别:喷砂除锈sa2.5级\n2.油漆品种:CZ-2型新型高分子饮水防腐涂料\n3.管道内壁防腐（二底三面）:先刷GZ-2底漆一道，面漆一道，然后刷底漆一道，再涂面漆二道，2道底漆干膜厚度大于100μm，3道面漆干膜厚度大于180μm，总干膜厚度大于280μm。","m2",69.31]
[8.2,"藕河管桥"]
[1,"040301004002","泥浆护壁成孔灌注桩","1.地层情况:砂砾\n2.空桩长度、桩长:H ≤ 20m\n3.桩径:Φ≤800\n4.成孔方法:回旋钻机钻孔\n5.混凝土种类、强度等级:C30","m",32.6]
[2,"040303002002","混凝土基础","1.混凝土强度等级:C30","m3",1.92]
[3,"040303005002","混凝土墩(台）身","1.部位:墩(台)身\n2.混凝土强度等级:C30","m3",6.78]
[4,"040501006003","管道架空跨越","1.管道架设高度:3.85\n2.管道材质及规格:Q235b、钢板卷管、D630×10\n3.接口方式:焊接接口\n4.固定及连接材料:固定工字钢10#、L=1.5m×8；连接角钢L50×6、L=0.97m×4；16厚钢板","m",46.3]
[5,"040502002001","钢管管件制作、安装","1.种类:30°弯头\n2.材质及规格:Q235B D630×8 La=170\n3.接口形式:焊接","个",4]
[6,"040502005005","阀门","1.种类:手动蝶阀\n2.材质及规格:DN80 L=114 P=1.0MPa\n3.连接方式:法兰连接","个",1]
[7,"040501002002","双盘短管","1.种类:双盘短管\n2.材质及规格:Q235B D89×6  L=200 1根；法兰盘、DN80、2片\n3.接口形式:焊接","m",0.2]
[8,"040502005006","阀门","1.种类:复合排气阀\n2.材质及规格:铸铁、DN80\n3.连接方式:法兰连接","个",1]
[9,"040901001004","现浇构件钢筋","1.钢筋种类:HRB400\n2.钢筋规格:10以外","t",3.631]
[10,"040901004002","钢筋笼","1.钢筋种类:Q235B、HPB300、HRB500\n2.钢筋规格:10以内、10以外","t",2.699]
[11,"040503002005","混凝土支墩","1.垫层材质、厚度:C20砼、10cm\n2.混凝土强度等级:C25","m3",5.66]
[12,"031201001003","管道刷油","1.除锈级别:喷砂除锈sa2.5级\n2.油漆品种:CZ-2型新型高分子饮水防腐涂料\n3.管道内壁防腐（二底二面）:先刷GZ-2底漆一道，面漆一道，然后刷底漆一道，再涂面漆一道，2道底漆干膜厚度大于100μm，2道面漆干膜厚度大于120μm，总干膜厚度大于200μm。","m2",90.14]
[13,"031201001004","管道刷油","1.除锈级别:喷砂除锈sa2.5级\n2.油漆品种:CZ-2型新型高分子饮水防腐涂料\n3.管道内壁防腐（二底三面）:先刷GZ-2底漆一道，面漆一道，然后刷底漆一道，再涂面漆二道，2道底漆干膜厚度大于100μm，3道面漆干膜厚度大于180μm，总干膜厚度大于280μm。","m2",90.14]
["九","村级加压站"]
[null,"D","加压站土建","1.类型:供水加压站砖混结构\n2.规格:单座面积40m2\n3.高度:建筑高度4m\n4.混凝土强度等级:C30","座",22]
["十","单价措施项目"]
[null,"041107002001","排水、降水",null,"昼夜",210]
["合计"]
["注：1、工程中所涉及的水表为远传智能水表。                                                                           2、施工中除球墨铸铁的管材、管件、阀门、智能水表外，其余所需材料均由施工单位制作或购置。                                              3、钢管、PE管连接附件包含在其投标报价中。"]

{"sheet":"总价措施项目清单与计价表","index":1,"n_rows":20,"n_cols":12,"rows_kept":20,"merged":[[0,0,0,12],[1,0,1,6],[1,7,1,9],[1,10,1,12],[2,2,2,3],[2,6,2,8],[2,11,2,12],[3,2,3,3],[3,6,3,8],[3,11,3,12],[4,2,4,3],[4,6,4,8],[4,11,4,12],[5,2,5,3],[5,6,5,8],[5,11,5,12],[6,2,6,3],[6,6,6,8],[6,11,6,12],[7,2,7,3],[7,6,7,8],[7,11,7,12],[8,2,8,3],[8,6,8,8],[8,11,8,12],[9,2,9,3],[9,6,9,8],[9,11,9,12],[10,2,10,3],[10,6,10,8],[10,11,10,12],[11,2,11,3],[11,6,11,8],[11,11,11,12],[12,2,12,3],[12,6,12,8],[12,11,12,12],[13,2,13,3],[13,6,13,8],[13,11,13,12],[14,2,14,3],[14,6,14,8],[14,11,14,12],[15,2,15,3],[15,6,15,8],[15,11,15,12],[16,2,16,3],[16,6,16,8],[16,11,16,12],[17,0,17,12],[18,5,18,12],[19,0,19,2],[19,8,19,11]],"flags":["formulas_cached_only"]}
["总价措施项目清单与计价表"]
["工程名称：铜山区城乡供水一体化工程区域供水完善工程施工03标段",{"$nulls":6},"标段：",null,null,"第1页 共1页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["1","041109001001","安全文明施工费",null,null,""]
["1.1",null,"基本费",null,"分部分项合计+单价措施项目合计-设备费","1.500"]
["1.2",null,"增加费",null,"分部分项合计+单价措施项目合计-设备费",""]
["2","041109002001","夜间施工",null,"分部分项合计+单价措施项目合计-设备费",""]
["3","041109003001","二次搬运",null,"分部分项合计+单价措施项目合计-设备费",""]
["4","041109004001","冬雨季施工",null,"分部分项合计+单价措施项目合计-设备费",""]
["5","041109005001","行车、行人干扰",null,"分部分项合计+单价措施项目合计-设备费",""]
["6","041109006001","地上、地下设施、建筑物的临时保护设施",null,"分部分项合计+单价措施项目合计-设备费",""]
["7","041109007001","已完工程及设备保护",null,"分部分项合计+单价措施项目合计-设备费",""]
["8","041109008001","临时设施",null,"分部分项合计+单价措施项目合计-设备费",""]
["9","041109009001","赶工措施",null,"分部分项合计+单价措施项目合计-设备费",""]
["10","041109010001","工程按质论价",null,"分部分项合计+单价措施项目合计-设备费",""]
["11","041109011001","特殊条件下施工增加费",null,"分部分项合计+单价措施项目合计-设备费",""]
[]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.1】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]

{"sheet":"其他项目清单与计价汇总","index":2,"n_rows":13,"n_cols":5,"rows_kept":13,"merged":[[0,0,0,4],[1,0,1,2],[10,2,10,4],[12,0,12,2],[12,3,12,4]],"flags":["formulas_cached_only"]}
["其他项目清单与计价汇总表"]
["工程名称：铜山区城乡供水一体化工程区域供水完善工程施工03标段",null,null,"标段：","第1页 共1页"]
["序号","项目名称","金额（元）","结算金额（元）","备注"]
["1","暂列金额",null,{"v":1080000,"d":"1080000.00"}]
["2","暂估价"]
["2.1","材料(工程设备)暂估价"]
["2.2","专业工程暂估价"]
["3","计日工"]
["4","总承包服务费"]
["5","索赔与现场签证"]
[null,null,"【新点2013清单造价江苏版 V10.3.1】"]
[]
["编制人（造价人员）：",null,null,"复核人（造价工程师）："]

{"sheet":"规费、税金项目计价表","index":3,"n_rows":31,"n_cols":10,"rows_kept":31,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,6],[1,7,1,10],[2,2,2,5],[2,6,2,7],[2,9,2,10],[3,2,3,5],[3,6,3,7],[3,9,3,10],[4,2,4,5],[4,6,4,7],[4,9,4,10],[5,2,5,5],[5,6,5,7],[5,9,5,10],[6,2,6,5],[6,6,6,7],[6,9,6,10],[7,2,7,5],[7,6,7,7],[7,9,7,10],[8,2,8,5],[8,6,8,7],[8,9,8,10],[9,2,9,5],[9,6,9,7],[9,9,9,10],[10,2,10,5],[10,6,10,7],[10,9,10,10],[11,2,11,5],[11,6,11,7],[11,9,11,10],[12,2,12,5],[12,6,12,7],[12,9,12,10],[13,2,13,5],[13,6,13,7],[13,9,13,10],[14,2,14,5],[14,6,14,7],[14,9,14,10],[15,2,15,5],[15,6,15,7],[15,9,15,10],[16,2,16,5],[16,6,16,7],[16,9,16,10],[17,2,17,5],[17,6,17,7],[17,9,17,10],[18,2,18,5],[18,6,18,7],[18,9,18,10],[19,2,19,5],[19,6,19,7],[19,9,19,10],[20,2,20,5],[20,6,20,7],[20,9,20,10],[21,2,21,5],[21,6,21,7],[21,9,21,10],[22,2,22,5],[22,6,22,7],[22,9,22,10],[23,2,23,5],[23,6,23,7],[23,9,23,10],[24,2,24,5],[24,6,24,7],[24,9,24,10],[25,2,25,5],[25,6,25,7],[25,9,25,10],[27,0,27,8],[27,9,27,10],[29,3,29,10],[30,0,30,2],[30,5,30,9]],"flags":["formulas_cached_only"]}
["规费、税金项目计价表"]
["工程名称：铜山区城乡供水一体化工程区域供水完善工程施工03标段",{"$nulls":3},"标段：",null,null,"第1页 共1页"]
["序号","项目名称","计算基础",{"$nulls":3},"计算基数(元)",null,"计算费率(％)","金额(元)"]
["1","规费","工程排污费+社会保险费+住房公积金",{"$nulls":5},"100.000"]
["1.1","社会保险费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"2.000"]
["1.2","住房公积金","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"0.340"]
["1.3","工程排污费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},""]
["2","税金","分部分项工程费+措施项目费+其他项目费+规费-除税甲供材料和甲供设备费/1.01",{"$nulls":5},"11.000"]
{"$rows_empty":19}
["合  计"]
[]
[{"$nulls":3},"【新点2013清单造价江苏版 V10.3.1】"]
["编制人（造价人员）：",{"$nulls":4},"复核人（造价工程师）："]