{"text_format":"3","workbook":"xls","n_sheets":101,"sheets":["汇总","顺河镇王寨村王寨东桥","顺河镇张口村张口南2桥","顺河镇白庙村孙庄桥","顺河镇大圣村裴庄北桥","顺河镇焦庄村周庄北桥","顺河镇王寨村李庄东桥","顺河镇李庄村河申北桥","顺河镇顺河村周屯南桥","顺河镇白庙村白庙新村前桥","顺河镇朱坑村康庄后桥","顺河镇大圣村黄庄东桥","顺河镇土屯村王双楼东桥","顺河镇张口村张口南1桥","顺河镇范庄村范庄西桥","顺河镇范庄村范庄中桥","顺河镇范庄村范庄北桥","顺河镇杨楼村后杨楼北桥","顺河镇杨楼村后杨楼西北桥","顺河镇岳庄村岳草楼东桥","顺河镇渠寨村季庄前桥","顺河镇大圣村大圣西桥","顺河镇焦庄村周庄西桥","顺河镇焦庄村焦庄东桥","王沟镇周庄寨村袁庄北桥","王沟镇王大庄村育才小学西桥","王沟镇孙许庄东南桥","王沟镇邵楼村邵楼西北桥","王沟镇王老家村前老鹤寺西北桥","王沟镇刘小集村杨楼西南桥","王沟镇王大庄村王楼东桥","王沟镇丁楼东北桥","王沟镇丁楼东桥","王沟镇丁楼东桥王大庄村朱阁南桥","王沟镇王大庄村王大庄西桥","王沟镇李溜村赵庄东桥","王沟镇李溜村丁庄北桥","王沟镇前王老家西南桥","王沟镇后王老家西南桥","王沟镇王老家村圣举鸭厂桥","王沟镇刘小集村代楼中队北桥","王沟镇常楼北桥","王沟镇石洼西南桥","王沟镇刘菜园村北蒋集桥","王沟镇李溜村圣达厂东北桥","王沟镇王老家村后王老家西桥","首羡镇张集村张集东南桥","首羡镇渠集村潘庄东南桥","首羡镇徐老家村徐老家大队后桥","首羡镇徐老家村徐老家东桥","首羡镇徐老家村王新庄桥","首羡镇温庄村白里庄南桥","首羡镇袁老家村高庙东桥","首羡镇温庄村小渠庄后桥","首羡镇李河东北桥","首羡镇温庄村前屯南桥","首羡镇三官庙村三官庙西桥","首羡镇温庄村后屯南桥","首羡镇和集南桥","首羡镇董庄村董庄1桥","首羡镇李药铺庄内桥","首羡镇葛针园村夏屯东桥","首羡镇三官庙村丁大庄北桥","首羡镇和集庄北桥","首羡镇于张庄东桥","首羡镇大渠庄后桥","赵庄镇单庄村奚庄东桥","赵庄镇大彭庄村安集南桥","赵庄镇孙庄村魏楼前桥","赵庄镇单庄村大奚庄前桥","赵庄镇王学屋村前张楼桥","赵庄镇王学屋村陆庙西桥","赵庄镇青林村青林南桥","赵庄镇王龙庄村王龙庄东桥","赵庄镇朱陈村小吴庄北桥","赵庄镇吴楼村谢庄前桥","赵庄镇吴楼村谢庄桥","赵庄镇大刘集村大刘集西桥","赵庄镇大吴庄村杨庄寺东桥","赵庄镇袁集村常庄南桥","赵庄镇鹿湾村鹿湾后桥","赵庄镇赵庄村赵庄东桥","赵庄镇赵庄村杨行桥","赵庄镇赵庄村杨行北桥","赵庄镇赵庄村杨行南桥","赵庄镇王学屋陆庙桥","赵庄镇王学屋村张后楼桥","赵庄镇王学屋村齐小楼前桥","赵庄镇孙庄村孙庄西桥","赵庄镇王龙庄村马楼东桥","赵庄镇许庄村王堤口北桥","赵庄镇许庄村王堤口西桥","孙楼街道办事处高楼村高楼二队桥","孙楼街道办事处陈楼村孙三楼桥","孙楼街道办事处张新庄村果园前桥","孙楼街道办事处张新庄村刘楼东桥","孙楼街道办事处小学东桥","孙楼街道办事处前季庙庄桥","孙楼镇三合村东桥","宋楼镇史大楼桥","宋楼刘庄桥"],"not_rendered":{"external_links":1,"defined_names":11},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"汇总","index":0,"n_rows":110,"n_cols":3,"rows_kept":110,"merged":[[0,0,0,2]],"flags":["formulas_cached_only"]}
["丰县2017年农村公益桥梁工程量清单汇总表"]
["编号","分组工程名称","总价（元）"]
[1,"顺河镇王寨村王寨东桥"]
[2,"顺河镇张口村张口南2桥"]
[3,"顺河镇白庙村孙庄桥"]
[4,"顺河镇大圣村裴庄北桥"]
[5,"顺河镇焦庄村周庄北桥"]
[6,"顺河镇王寨村李庄东桥"]
[7,"顺河镇李庄村河申北桥"]
[8,"顺河镇顺河村周屯南桥"]
[9,"顺河镇白庙村白庙新村前桥"]
[10,"顺河镇朱坑村康庄后桥"]
[11,"顺河镇大圣村黄庄东桥"]
[12,"顺河镇土屯村王双楼东桥"]
[13,"顺河镇张口村张口南1桥"]
[14,"顺河镇范庄村范庄西桥"]
[15,"顺河镇范庄村范庄中桥"]
[16,"顺河镇范庄村范庄北桥"]
[17,"顺河镇杨楼村后杨楼北桥"]
[18,"顺河镇杨楼村后杨楼西北桥"]
[19,"顺河镇岳庄村岳草楼东桥"]
[20,"顺河镇渠寨村季庄前桥"]
[21,"顺河镇大圣村大圣西桥"]
[22,"顺河镇焦庄村周庄西桥"]
[23,"顺河镇焦庄村焦庄东桥"]
[24,"王沟镇周庄寨村袁庄北桥"]
[25,"王沟镇王大庄村育才小学西桥"]
[26,"王沟镇孙许庄东南桥"]
[27,"王沟镇邵楼村邵楼西北桥"]
[28,"王沟镇王老家村前老鹤寺西北桥"]
[29,"王沟镇刘小集村杨楼西南桥"]
[30,"王沟镇王大庄村王楼东桥"]
[31,"王沟镇丁楼东北桥"]
[32,"王沟镇丁楼东桥"]
[33,"王沟镇丁楼东桥王大庄村朱阁南桥"]
[34,"王沟镇王大庄村王大庄西桥"]
[35,"王沟镇李溜村赵庄东桥"]
[36,"王沟镇李溜村丁庄北桥"]
[37,"王沟镇前王老家西南桥"]
[38,"王沟镇后王老家西南桥"]
[39,"王沟镇王老家村圣举鸭厂桥"]
[40,"王沟镇刘小集村代楼中队北桥"]
[41,"王沟镇常楼北桥"]
[42,"王沟镇石洼西南桥"]
[43,"王沟镇刘菜园村北蒋集桥"]
[44,"王沟镇李溜村圣达厂东北桥"]
[45,"王沟镇王老家村后王老家西桥"]
[46,"首羡镇张集村张集东南桥"]
[47,"首羡镇渠集村潘庄东南桥"]
[48,"首羡镇徐老家村徐老家大队后桥"]
[49,"首羡镇徐老家村徐老家东桥"]
[50,"首羡镇徐老家村王新庄桥"]
[51,"首羡镇温庄村白里庄南桥"]
[52,"首羡镇袁老家村高庙东桥"]
[53,"首羡镇温庄村小渠庄后桥"]
[54,"首羡镇李河东北桥"]
[55,"首羡镇温庄村前屯南桥"]
[56,"首羡镇三官庙村三官庙西桥"]
[57,"首羡镇温庄村后屯南桥"]
[58,"首羡镇和集南桥"]
[59,"首羡镇董庄村董庄1桥"]
[60,"首羡镇李药铺庄内桥"]
[61,"首羡镇葛针园村夏屯东桥"]
[62,"首羡镇三官庙村丁大庄北桥"]
[63,"首羡镇和集庄北桥"]
[64,"首羡镇于张庄东桥"]
[65,"首羡镇大渠庄后桥"]
[66,"赵庄镇单庄村奚庄东桥"]
[67,"赵庄镇大彭庄村安集南桥"]
[68,"赵庄镇孙庄村魏楼前桥"]
[69,"赵庄镇单庄村大奚庄前桥"]
[70,"赵庄镇王学屋村前张楼桥"]
[71,"赵庄镇王学屋村陆庙西桥"]
[72,"赵庄镇青林村青林南桥"]
[73,"赵庄镇王龙庄村王龙庄东桥"]
[74,"赵庄镇朱陈村小吴庄北桥"]
[75,"赵庄镇吴楼村谢庄前桥"]
[76,"赵庄镇吴楼村谢庄桥"]
[77,"赵庄镇大刘集村大刘集西桥"]
[78,"赵庄镇大吴庄村杨庄寺东桥"]
[79,"赵庄镇袁集村常庄南桥"]
[80,"赵庄镇鹿湾村鹿湾后桥"]
[81,"赵庄镇赵庄村赵庄东桥"]
[82,"赵庄镇赵庄村杨行桥"]
[83,"赵庄镇赵庄村杨行北桥"]
[84,"赵庄镇赵庄村任庄南桥"]
[85,"赵庄镇王学屋村陆庙桥"]
[86,"赵庄镇王学屋村张楼后桥"]
[87,"赵庄镇王学屋村齐小楼前桥"]
[88,"赵庄镇孙庄村孙庄西桥"]
[89,"赵庄镇王龙庄村马楼东桥"]
[90,"赵庄镇许庄村王堤口北桥"]
[91,"赵庄镇许庄村王堤口西桥"]
[92,"孙楼街道办事处高楼村高楼二队桥"]
[93,"孙楼街道办事处陈楼村孙三楼桥"]
[94,"孙楼街道办事处张新庄村果园前桥"]
[95,"孙楼街道办事处张新庄村刘楼东桥"]
[96,"孙楼街道办事处小学东桥"]
[97,"孙楼街道办事处前季庙庄桥"]
[98,"孙楼镇三合村东桥"]
[99,"宋楼镇史大楼桥"]
[100,"宋楼刘庄桥"]
[null,"组1～组100合计（一）"]
[null,"备用金(二)",{"v":50000,"d":"50000.00"}]
[null,"安全文明措施费（三）",{"v":150000,"d":"150000.00"}]
[null,"投标总金额（一）+（二）+（三）"]
[]
[null,"投标人（盖单位章）："]
[null,"法定代表人（或委托代理人）："]
[null,"年       月      日"]

{"sheet":"顺河镇王寨村王寨东桥","index":1,"n_rows":28,"n_cols":7,"rows_kept":28,"merged":[[0,0,0,6],[1,2,1,6],[27,0,27,3],[27,4,27,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：1",null,"分组工程名称：顺河镇王寨村王寨东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":40,"d":"40.00"}]
[2,"土方回填压实","m3",{"v":60,"d":"60.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":108,"d":"108.00"}]
[2,"C25灌注桩混凝土","m3",{"v":54.4,"d":"54.40"}]
[3,"灌注桩钢筋笼制安","t",4.35]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":20.5,"d":"20.50"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":2.6,"d":"2.60"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制安装","m3",{"v":38.9,"d":"38.90"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":14.4,"d":"14.40"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作及安装","t",15.53]
["四","其他工程"]
[1,"板式橡胶支座","dm3",{"v":52.5,"d":"52.50"}]
[2,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[4,"桥铭牌","个",{"v":2,"d":"2.00"},null,null,"总价"]
[5,"限载标志","个",{"v":2,"d":"2.00"},null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",{"v":300,"d":"300.00"},null,null,"含打桩平台"]
[2,"施工降排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]

{"sheet":"顺河镇张口村张口南2桥","index":2,"n_rows":37,"n_cols":7,"rows_kept":37,"merged":[[0,0,0,6],[1,2,1,6],[36,0,36,3],[36,4,36,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：2",null,"分组工程名称：顺河镇张口村张口南2桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":260,"d":"260.00"}]
[2,"土方回填压实","m3",{"v":210,"d":"210.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":109.2,"d":"109.20"}]
[2,"C25灌注桩混凝土","m3",{"v":54.9,"d":"54.90"}]
[3,"灌注桩钢筋笼制安","t",4.39]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":20.7,"d":"20.70"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":38.9,"d":"38.90"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[5,"C25挡墙侧墙","m3",{"v":9,"d":"9.00"},null,null,"模板、脚手架摊销"]
[6,"管涵基础","m3",{"v":4.2,"d":"4.20"},null,null,"模板、脚手架摊销"]
[7,"C25挡墙底板","m3",{"v":12.1,"d":"12.10"},null,null,"模板、脚手架摊销"]
[8,"120cm涵管购置安装","m",{"v":6,"d":"6.00"},null,null,"模板、脚手架摊销"]
[9,"C25砼防撞栏杆","m3",{"v":19.4,"d":"19.40"},null,null,"模板、脚手架摊销"]
[10,"C20素砼格梗","m3",{"v":2,"d":"2.00"},null,null,"模板、脚手架摊销"]
[11,"C25现浇砼护坡","m3",{"v":4,"d":"4.00"},null,null,"模板、脚手架摊销"]
[12,"钢筋制作及安装","t",17.97]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":3,"d":"3.00"}]
[2,"黄砂垫层 ","m3",{"v":3,"d":"3.00"}]
[3,"板式橡胶支座","dm3",{"v":52.5,"d":"52.50"}]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
[8,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",400,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇白庙村孙庄桥","index":3,"n_rows":29,"n_cols":7,"rows_kept":29,"merged":[[0,0,0,6],[1,2,1,6],[28,0,28,3],[28,4,28,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：3",null,"分组工程名称：顺河镇白庙村孙庄桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":260,"d":"260.00"}]
[2,"土方回填压实","m3",{"v":180,"d":"180.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":78.2,"d":"78.20"}]
[2,"C25灌注桩混凝土","m3",{"v":39.3,"d":"39.30"}]
[3,"灌注桩钢筋笼制安","t",3.14]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":15.7,"d":"15.70"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":2.3,"d":"2.30"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":8.4,"d":"8.40"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作及安装","t",8.59]
["四","其他工程"]
[1,"板式橡胶支座","dm3",30.24]
[2,"桥台GQF-F-6伸缩装置","m",{"v":10,"d":"10.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":5.2,"d":"5.20"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇大圣村裴庄北桥","index":4,"n_rows":32,"n_cols":7,"rows_kept":32,"merged":[[0,0,0,6],[1,2,1,6],[31,0,31,3],[31,4,31,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：4",null,"分组工程名称：顺河镇大圣村裴庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":200,"d":"200.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":74.2,"d":"74.20"}]
[2,"C25灌注桩混凝土","m3",{"v":37.3,"d":"37.30"}]
[3,"灌注桩钢筋笼制安","t",2.98]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",16.96,null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":9.3,"d":"9.30"},null,null,"模板、脚手架摊销"]
[5,"C25素砼格梗","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[6,"C25现浇砼护坡","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",8.87]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":4.2,"d":"4.20"}]
[2,"黄砂垫层 ","m3",{"v":4.2,"d":"4.20"}]
[3,"板式橡胶支座","dm3",26.25]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":3.9,"d":"3.90"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
[8,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇焦庄村周庄北桥","index":5,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[0,0,0,6],[1,2,1,6],[26,0,26,3],[26,4,26,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：5",null,"分组工程名称：顺河镇焦庄村周庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":160,"d":"160.00"}]
[2,"土方回填压实","m3",{"v":100,"d":"100.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":74.2,"d":"74.20"}]
[2,"C25灌注桩混凝土","m3",{"v":37.3,"d":"37.30"}]
[3,"灌注桩钢筋笼制安","t",2.98]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":15.7,"d":"15.70"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":9.3,"d":"9.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作及安装","t",8.71]
["四","其他工程"]
[1,"板式橡胶支座","dm3",26.25]
[2,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":3.9,"d":"3.90"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",200,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇王寨村李庄东桥","index":6,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[0,0,0,6],[1,2,1,6],[34,0,34,3],[34,4,34,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：6",null,"分组工程名称：顺河镇王寨村李庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":100,"d":"100.00"}]
[2,"土方回填压实","m3",{"v":120,"d":"120.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":74.2,"d":"74.20"}]
[2,"C25灌注桩混凝土","m3",{"v":37.3,"d":"37.30"}]
[3,"灌注桩钢筋笼制安","t",2.98]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":15.2,"d":"15.20"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":8.4,"d":"8.40"},null,null,"模板、脚手架摊销"]
[5,"C20素砼格梗","m3",{"v":2.1,"d":"2.10"},null,null,"模板、脚手架摊销"]
[6,"C25现浇砼护坡","m3",{"v":4,"d":"4.00"},null,null,"模板、脚手架摊销"]
[7,"C20道路路面","m2",{"v":6,"d":"6.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作及安装","t",{"v":8.5,"d":"8.50"}]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":3,"d":"3.00"}]
[2,"黄砂垫层 ","m3",{"v":3,"d":"3.00"}]
[3,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[4,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",26.25]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":3.9,"d":"3.90"}]
[8,"桥铭牌","个",2,null,null,"总价"]
[9,"限载标志","个",2,null,null,"总价"]
[10,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇李庄村河申北桥","index":7,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[0,0,0,6],[1,2,1,6],[34,0,34,3],[34,4,34,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：7",null,"分组工程名称：顺河镇李庄村河申北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":160,"d":"160.00"}]
[2,"土方回填压实","m3",{"v":100,"d":"100.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":74.2,"d":"74.20"}]
[2,"C25灌注桩混凝土","m3",{"v":37.3,"d":"37.30"}]
[3,"灌注桩钢筋笼制安","t",2.98]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":15.7,"d":"15.70"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":8.7,"d":"8.70"},null,null,"模板、脚手架摊销"]
[5,"C20素砼格梗","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[6,"C25现浇砼护坡","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[7,"C20道路路面","m2",{"v":6,"d":"6.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作及安装","t",8.63]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":4.2,"d":"4.20"}]
[2,"黄砂垫层 ","m3",{"v":4.2,"d":"4.20"}]
[3,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[4,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",26.25]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":3.9,"d":"3.90"}]
[8,"桥铭牌","个",2,null,null,"总价"]
[9,"限载标志","个",2,null,null,"总价"]
[10,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇顺河村周屯南桥","index":8,"n_rows":34,"n_cols":7,"rows_kept":34,"merged":[[0,0,0,6],[1,2,1,6],[33,0,33,3],[33,4,33,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：8",null,"分组工程名称：顺河镇顺河村周屯南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":200,"d":"200.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":78.2,"d":"78.20"}]
[2,"C25灌注桩混凝土","m3",{"v":39.3,"d":"39.30"}]
[3,"灌注桩钢筋笼制安","t",3.14]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":15.6,"d":"15.60"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",0.86,null,null,"模板、脚手架摊销"]
[4,"C25挡墙侧墙","m3",{"v":9,"d":"9.00"},null,null,"模板、脚手架摊销"]
[5,"管涵基础","m3",{"v":3.2,"d":"3.20"},null,null,"模板、脚手架摊销"]
[6,"C25挡墙底板","m3",{"v":11.2,"d":"11.20"},null,null,"模板、脚手架摊销"]
[7,"C20道路路面","m2",{"v":120,"d":"120.00"},null,null,"模板、脚手架摊销"]
[8,"120cm涵管购置安装","m",{"v":6,"d":"6.00"},null,null,"模板、脚手架摊销"]
[9,"C25砼防撞栏杆","m3",{"v":13.1,"d":"13.10"},null,null,"模板、脚手架摊销"]
[10,"钢筋制作及安装","t",10.81]
["四","其他工程"]
[1,"二灰结石 压实厚度（cm） 20","m2",{"v":128,"d":"128.00"}]
[2,"二灰结石 石灰土（cm） 30","m2",{"v":128,"d":"128.00"}]
[3,"板式橡胶支座","dm3",26.25]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",200,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇白庙村白庙新村前桥","index":9,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[0,0,0,6],[1,2,1,6],[30,0,30,3],[30,4,30,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：9",null,"分组工程名称：顺河镇白庙村白庙新村前桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":160,"d":"160.00"}]
[2,"土方回填压实","m3",{"v":80,"d":"80.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":84.7,"d":"84.70"}]
[2,"C25灌注桩混凝土","m3",{"v":43.9,"d":"43.90"}]
[3,"灌注桩钢筋笼制安","t",3.51]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":20.4,"d":"20.40"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":2.4,"d":"2.40"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制安装","m3",{"v":21.6,"d":"21.60"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":10.4,"d":"10.40"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":10.2,"d":"10.20"},null,null,"模板、脚手架摊销"]
[6,"C20道路路面","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",10.65]
["四","其他工程"]
[1,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[2,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[3,"板式橡胶支座","dm3",30.24]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":5.2,"d":"5.20"}]
[6,"桥铭牌","个",{"v":2,"d":"2.00"},null,null,"总价"]
[7,"限载标志","个",{"v":2,"d":"2.00"},null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",{"v":200,"d":"200.00"},null,null,"含打桩平台"]
[2,"施工降排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]

{"sheet":"顺河镇朱坑村康庄后桥","index":10,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：10",null,"分组工程名称：顺河镇朱坑村康庄后桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":450,"d":"450.00"}]
[2,"土方回填压实","m3",{"v":320,"d":"320.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",106.54]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
[5,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇大圣村黄庄东桥","index":11,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：11",null,"分组工程名称：顺河镇大圣村黄庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":450,"d":"450.00"}]
[2,"土方回填压实","m3",{"v":340,"d":"340.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":172.4,"d":"172.40"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
[5,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇土屯村王双楼东桥","index":12,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：12",null,"分组工程名称：顺河镇土屯村王双楼东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":450,"d":"450.00"}]
[2,"土方回填压实","m3",{"v":340,"d":"340.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":172.4,"d":"172.40"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
[5,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇张口村张口南1桥","index":13,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：13",null,"分组工程名称：顺河镇张口村张口南1桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":400,"d":"400.00"}]
[2,"土方回填压实","m3",{"v":300,"d":"300.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":35.9,"d":"35.90"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.4,"d":"8.40"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.18]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇范庄村范庄西桥","index":14,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：14",null,"分组工程名称：顺河镇范庄村范庄西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":540,"d":"540.00"}]
[2,"土方回填压实","m3",{"v":350,"d":"350.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.8,"d":"8.80"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇范庄村范庄中桥","index":15,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：15",null,"分组工程名称：顺河镇范庄村范庄中桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":540,"d":"540.00"}]
[2,"土方回填压实","m3",{"v":350,"d":"350.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.8,"d":"8.80"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇范庄村范庄北桥","index":16,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：16",null,"分组工程名称：顺河镇范庄村范庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":300,"d":"300.00"}]
[2,"土方回填压实","m3",{"v":230,"d":"230.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":25.6,"d":"25.60"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":29.8,"d":"29.80"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":7.2,"d":"7.20"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",7.73]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇杨楼村后杨楼北桥","index":17,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：17",null,"分组工程名称：顺河镇杨楼村后杨楼北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":300,"d":"300.00"}]
[2,"土方回填压实","m3",{"v":230,"d":"230.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":25.6,"d":"25.60"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":29.8,"d":"29.80"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":7.2,"d":"7.20"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",7.63]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇杨楼村后杨楼西北桥","index":18,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：18",null,"分组工程名称：顺河镇杨楼村后杨楼西北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":300,"d":"300.00"}]
[2,"土方回填压实","m3",{"v":230,"d":"230.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":25.6,"d":"25.60"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":29.8,"d":"29.80"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":7.2,"d":"7.20"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",7.63]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇岳庄村岳草楼东桥","index":19,"n_rows":24,"n_cols":7,"rows_kept":24,"merged":[[0,0,0,6],[1,2,1,6],[23,0,23,3],[23,4,23,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：19",null,"分组工程名称：顺河镇岳庄村岳草楼东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":230,"d":"230.00"}]
[2,"土方回填压实","m3",{"v":180,"d":"180.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.8,"d":"5.80"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":48,"d":"48.00"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":24.5,"d":"24.50"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6.7,"d":"6.70"},null,null,"模板、脚手架摊销"]
[5,"C25砼路面恢复","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",{"v":9.7,"d":"9.70"}]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m3",{"v":64,"d":"64.00"}]
[2,"道路路基 石灰土 30","m3",{"v":68,"d":"68.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇渠寨村季庄前桥","index":20,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：20",null,"分组工程名称：顺河镇渠寨村季庄前桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":130,"d":"130.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":13.5,"d":"13.50"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":26,"d":"26.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":3,"d":"3.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",2.09]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":26,"d":"26.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇大圣村大圣西桥","index":21,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：21",null,"分组工程名称：顺河镇大圣村大圣西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":130,"d":"130.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":13.5,"d":"13.50"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":26,"d":"26.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":3,"d":"3.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",2.09]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":26,"d":"26.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇焦庄村周庄西桥","index":22,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：22",null,"分组工程名称：顺河镇焦庄村周庄西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":160,"d":"160.00"}]
[2,"土方回填压实","m3",{"v":110,"d":"110.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":34.8,"d":"34.80"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":14.9,"d":"14.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.87]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",1,null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"顺河镇焦庄村焦庄东桥","index":23,"n_rows":21,"n_cols":7,"rows_kept":21,"merged":[[0,0,0,6],[1,2,1,6],[20,0,20,3],[20,4,20,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：23",null,"分组工程名称：顺河镇焦庄村焦庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":160,"d":"160.00"}]
[2,"土方回填压实","m3",{"v":80,"d":"80.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":34.8,"d":"34.80"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":14.9,"d":"14.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.87]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇周庄寨村袁庄北桥","index":24,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[0,0,0,6],[1,2,1,6],[30,0,30,3],[30,4,30,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：24",null,"分组工程名称：王沟镇周庄寨村袁庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":80,"d":"80.00"}]
[2,"土方回填压实","m3",{"v":60,"d":"60.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":109.2,"d":"109.20"}]
[2,"C25灌注桩混凝土","m3",{"v":54.9,"d":"54.90"}]
[3,"灌注桩钢筋笼制安","t",4.39]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",19.88,null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":2.6,"d":"2.60"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":38.9,"d":"38.90"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":14.1,"d":"14.10"},null,null,"模板、脚手架摊销"]
[6,"C25道路路面","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",15.41]
["四","其他工程"]
[1,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[2,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[3,"板式橡胶支座","dm3",{"v":52.5,"d":"52.50"}]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",200,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇王大庄村育才小学西桥","index":25,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[0,0,0,6],[1,2,1,6],[30,0,30,3],[30,4,30,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：25",null,"分组工程名称：王沟镇王大庄村育才小学西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":70,"d":"70.00"}]
[2,"土方回填压实","m3",{"v":60,"d":"60.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":78.2,"d":"78.20"}]
[2,"C25灌注桩混凝土","m3",{"v":39.3,"d":"39.30"}]
[3,"灌注桩钢筋笼制安","t",3.14]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":17,"d":"17.00"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制安装","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":9.3,"d":"9.30"},null,null,"模板、脚手架摊销"]
[5,"C20道路路面","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作及安装","t",8.87]
["四","其他工程"]
[1,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[2,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[3,"板式橡胶支座","dm3",26.25]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":3.9,"d":"3.90"}]
[6,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[7,"桥铭牌","个",{"v":2,"d":"2.00"},null,null,"总价"]
[8,"限载标志","个",{"v":2,"d":"2.00"},null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",{"v":200,"d":"200.00"},null,null,"含打桩平台"]
[2,"施工降排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]

{"sheet":"王沟镇孙许庄东南桥","index":26,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[0,0,0,6],[1,2,1,6],[30,0,30,3],[30,4,30,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：26",null,"分组工程名称：王沟镇孙许庄东南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":80,"d":"80.00"}]
[2,"土方回填压实","m3",{"v":60,"d":"60.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":119.4,"d":"119.40"}]
[2,"C25灌注桩混凝土","m3",{"v":60,"d":"60.00"}]
[3,"灌注桩钢筋笼制安","t",{"v":4.8,"d":"4.80"}]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",22.11,null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":15.7,"d":"15.70"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":12.3,"d":"12.30"},null,null,"模板、脚手架摊销"]
[6,"C25道路路面","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",15.59]
["四","其他工程"]
[1,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[2,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[3,"板式橡胶支座","dm3",45.36]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",200,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇邵楼村邵楼西北桥","index":27,"n_rows":30,"n_cols":7,"rows_kept":30,"merged":[[0,0,0,6],[1,2,1,6],[29,0,29,3],[29,4,29,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：27",null,"分组工程名称：王沟镇邵楼村邵楼西北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":540,"d":"540.00"}]
[2,"土方回填压实","m3",{"v":350,"d":"350.00"}]
["二","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[2,"C25桥台墙身","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[3,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":4.8,"d":"4.80"},null,null,"模板、脚手架摊销"]
[5,"C25素砼格梗","m3",0.93,null,null,"模板、脚手架摊销"]
[6,"C25现浇砼护坡","m3",0.13,null,null,"模板、脚手架摊销"]
[7,"C25砼封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[8,"C25砼防撞栏杆","m3",{"v":8.8,"d":"8.80"},null,null,"模板、脚手架摊销"]
[9,"钢筋制作及安装","t",9.36]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":0.1,"d":"0.10"}]
[2,"黄砂垫层 ","m3",{"v":0.1,"d":"0.10"}]
[3,"桥台GQF-F-6伸缩装置","m",{"v":10,"d":"10.00"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":5.2,"d":"5.20"}]
[5,"桥铭牌","个",2,null,null,"总价"]
[6,"限载标志","个",2,null,null,"总价"]
[7,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇王老家村前老鹤寺西北桥","index":28,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：28",null,"分组工程名称：王沟镇王老家村前老鹤寺西北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":200,"d":"200.00"}]
[2,"土方回填压实","m3",{"v":150,"d":"150.00"}]
["二","混凝土工程"]
[1,"C30箱涵","m3",{"v":25.4,"d":"25.40"},null,null,"模板、脚手架摊销"]
[2,"C30耳墙","m3",{"v":26.3,"d":"26.30"},null,null,"模板、脚手架摊销"]
[3,"C25砼封底","m3",{"v":5.9,"d":"5.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":7.1,"d":"7.10"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",11.27]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",13.26]
[2,"桥面铸铁排水管（φ10）","m",{"v":3.9,"d":"3.90"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇刘小集村杨楼西南桥","index":29,"n_rows":24,"n_cols":7,"rows_kept":24,"merged":[[0,0,0,6],[1,2,1,6],[23,0,23,3],[23,4,23,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：29",null,"分组工程名称：王沟镇刘小集村杨楼西南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":36.1,"d":"36.10"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[5,"C25砼路面恢复","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",9.79]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m3",{"v":64,"d":"64.00"}]
[2,"道路路基 石灰土 30","m3",{"v":68,"d":"68.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇王大庄村王楼东桥","index":30,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：30",null,"分组工程名称：王沟镇王大庄村王楼东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":11.4,"d":"11.40"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",{"v":9.1,"d":"9.10"},null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":21,"d":"21.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":2.4,"d":"2.40"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",1.75]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":21,"d":"21.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇丁楼东北桥","index":31,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[0,0,0,6],[1,2,1,6],[26,0,26,3],[26,4,26,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：31",null,"分组工程名称：王沟镇丁楼东北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":250,"d":"250.00"}]
[2,"土方回填压实","m3",{"v":200,"d":"200.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":1.2,"d":"1.20"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",{"v":3.2,"d":"3.20"},null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":23.9,"d":"23.90"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":11.3,"d":"11.30"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":5.1,"d":"5.10"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",4.89]
["四","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":8.4,"d":"8.40"}]
[2,"碎石垫层 ","m3",{"v":2.4,"d":"2.40"}]
[3,"黄砂垫层 ","m3",{"v":2.4,"d":"2.40"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[5,"桥铭牌","个",2,null,null,"总价"]
[6,"限载标志","个",2,null,null,"总价"]
[7,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇丁楼东桥","index":32,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：32",null,"分组工程名称：王沟镇丁楼东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":280,"d":"280.00"}]
[2,"土方回填压实","m3",{"v":230,"d":"230.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":3.1,"d":"3.10"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",{"v":10.1,"d":"10.10"},null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":25.7,"d":"25.70"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":16.8,"d":"16.80"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":6,"d":"6.00"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",5.68]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":7.6,"d":"7.60"}]
[2,"黄砂垫层 ","m3",{"v":7.6,"d":"7.60"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇丁楼东桥王大庄村朱阁南桥","index":33,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[0,0,0,6],[1,2,1,6],[26,0,26,3],[26,4,26,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：33",null,"分组工程名称：王沟镇丁楼东桥王大庄村朱阁南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":410,"d":"410.00"}]
[2,"土方回填压实","m3",{"v":310,"d":"310.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":3.5,"d":"3.50"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":3.1,"d":"3.10"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",{"v":5.1,"d":"5.10"},null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":54.5,"d":"54.50"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":16.7,"d":"16.70"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",{"v":10.2,"d":"10.20"}]
["四","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":28.3,"d":"28.30"}]
[2,"碎石垫层 ","m3",{"v":3.8,"d":"3.80"}]
[3,"黄砂垫层 ","m3",{"v":3.8,"d":"3.80"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[5,"桥铭牌","个",2,null,null,"总价"]
[6,"限载标志","个",2,null,null,"总价"]
[7,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇王大庄村王大庄西桥","index":34,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：34",null,"分组工程名称：王沟镇王大庄村王大庄西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":190,"d":"190.00"}]
[2,"土方回填压实","m3",{"v":130,"d":"130.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":34.8,"d":"34.80"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":14.9,"d":"14.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5,"d":"5.00"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.81]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇李溜村赵庄东桥","index":35,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：35",null,"分组工程名称：王沟镇李溜村赵庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":170,"d":"170.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":23.7,"d":"23.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":16.9,"d":"16.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",5.32]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇李溜村丁庄北桥","index":36,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,0,1,1],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：36",null,"              分组工程名称：王沟镇李溜村丁庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":250,"d":"250.00"}]
[2,"土方回填压实","m3",{"v":210,"d":"210.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":23.9,"d":"23.90"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":13.6,"d":"13.60"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",5.09]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇前王老家西南桥","index":37,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：37",null,"            分组工程名称：王沟镇前王老家西南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":23.7,"d":"23.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":16.9,"d":"16.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",5.32]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇后王老家西南桥","index":38,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：38",null,"分组工程名称：王沟镇后王老家西南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.2,"d":"37.20"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":19,"d":"19.00"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",7.61]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇王老家村圣举鸭厂桥","index":39,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：39",null,"分组工程名称：王沟镇王老家村圣举鸭厂桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":250,"d":"250.00"}]
[2,"土方回填压实","m3",{"v":210,"d":"210.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":2.5,"d":"2.50"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",{"v":6.4,"d":"6.40"},null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":23.9,"d":"23.90"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":13.6,"d":"13.60"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",5.09]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":4.8,"d":"4.80"}]
[2,"黄砂垫层 ","m3",{"v":4.8,"d":"4.80"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇刘小集村代楼中队北桥","index":40,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：40",null,"分组工程名称：王沟镇刘小集村代楼中队北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.2,"d":"37.20"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":15.3,"d":"15.30"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",7.25]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇常楼北桥","index":41,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：41",null,"分组工程名称：王沟镇常楼北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":180,"d":"180.00"}]
[2,"土方回填压实","m3",{"v":140,"d":"140.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":21.5,"d":"21.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":11.9,"d":"11.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",4.59]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇石洼西南桥","index":42,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：42",null,"分组工程名称：王沟镇石洼西南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":190,"d":"190.00"}]
[2,"土方回填压实","m3",{"v":140,"d":"140.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":34.8,"d":"34.80"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":12.9,"d":"12.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.67]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇刘菜园村北蒋集桥","index":43,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：43",null,"分组工程名称：王沟镇刘菜园村北蒋集桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":240,"d":"240.00"}]
[2,"土方回填压实","m3",{"v":180,"d":"180.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",3.12,null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",2.02,null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":15.4,"d":"15.40"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":6.2,"d":"6.20"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",6.99]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":2.5,"d":"2.50"}]
[2,"黄砂垫层 ","m3",{"v":2.5,"d":"2.50"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇李溜村圣达厂东北桥","index":44,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：44",null,"分组工程名称：王沟镇李溜村圣达厂东北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":240,"d":"240.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",3.12,null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",2.02,null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":15.4,"d":"15.40"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":6.2,"d":"6.20"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",6.99]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":2.5,"d":"2.50"}]
[2,"黄砂垫层 ","m3",{"v":2.5,"d":"2.50"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"王沟镇王老家村后王老家西桥","index":45,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：45",null,"分组工程名称：王沟镇王老家村后王老家西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",3.12,null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.44]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇张集村张集东南桥","index":46,"n_rows":32,"n_cols":7,"rows_kept":32,"merged":[[0,0,0,6],[1,2,1,6],[31,0,31,3],[31,4,31,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：46",null,"分组工程名称：首羡镇张集村张集东南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":60,"d":"60.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":106.2,"d":"106.20"}]
[2,"C25灌注桩混凝土","m3",{"v":53.4,"d":"53.40"}]
[3,"灌注桩钢筋笼制安","t",4.27]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":20.4,"d":"20.40"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":2.6,"d":"2.60"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制安装","m3",{"v":38.9,"d":"38.90"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[5,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":14.7,"d":"14.70"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",15.55]
["四","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":64,"d":"64.00"}]
[2,"道路路基 石灰土 30","m2",{"v":68,"d":"68.00"}]
[3,"板式橡胶支座","dm3",{"v":52.5,"d":"52.50"}]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[6,"老桥拆除","项",{"v":1,"d":"1.00"}]
[7,"桥铭牌","个",{"v":2,"d":"2.00"},null,null,"总价"]
[8,"限载标志","个",{"v":2,"d":"2.00"},null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",{"v":300,"d":"300.00"},null,null,"含打桩平台"]
[2,"施工降排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]

{"sheet":"首羡镇渠集村潘庄东南桥","index":47,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[0,0,0,6],[1,2,1,6],[34,0,34,3],[34,4,34,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：47",null,"分组工程名称：首羡镇渠集村潘庄东南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":60,"d":"60.00"}]
[2,"土方回填压实","m3",{"v":80,"d":"80.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":108.2,"d":"108.20"}]
[2,"C25灌注桩混凝土","m3",{"v":54.4,"d":"54.40"}]
[3,"灌注桩钢筋笼制安","t",4.35]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":22.1,"d":"22.10"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":38.9,"d":"38.90"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":15.3,"d":"15.30"},null,null,"模板、脚手架摊销"]
[6,"C25素砼格梗","m3",{"v":10.7,"d":"10.70"},null,null,"模板、脚手架摊销"]
[7,"C25现浇砼护坡","m3",{"v":16.4,"d":"16.40"},null,null,"模板、脚手架摊销"]
[8,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[9,"钢筋制作及安装","t",15.93]
["四","其他工程"]
[1,"碎石垫层 ","m3",12.27]
[2,"黄砂垫层 ","m3",12.27]
[3,"道路路基 二灰结石 20","m2",{"v":64,"d":"64.00"}]
[4,"道路路基 石灰土 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",26.25]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":3.9,"d":"3.90"}]
[8,"桥铭牌","个",2,null,null,"总价"]
[9,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇徐老家村徐老家大队后桥","index":48,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：48",null,"分组工程名称：首羡镇徐老家村徐老家大队后桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":550,"d":"550.00"}]
[2,"土方回填压实","m3",{"v":350,"d":"350.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":4.8,"d":"4.80"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.8,"d":"8.80"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇徐老家村徐老家东桥","index":49,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：49",null,"分组工程名称：首羡镇徐老家村徐老家东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":550,"d":"550.00"}]
[2,"土方回填压实","m3",{"v":350,"d":"350.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":4.8,"d":"4.80"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.8,"d":"8.80"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",80]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇徐老家村王新庄桥","index":50,"n_rows":29,"n_cols":7,"rows_kept":29,"merged":[[0,0,0,6],[1,2,1,6],[28,0,28,3],[28,4,28,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：50",null,"分组工程名称：首羡镇徐老家村王新庄桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":550,"d":"550.00"}]
[2,"土方回填压实","m3",{"v":350,"d":"350.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":1.2,"d":"1.20"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",0.23,null,null,"模板、脚手架摊销"]
[4,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[5,"C25桥台","m3",{"v":36.7,"d":"36.70"},null,null,"模板、脚手架摊销"]
[6,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[7,"C30桥面板预制安装","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[8,"C40砼桥面铺装（含铰缝）","m3",{"v":4.8,"d":"4.80"},null,null,"模板、脚手架摊销"]
[9,"C25防撞护栏","m3",{"v":8.8,"d":"8.80"},null,null,"模板、脚手架摊销"]
[10,"钢筋制作安装 ","t",9.36]
["三","其他工程"]
[1,"碎石垫层 ","m3",0.17]
[2,"黄砂垫层 ","m3",0.17]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",80]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇温庄村白里庄南桥","index":51,"n_rows":32,"n_cols":7,"rows_kept":32,"merged":[[0,0,0,6],[1,2,1,6],[31,0,31,3],[31,4,31,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：51",null,"分组工程名称：首羡镇温庄村白里庄南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":550,"d":"550.00"}]
[2,"土方回填压实","m3",{"v":350,"d":"350.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":0.9,"d":"0.90"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",0.11,null,null,"模板、脚手架摊销"]
[4,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[5,"C25桥台","m3",{"v":25.6,"d":"25.60"},null,null,"模板、脚手架摊销"]
[6,"C25桥台底板","m3",{"v":29.8,"d":"29.80"},null,null,"模板、脚手架摊销"]
[7,"C30桥面板预制安装","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[8,"C40砼桥面铺装（含铰缝）","m3",{"v":4.8,"d":"4.80"},null,null,"模板、脚手架摊销"]
[9,"C30混凝土路面 压实厚度(cm) 20","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[10,"C25防撞护栏","m3",{"v":7.2,"d":"7.20"},null,null,"模板、脚手架摊销"]
[11,"钢筋制作安装 ","t",7.63]
["三","其他工程"]
[1,"碎石垫层 ","m3",0.08]
[2,"黄砂垫层 ","m3",0.08]
[3,"道路路基 二灰结石 20","m2",{"v":64,"d":"64.00"}]
[4,"道路路基 石灰土 30","m2",{"v":68,"d":"68.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
[8,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",80]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇袁老家村高庙东桥","index":52,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：52",null,"分组工程名称：首羡镇袁老家村高庙东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":36.1,"d":"36.10"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[5,"C25砼路面恢复","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",{"v":7.3,"d":"7.30"}]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m3",{"v":64,"d":"64.00"}]
[2,"道路路基 石灰土 30","m3",{"v":68,"d":"68.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"老桥拆除","项",{"v":1,"d":"1.00"}]
[5,"桥铭牌","个",2,null,null,"总价"]
[6,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇温庄村小渠庄后桥","index":53,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：53",null,"分组工程名称：首羡镇温庄村小渠庄后桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":36.1,"d":"36.10"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[5,"C25砼路面恢复","m2",{"v":80,"d":"80.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",{"v":7.3,"d":"7.30"}]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m3",{"v":85,"d":"85.00"}]
[2,"道路路基 石灰土 30","m3",{"v":90,"d":"90.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"老桥拆除","项",{"v":1,"d":"1.00"}]
[5,"桥铭牌","个",2,null,null,"总价"]
[6,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇李河东北桥","index":54,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：54",null,"分组工程名称：首羡镇李河东北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":250,"d":"250.00"}]
[2,"土方回填压实","m3",{"v":190,"d":"190.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":57.3,"d":"57.30"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":26.3,"d":"26.30"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":7.1,"d":"7.10"},null,null,"模板、脚手架摊销"]
[5,"C25砼路面恢复","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",11.27]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":13.3,"d":"13.30"}]
[2,"道路路基 二灰结石 20","m3",{"v":64,"d":"64.00"}]
[3,"道路路基 石灰土 30","m3",{"v":68,"d":"68.00"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[5,"老桥拆除","项",{"v":1,"d":"1.00"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇温庄村前屯南桥","index":55,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：55",null,"分组工程名称：首羡镇温庄村前屯南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":250,"d":"250.00"}]
[2,"土方回填压实","m3",{"v":190,"d":"190.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":39.4,"d":"39.40"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":21.7,"d":"21.70"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6,"d":"6.00"},null,null,"模板、脚手架摊销"]
[5,"C25砼路面恢复","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",8.13]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m3",{"v":64,"d":"64.00"}]
[2,"道路路基 石灰土 30","m3",{"v":68,"d":"68.00"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"老桥拆除","项",{"v":1,"d":"1.00"}]
[5,"桥铭牌","个",2,null,null,"总价"]
[6,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇三官庙村三官庙西桥","index":56,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：56",null,"分组工程名称：首羡镇三官庙村三官庙西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":130,"d":"130.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":13.5,"d":"13.50"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":26,"d":"26.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":3,"d":"3.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",2.09]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":26,"d":"26.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇温庄村后屯南桥","index":57,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：57",null,"分组工程名称：首羡镇温庄村后屯南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":130,"d":"130.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":13.5,"d":"13.50"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":26,"d":"26.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":3,"d":"3.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",2.09]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":26,"d":"26.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇和集南桥","index":58,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：58",null,"分组工程名称：首羡镇和集南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":170,"d":"170.00"}]
[2,"土方回填压实","m3",{"v":130,"d":"130.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":23.9,"d":"23.90"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":12.7,"d":"12.70"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.1,"d":"5.10"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",5.01]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇董庄村董庄1桥","index":59,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：59",null,"分组工程名称：首羡镇董庄村董庄1桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":140,"d":"140.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":1.3,"d":"1.30"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",{"v":3.4,"d":"3.40"},null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":23.9,"d":"23.90"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":10.6,"d":"10.60"},null,null,"模板、脚手架摊销"]
[6,"C25砼防撞栏杆","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作及安装","t",6.13]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":2.6,"d":"2.60"}]
[2,"黄砂垫层 ","m3",{"v":2.6,"d":"2.60"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇李药铺庄内桥","index":60,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6],[1,2,1,6],[22,0,22,3],[22,4,22,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：60",null,"分组工程名称：首羡镇李药铺庄内桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":190,"d":"190.00"}]
[2,"土方回填压实","m3",{"v":120,"d":"120.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":34.8,"d":"34.80"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":12.9,"d":"12.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.5,"d":"4.50"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.61]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":12,"d":"12.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",{"v":1,"d":"1.00"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇葛针园村夏屯东桥","index":61,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：61",null,"分组工程名称：首羡镇葛针园村夏屯东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":170,"d":"170.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":23.7,"d":"23.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":16.9,"d":"16.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",5.32]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇三官庙村丁大庄北桥","index":62,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：62",null,"分组工程名称：首羡镇三官庙村丁大庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":240,"d":"240.00"}]
[2,"土方回填压实","m3",{"v":170,"d":"170.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":3.5,"d":"3.50"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":50.7,"d":"50.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":12.6,"d":"12.60"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.9,"d":"5.90"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",9.08]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇和集庄北桥","index":63,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：63",null,"分组工程名称：首羡镇和集庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",3.12,null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.44]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇于张庄东桥","index":64,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：64",null,"分组工程名称：首羡镇于张庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",3.12,null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.44]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"首羡镇大渠庄后桥","index":65,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：65",null,"分组工程名称：首羡镇大渠庄后桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",3.12,null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.44]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇单庄村奚庄东桥","index":66,"n_rows":40,"n_cols":7,"rows_kept":40,"merged":[[0,0,0,6],[1,2,1,6],[39,0,39,3],[39,4,39,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：66",null,"分组工程名称：赵庄镇单庄村奚庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":110,"d":"110.00"}]
[2,"土方回填压实","m3",{"v":130,"d":"130.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":108.2,"d":"108.20"}]
[2,"C25灌注桩混凝土","m3",{"v":54.4,"d":"54.40"}]
[3,"灌注桩钢筋笼制安","t",4.35]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":20.8,"d":"20.80"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":3.1,"d":"3.10"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":38.9,"d":"38.90"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[5,"C25U型侧墙","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[6,"管涵基础","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[7,"C25挡墙底板","m3",{"v":17.5,"d":"17.50"},null,null,"模板、脚手架摊销"]
[8,"120cm涵管购置安装","m",{"v":6,"d":"6.00"},null,null,"模板、脚手架摊销"]
[9,"C25砼防撞栏杆","m3",{"v":16.2,"d":"16.20"},null,null,"模板、脚手架摊销"]
[10,"C20素砼格梗","m3",{"v":11,"d":"11.00"},null,null,"模板、脚手架摊销"]
[11,"C25现浇砼护坡","m3",{"v":12.8,"d":"12.80"},null,null,"模板、脚手架摊销"]
[12,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[13,"钢筋制作及安装","t",17.79]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":9.6,"d":"9.60"}]
[2,"黄砂垫层 ","m3",{"v":9.6,"d":"9.60"}]
[3,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[4,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",{"v":52.5,"d":"52.50"}]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[8,"桥铭牌","个",2,null,null,"总价"]
[9,"限载标志","个",2,null,null,"总价"]
[10,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇大彭庄村安集南桥","index":67,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[0,0,0,6],[1,2,1,6],[34,0,34,3],[34,4,34,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：67",null,"分组工程名称：赵庄镇大彭庄村安集南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":60,"d":"60.00"}]
[2,"土方回填压实","m3",{"v":80,"d":"80.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":78.2,"d":"78.20"}]
[2,"C25灌注桩混凝土","m3",{"v":39.3,"d":"39.30"}]
[3,"灌注桩钢筋笼制安","t",3.14]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":17.5,"d":"17.50"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[6,"C20素砼格梗","m3",{"v":4.2,"d":"4.20"},null,null,"模板、脚手架摊销"]
[7,"C25现浇砼护坡","m3",{"v":2.6,"d":"2.60"},null,null,"模板、脚手架摊销"]
[8,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[9,"钢筋制作及安装","t",8.98]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":1.9,"d":"1.90"}]
[2,"黄砂垫层 ","m3",{"v":1.9,"d":"1.90"}]
[3,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[4,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",26.25]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[8,"桥铭牌","个",2,null,null,"总价"]
[9,"限载标志","个",2,null,null,"总价"]
[10,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",200,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇孙庄村魏楼前桥","index":68,"n_rows":30,"n_cols":7,"rows_kept":30,"merged":[[0,0,0,6],[1,2,1,6],[29,0,29,3],[29,4,29,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：68",null,"分组工程名称：赵庄镇孙庄村魏楼前桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":260,"d":"260.00"}]
[2,"土方回填压实","m3",{"v":80,"d":"80.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":78.2,"d":"78.20"}]
[2,"C25灌注桩混凝土","m3",{"v":39.3,"d":"39.30"}]
[3,"灌注桩钢筋笼制安","t",3.14]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":16.5,"d":"16.50"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[5,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作及安装","t",8.78]
["四","其他工程"]
[1,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[2,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[3,"板式橡胶支座","dm3",26.25]
[4,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",200,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇单庄村大奚庄前桥","index":69,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[0,0,0,6],[1,2,1,6],[34,0,34,3],[34,4,34,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：69",null,"分组工程名称：赵庄镇单庄村大奚庄前桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":60,"d":"60.00"}]
[2,"土方回填压实","m3",{"v":80,"d":"80.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":78.2,"d":"78.20"}]
[2,"C25灌注桩混凝土","m3",{"v":39.3,"d":"39.30"}]
[3,"灌注桩钢筋笼制安","t",3.14]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":15.7,"d":"15.70"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":8.7,"d":"8.70"},null,null,"模板、脚手架摊销"]
[6,"C20素砼格梗","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[7,"C25现浇砼护坡","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[8,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[9,"钢筋制作及安装","t",8.63]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":4.2,"d":"4.20"}]
[2,"黄砂垫层 ","m3",{"v":4.2,"d":"4.20"}]
[3,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[4,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",26.25]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[8,"桥铭牌","个",2,null,null,"总价"]
[9,"限载标志","个",2,null,null,"总价"]
[10,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",200,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计",{"$nulls":3},{"v":0,"d":"0.00"}]

{"sheet":"赵庄镇王学屋村前张楼桥","index":70,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：70",null,"分组工程名称：赵庄镇王学屋村前张楼桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":110,"d":"110.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":30.9,"d":"30.90"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":11,"d":"11.00"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.5,"d":"4.50"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.65]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇王学屋村陆庙西桥","index":71,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：71",null,"分组工程名称：赵庄镇王学屋村陆庙西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":110,"d":"110.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2,"d":"2.00"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":27.8,"d":"27.80"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":11,"d":"11.00"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.4,"d":"4.40"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.18]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇青林村青林南桥","index":72,"n_rows":25,"n_cols":7,"rows_kept":25,"merged":[[0,0,0,6],[1,2,1,6],[24,0,24,3],[24,4,24,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：72",null,"分组工程名称：赵庄镇青林村青林南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":260,"d":"260.00"}]
[2,"土方回填压实","m3",{"v":170,"d":"170.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[2,"C25冒梁（含挡块）","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[3,"C25桥台","m3",{"v":29.7,"d":"29.70"},null,null,"模板、脚手架摊销"]
[4,"C25桥台底板","m3",{"v":28.5,"d":"28.50"},null,null,"模板、脚手架摊销"]
[5,"C30桥面板预制安装","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[6,"C40砼桥面铺装（含铰缝）","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[7,"C25防撞护栏","m3",{"v":8.1,"d":"8.10"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",8.42]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"桥铭牌","个",2,null,null,"总价"]
[3,"限载标志","个",2,null,null,"总价"]
[4,"老桥拆除","项",1,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇王龙庄村王龙庄东桥","index":73,"n_rows":29,"n_cols":7,"rows_kept":29,"merged":[[0,0,0,6],[1,2,1,6],[28,0,28,3],[28,4,28,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：73",null,"分组工程名称：赵庄镇王龙庄村王龙庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":130,"d":"130.00"}]
[2,"土方回填压实","m3",{"v":80,"d":"80.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[2,"C25素砼格梗","m3",{"v":1.4,"d":"1.40"},null,null,"模板、脚手架摊销"]
[3,"C25现浇砼护坡","m3",{"v":1.2,"d":"1.20"},null,null,"模板、脚手架摊销"]
[4,"C30箱涵","m3",{"v":33.4,"d":"33.40"},null,null,"模板、脚手架摊销"]
[5,"C30耳墙","m3",{"v":13.4,"d":"13.40"},null,null,"模板、脚手架摊销"]
[6,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[7,"C25砼防撞栏杆","m3",{"v":5,"d":"5.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作及安装","t",6.48]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":0.9,"d":"0.90"}]
[2,"黄砂垫层 ","m3",{"v":0.9,"d":"0.90"}]
[3,"道路路基 二灰结石 20","m2",{"v":64,"d":"64.00"}]
[4,"道路路基 石灰土 30","m2",{"v":68,"d":"68.00"}]
[5,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
[8,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇朱陈村小吴庄北桥","index":74,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：74",null,"分组工程名称：赵庄镇朱陈村小吴庄北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":180,"d":"180.00"}]
[2,"土方回填压实","m3",{"v":120,"d":"120.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.6,"d":"5.60"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":36,"d":"36.00"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":17,"d":"17.00"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6.9,"d":"6.90"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",7.31]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"}]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇吴楼村谢庄前桥","index":75,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：75",null,"分组工程名称：赵庄镇吴楼村谢庄前桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":130,"d":"130.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":13.5,"d":"13.50"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":26,"d":"26.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":3,"d":"3.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",2.09]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":26,"d":"26.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇吴楼村谢庄桥","index":76,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：76",null,"分组工程名称：赵庄镇吴楼村谢庄桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":130,"d":"130.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":13.5,"d":"13.50"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",{"v":10.8,"d":"10.80"},null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":26,"d":"26.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":3,"d":"3.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",2.09]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":26,"d":"26.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇大刘集村大刘集西桥","index":77,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：77",null,"分组工程名称：赵庄镇大刘集村大刘集西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":11.4,"d":"11.40"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",9.13,null,null,"模板、脚手架摊销"]
[5,"C25混凝土路面","m2",{"v":21,"d":"21.00"},null,null,"模板、脚手架摊销"]
[6,"φ120cm管涵购置铺设\n","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[7,"C25防撞护栏","m3",{"v":2.4,"d":"2.40"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作安装 ","t",1.75]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":21,"d":"21.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇大吴庄村杨庄寺东桥","index":78,"n_rows":28,"n_cols":7,"rows_kept":28,"merged":[[0,0,0,6],[1,2,1,6],[27,0,27,3],[27,4,27,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：78",null,"分组工程名称：赵庄镇大吴庄村杨庄寺东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":120,"d":"120.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":4.9,"d":"4.90"},null,null,"模板、脚手架摊销"]
[2,"C25管涵底板","m3",{"v":6.8,"d":"6.80"},null,null,"模板、脚手架摊销"]
[3,"C25挡墙底板","m3",{"v":11.4,"d":"11.40"},null,null,"模板、脚手架摊销"]
[4,"C25挡墙墙身","m3",9.13,null,null,"模板、脚手架摊销"]
[5,"C25U型槽底板","m3",{"v":4.7,"d":"4.70"},null,null,"模板、脚手架摊销"]
[6,"C25U型槽墙身","m3",{"v":4.6,"d":"4.60"},null,null,"模板、脚手架摊销"]
[7,"C25混凝土路面","m2",{"v":21,"d":"21.00"},null,null,"模板、脚手架摊销"]
[8,"φ120cm管涵购置铺设","m3",{"v":6,"d":"6.00"},null,null,"含安装"]
[9,"C25防撞护栏","m3",{"v":2.4,"d":"2.40"},null,null,"模板、脚手架摊销"]
[10,"钢筋制作安装 ","t",1.75]
["三","其他工程"]
[1,"道路路基 二灰结石 20","m2",{"v":21,"d":"21.00"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",1,null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",60]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇袁集村常庄南桥","index":79,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6],[1,2,1,6],[22,0,22,3],[22,4,22,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：79",null,"分组工程名称：赵庄镇袁集村常庄南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":150,"d":"150.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.2,"d":"37.20"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":17,"d":"17.00"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.9,"d":"5.90"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",7.41]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":9.1,"d":"9.10"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇鹿湾村鹿湾后桥","index":80,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：80",null,"分组工程名称：赵庄镇鹿湾村鹿湾后桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":160,"d":"160.00"}]
[2,"土方回填压实","m3",{"v":110,"d":"110.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":9.1,"d":"9.10"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.7,"d":"4.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",5.96]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇赵庄村赵庄东桥","index":81,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：81",null,"分组工程名称：赵庄镇赵庄村赵庄东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":180,"d":"180.00"}]
[2,"土方回填压实","m3",{"v":140,"d":"140.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":21.5,"d":"21.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":11.9,"d":"11.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",4.59]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇赵庄村杨行桥","index":82,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[0,0,0,6],[1,2,1,6],[26,0,26,3],[26,4,26,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：82",null,"分组工程名称：赵庄镇赵庄村杨行桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":250,"d":"250.00"}]
[2,"土方回填压实","m3",{"v":200,"d":"200.00"}]
["二","混凝土工程"]
[1,"C25格梗","m3",{"v":1.2,"d":"1.20"},null,null,"模板、脚手架摊销"]
[2,"C25现浇砼护坡","m3",{"v":3.2,"d":"3.20"},null,null,"模板、脚手架摊销"]
[3,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[4,"C25箱涵洞","m3",{"v":23.9,"d":"23.90"},null,null,"模板、脚手架摊销"]
[5,"C25耳墙","m3",{"v":11.3,"d":"11.30"},null,null,"模板、脚手架摊销"]
[6,"C25防撞护栏","m3",{"v":4.7,"d":"4.70"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作安装 ","t",4.86]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":10.1,"d":"10.10"}]
[2,"碎石垫层 ","m3",{"v":2.4,"d":"2.40"}]
[3,"黄砂垫层 ","m3",{"v":2.4,"d":"2.40"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[5,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[6,"桥铭牌","个",{"v":2,"d":"2.00"},null,null,"总价"]
[7,"限载标志","个",{"v":2,"d":"2.00"},null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",{"v":50,"d":"50.00"}]
[2,"施工降排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]

{"sheet":"赵庄镇赵庄村杨行北桥","index":83,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：83",null,"分组工程名称：赵庄镇赵庄村杨行北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":190,"d":"190.00"}]
[2,"土方回填压实","m3",{"v":130,"d":"130.00"}]
["二","混凝土工程"]
[1,"C25格梗","m3",{"v":1.2,"d":"1.20"},null,null,"模板、脚手架摊销"]
[2,"C25现浇砼护坡","m3",{"v":3.2,"d":"3.20"},null,null,"模板、脚手架摊销"]
[3,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[4,"C25箱涵洞","m3",{"v":34.8,"d":"34.80"},null,null,"模板、脚手架摊销"]
[5,"C25耳墙","m3",{"v":14.9,"d":"14.90"},null,null,"模板、脚手架摊销"]
[6,"C25防撞护栏","m3",{"v":4.5,"d":"4.50"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作安装 ","t",6.77]
["三","其他工程"]
[1,"碎石垫层 ","m3",{"v":2.4,"d":"2.40"}]
[2,"黄砂垫层 ","m3",{"v":2.4,"d":"2.40"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[4,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[5,"桥铭牌","个",{"v":2,"d":"2.00"},null,null,"总价"]
[6,"限载标志","个",{"v":2,"d":"2.00"},null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",{"v":50,"d":"50.00"}]
[2,"施工降排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]

{"sheet":"赵庄镇赵庄村杨行南桥","index":84,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[0,0,0,6],[1,2,1,6],[26,0,26,3],[26,4,26,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：84",null,"分组工程名称：赵庄镇赵庄村杨行南桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":130,"d":"130.00"}]
["二","混凝土工程"]
[1,"C25格梗","m3",{"v":1.4,"d":"1.40"},null,null,"模板、脚手架摊销"]
[2,"C25现浇砼护坡","m3",{"v":5.1,"d":"5.10"},null,null,"模板、脚手架摊销"]
[3,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[4,"C25箱涵洞","m3",{"v":37.2,"d":"37.20"},null,null,"模板、脚手架摊销"]
[5,"C25耳墙","m3",{"v":19,"d":"19.00"},null,null,"模板、脚手架摊销"]
[6,"C25防撞护栏","m3",{"v":6.3,"d":"6.30"},null,null,"模板、脚手架摊销"]
[7,"钢筋制作安装 ","t",{"v":7.6,"d":"7.60"}]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":27.5,"d":"27.50"}]
[2,"碎石垫层 ","m3",{"v":3.8,"d":"3.80"}]
[3,"黄砂垫层 ","m3",{"v":3.8,"d":"3.80"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[5,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[6,"桥铭牌","个",{"v":2,"d":"2.00"},null,null,"总价"]
[7,"限载标志","个",{"v":2,"d":"2.00"},null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",{"v":50,"d":"50.00"}]
[2,"施工降排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]

{"sheet":"赵庄镇王学屋陆庙桥","index":85,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6],[1,2,1,6],[22,0,22,3],[22,4,22,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：85",null,"分组工程名称：赵庄镇王学屋陆庙桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":140,"d":"140.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":22.1,"d":"22.10"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":9.7,"d":"9.70"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.7,"d":"4.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",4.46]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":10.8,"d":"10.80"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇王学屋村张后楼桥","index":86,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6],[1,2,1,6],[22,0,22,3],[22,4,22,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：86",null,"分组工程名称：赵庄镇王学屋村张后楼桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":230,"d":"230.00"}]
[2,"土方回填压实","m3",{"v":180,"d":"180.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":19.7,"d":"19.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":10.5,"d":"10.50"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.7,"d":"4.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",4.16]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":20.5,"d":"20.50"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇王学屋村齐小楼前桥","index":87,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：87",null,"分组工程名称：赵庄镇王学屋村齐小楼前桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":190,"d":"190.00"}]
[2,"土方回填压实","m3",{"v":130,"d":"130.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":34.8,"d":"34.80"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":14.9,"d":"14.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.5,"d":"4.50"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.77]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇孙庄村孙庄西桥","index":88,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：88",null,"分组工程名称：赵庄镇孙庄村孙庄西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":250,"d":"250.00"}]
[2,"土方回填压实","m3",{"v":200,"d":"200.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.2,"d":"2.20"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":23.9,"d":"23.90"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":13.6,"d":"13.60"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":100,"d":"100.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",5.09]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":10.1,"d":"10.10"}]
[2,"二灰结石 压实厚度（cm） 20","m2",{"v":110,"d":"110.00"}]
[3,"二灰结石 石灰土（cm） 30","m2",{"v":120,"d":"120.00"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[5,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇王龙庄村马楼东桥","index":89,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6],[1,2,1,6],[22,0,22,3],[22,4,22,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：89",null,"分组工程名称：赵庄镇王龙庄村马楼东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":230,"d":"230.00"}]
[2,"土方回填压实","m3",{"v":190,"d":"190.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":19.7,"d":"19.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.7,"d":"8.70"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.1,"d":"4.10"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",3.97]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":8.6,"d":"8.60"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇许庄村王堤口北桥","index":90,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：90",null,"分组工程名称：赵庄镇许庄村王堤口北桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":3.1,"d":"3.10"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.44]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"赵庄镇许庄村王堤口西桥","index":91,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：91",null,"分组工程名称：赵庄镇许庄村王堤口西桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":3.1,"d":"3.10"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.44]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"孙楼街道办事处高楼村高楼二队桥","index":92,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[0,0,0,6],[1,2,1,6],[34,0,34,3],[34,4,34,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：92",null,"分组工程名称：孙楼街道办事处高楼村高楼二队桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":60,"d":"60.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":109.2,"d":"109.20"}]
[2,"C25灌注桩混凝土","m3",{"v":54.9,"d":"54.90"}]
[3,"灌注桩钢筋笼制安","t",4.39]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":20.8,"d":"20.80"},null,null,"模板、脚手架摊销"]
[2,"C25桥墩","m3",{"v":3.6,"d":"3.60"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":38.9,"d":"38.90"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":17.1,"d":"17.10"},null,null,"模板、脚手架摊销"]
[5,"C25砼防撞栏杆","m3",{"v":14.7,"d":"14.70"},null,null,"模板、脚手架摊销"]
[6,"C20素砼格梗","m3",{"v":5.4,"d":"5.40"},null,null,"模板、脚手架摊销"]
[7,"C25现浇砼护坡","m3",{"v":15.7,"d":"15.70"},null,null,"模板、脚手架摊销"]
[8,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[9,"钢筋制作及安装","t",15.69]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":11.8,"d":"11.80"}]
[2,"黄砂垫层 ","m3",{"v":11.8,"d":"11.80"}]
[3,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[4,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",{"v":52.5,"d":"52.50"}]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[8,"桥铭牌","个",2,null,null,"总价"]
[9,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计",{"$nulls":3},{"v":0,"d":"0.00"}]

{"sheet":"孙楼街道办事处陈楼村孙三楼桥","index":93,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[0,0,0,6],[1,2,1,6],[34,0,34,3],[34,4,34,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：93",null,"分组工程名称：孙楼街道办事处陈楼村孙三楼桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":60,"d":"60.00"}]
[2,"土方回填压实","m3",{"v":90,"d":"90.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":73,"d":"73.00"}]
[2,"C25灌注桩混凝土","m3",{"v":36.7,"d":"36.70"}]
[3,"灌注桩钢筋笼制安","t",2.93]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":17,"d":"17.00"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":14.1,"d":"14.10"},null,null,"模板、脚手架摊销"]
[5,"C20素砼格梗","m3",{"v":10.5,"d":"10.50"},null,null,"模板、脚手架摊销"]
[6,"C25现浇砼护坡","m3",{"v":11.3,"d":"11.30"},null,null,"模板、脚手架摊销"]
[7,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[8,"钢筋制作及安装","t",{"v":9.5,"d":"9.50"}]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":8.5,"d":"8.50"}]
[2,"黄砂垫层 ","m3",{"v":8.5,"d":"8.50"}]
[3,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[4,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",26.25]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[8,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[9,"桥铭牌","个",2,null,null,"总价"]
[10,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"孙楼街道办事处张新庄村果园前桥","index":94,"n_rows":29,"n_cols":7,"rows_kept":29,"merged":[[0,0,0,6],[1,2,1,6],[28,0,28,3],[28,4,28,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：94",null,"分组工程名称：孙楼街道办事处张新庄村果园前桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":440,"d":"440.00"}]
[2,"土方回填压实","m3",{"v":280,"d":"280.00"}]
["二","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":5.5,"d":"5.50"},null,null,"模板、脚手架摊销"]
[2,"C25桥台墙身","m3",{"v":35.9,"d":"35.90"},null,null,"模板、脚手架摊销"]
[3,"C25桥台底板","m3",{"v":32.4,"d":"32.40"},null,null,"模板、脚手架摊销"]
[3,"C30桥面板预制","m3",{"v":9.6,"d":"9.60"},null,null,"模板、脚手架摊销"]
[4,"C40砼桥面铺装（含铰缝）","m3",{"v":4.8,"d":"4.80"},null,null,"模板、脚手架摊销"]
[5,"C25素砼格梗","m3",{"v":0.7,"d":"0.70"},null,null,"模板、脚手架摊销"]
[6,"C25现浇砼护坡","m3",{"v":0.1,"d":"0.10"},null,null,"模板、脚手架摊销"]
[7,"C25砼封底","m3",{"v":6.1,"d":"6.10"},null,null,"模板、脚手架摊销"]
[8,"C25砼防撞栏杆","m3",{"v":8.4,"d":"8.40"},null,null,"模板、脚手架摊销"]
[9,"钢筋制作及安装","t",9.18]
["四","其他工程"]
[1,"碎石垫层 ","m3",{"v":0.1,"d":"0.10"}]
[2,"黄砂垫层 ","m3",{"v":0.1,"d":"0.10"}]
[3,"桥面铸铁排水管（φ10）","m",{"v":5.2,"d":"5.20"}]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
[6,"老桥拆除","项",1,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"孙楼街道办事处张新庄村刘楼东桥","index":95,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6],[1,2,1,6],[22,0,22,3],[22,4,22,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：95",null,"分组工程名称：孙楼街道办事处张新庄村刘楼东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":140,"d":"140.00"}]
[2,"土方回填压实","m3",{"v":100,"d":"100.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":19.7,"d":"19.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":10.5,"d":"10.50"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":4.7,"d":"4.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",4.16]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":8.6,"d":"8.60"}]
[2,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[3,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[4,"桥铭牌","个",2,null,null,"总价"]
[5,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"孙楼街道办事处小学东桥","index":96,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：96",null,"分组工程名称：孙楼街道办事处小学东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":170,"d":"170.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":1.9,"d":"1.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":23.7,"d":"23.70"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":16.9,"d":"16.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.3,"d":"5.30"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",5.32]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"孙楼街道办事处前季庙庄桥","index":97,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：97",null,"分组工程名称：孙楼街道办事处前季庙庄桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":220,"d":"220.00"}]
[2,"土方回填压实","m3",{"v":170,"d":"170.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":2.7,"d":"2.70"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.2,"d":"37.20"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":19,"d":"19.00"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":6.5,"d":"6.50"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",7.61]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"孙楼镇三合村东桥","index":98,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,2,1,6],[21,0,21,3],[21,4,21,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：98",null,"分组工程名称：孙楼镇三合村东桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":210,"d":"210.00"}]
[2,"土方回填压实","m3",{"v":160,"d":"160.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":3.1,"d":"3.10"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":37.5,"d":"37.50"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":8.9,"d":"8.90"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":5.7,"d":"5.70"},null,null,"模板、脚手架摊销"]
[5,"钢筋制作安装 ","t",6.44]
["三","其他工程"]
[1,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[2,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[3,"桥铭牌","个",2,null,null,"总价"]
[4,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",50]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"宋楼镇史大楼桥","index":99,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[0,0,0,6],[1,2,1,6],[30,0,30,3],[30,4,30,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：99",null,"分组工程名称：宋楼镇史大楼桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":60,"d":"60.00"}]
[2,"土方回填压实","m3",{"v":70,"d":"70.00"}]
["二","桩基础工程"]
[1,"回旋钻机钻孔 ","m",{"v":80.2,"d":"80.20"}]
[2,"C25灌注桩混凝土","m3",{"v":40.3,"d":"40.30"}]
[3,"灌注桩钢筋笼制安","t",3.22]
["三","混凝土工程"]
[1,"C25冒梁、耳墙","m3",{"v":15.7,"d":"15.70"},null,null,"模板、脚手架摊销"]
[2,"C30桥面板预制","m3",{"v":19.5,"d":"19.50"},null,null,"模板、脚手架摊销"]
[3,"C40砼桥面铺装（含铰缝）","m3",{"v":8.6,"d":"8.60"},null,null,"模板、脚手架摊销"]
[4,"C25砼防撞栏杆","m3",{"v":8.7,"d":"8.70"},null,null,"模板、脚手架摊销"]
[5,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作及安装","t",8.63]
["四","其他工程"]
[1,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[2,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[5,"板式橡胶支座","dm3",26.25]
[6,"桥台GQF-F-6伸缩装置","m",{"v":12,"d":"12.00"}]
[7,"桥面铸铁排水管（φ10）","m",{"v":7.8,"d":"7.80"}]
[8,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[9,"桥铭牌","个",2,null,null,"总价"]
[10,"限载标志","个",2,null,null,"总价"]
["五","临时工程"]
[1,"围堰打拆","m3",300,null,null,"含打桩平台"]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]

{"sheet":"宋楼刘庄桥","index":100,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,2,1,6],[25,0,25,3],[25,4,25,6]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：100",null,"分组工程名称：宋楼刘庄桥"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":200,"d":"200.00"}]
[2,"土方回填压实","m3",{"v":150,"d":"150.00"}]
["二","混凝土工程"]
[1,"C25封底","m3",{"v":5.9,"d":"5.90"},null,null,"模板、脚手架摊销"]
[2,"C25箱涵洞","m3",{"v":57.3,"d":"57.30"},null,null,"模板、脚手架摊销"]
[3,"C25耳墙","m3",{"v":26.3,"d":"26.30"},null,null,"模板、脚手架摊销"]
[4,"C25防撞护栏","m3",{"v":7.1,"d":"7.10"},null,null,"模板、脚手架摊销"]
[5,"C30混凝土路面 压实厚度(cm) 20\n","m2",{"v":60,"d":"60.00"},null,null,"模板、脚手架摊销"]
[6,"钢筋制作安装 ","t",11.27]
["三","其他工程"]
[1,"换填级配碎石 压实度≥0.95","m3",{"v":13.3,"d":"13.30"}]
[2,"二灰结石 压实厚度（cm） 20","m2",{"v":64,"d":"64.00"}]
[3,"二灰结石 石灰土（cm） 30","m2",{"v":68,"d":"68.00"}]
[4,"桥面铸铁排水管（φ10）","m",{"v":2.6,"d":"2.60"}]
[5,"老桥拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
[6,"桥铭牌","个",2,null,null,"总价"]
[7,"限载标志","个",2,null,null,"总价"]
["四","临时工程"]
[1,"围堰打拆","m3",100]
[2,"施工降排水","项",1,null,null,"总价"]
[3,"其他临时工程","项",1,null,null,"总价"]
["合计"]