{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["区域供水完善管材03标段汇总表","区域供水完善管材03标段管材清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"区域供水完善管材03标段汇总表","index":0,"n_rows":10,"n_cols":3,"rows_kept":10,"merged":[[0,0,0,2],[6,0,6,2]],"flags":["formulas_cached_only"]}
["铜山区城乡供水一体化工程区域供水完善工程球墨铸铁管采购03标段                      投标报价汇总表"]
["组号","工程名称","报价金额(元)"]
["一","管材管件"]
["二","到工检测试验费","管材管件费的5%"]
["三","备用金",{"v":390000,"d":"390000.00"}]
[null,"投标报价总金额=一+二+三"]
["注：到工检测试验费由招标人掌握使用。"]
[null,"                                        投标人：(盖单位章)"]
[null,"                                       法定代表人（或委托代理人）（签名）："]
[null,"                                               年     月     日"]

{"sheet":"区域供水完善管材03标段管材清单","index":1,"n_rows":41,"n_cols":8,"rows_kept":41,"merged":[[0,0,0,7],[37,0,37,7]],"flags":["formulas_cached_only"]}
["铜山区城乡供水一体化工程区域供水完善工程球墨铸铁管采购03标段\n材料采购清单"]
["序号","材料名称","项目特征描述","计量\r\n单位","工程量","单价（元）","合价（元）","备注"]
["一","管材管件"]
[1,"铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN800\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",5792]
[2,"铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN600\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",5805]
[3,"铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN300\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",694]
[4,"铸铁管","1.垫层、基础材质及厚度:砂垫层200厚\n2.材质及规格:球墨铸铁DN200\n3.接口方式:胶圈接口\n4.铺设深度:1.5m\n5.管道检验及试验要求:1.0MPa","m",10]
[5,"盲堵板","1.名称：法兰盲板\n2.材质规格：球墨铸铁 DN800","个",1]
[6,"盲堵板","1.名称：法兰盲板\n2.材质规格：球墨铸铁 DN200","个",3]
[7,"铸铁管管件","1.种类:盘承短管\n2.材质及规格:球墨铸铁 DN800\n3.接口形式:胶圈接口","个",1]
[8,"铸铁管管件","1.种类:盘插短管\n2.材质及规格:球墨铸铁 DN800\n3.接口形式:胶圈接口","个",1]
[9,"铸铁管管件","1.种类:盘承短管\n2.材质及规格:球墨铸铁 DN600\n3.接口形式:胶圈接口","个",8]
[10,"铸铁管管件","1.种类:盘插短管\n2.材质及规格:球墨铸铁 DN600\n3.接口形式:胶圈接口","个",8]
[11,"铸铁管管件","1.种类:45°弯头\n2.材质及规格:球墨铸铁、DN800\n3.接口形式:胶圈接口","个",1]
[12,"铸铁管管件","1.种类:11.25°弯头\n2.材质及规格:球墨铸铁、DN600\n3.接口形式:胶圈接口","个",12]
[13,"铸铁管管件","1.种类:22.5° 弯头\n2.材质及规格:球墨铸铁、DN600\n3.接口形式:胶圈接口","个",2]
[14,"铸铁管管件","1.种类:90°弯头\n2.材质及规格:球墨铸铁、DN600\n3.接口形式:胶圈接口","个",1]
[15,"铸铁管管件","1.种类:插堵\n2.材质及规格:球墨铸铁 DN300\n3.接口形式:胶圈接口","个",1]
[16,"铸铁管管件","1.种类:盘插短管\n2.材质及规格:球墨铸铁 DN300\n3.接口形式:胶圈接口","个",1]
[17,"铸铁管管件","1.种类:盘承短管\n2.材质及规格:球墨铸铁 DN300\n3.接口形式:胶圈接口","个",1]
[18,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN300×200\n3.接口形式:橡胶圈","个",1]
[19,"铸铁管管件","1.种类:钢塑转换管件\n2.材质及规格:DN300","个",2]
[20,"铸铁管管件","1.种类:闷板\n2.材质及规格:球墨铸铁 DN200","个",1]
[21,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁、DN800×DN200\n3.接口形式:胶圈接口","个",1]
[22,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁、DN800×DN300\n3.接口形式:胶圈接口","个",1]
[23,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁、DN600×DN200\n3.接口形式:胶圈接口","个",3]
[24,"盲堵板","1.名称：法兰承堵\n2.材质规格：球墨铸铁 DN600","个",1]
[25,"盲堵板","1.名称：法兰闷板\n2.材质规格：球墨铸铁 DN200","个",1]
[26,"盲堵板","1.名称：法兰闷板\n2.材质规格：球墨铸铁 DN300","个",1]
[27,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN800×250\n3.接口形式:橡胶圈","个",4]
[28,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁 DN800×100 P=1.0MPa；","个",14]
[29,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN800×250\n3.接口形式:橡胶圈","个",2]
[30,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN600×200\n3.接口形式:橡胶圈","个",3]
[31,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁 DN600×80 P=1.0MPa；","个",6]
[32,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁，DN300×100\n3.接口形式:橡胶圈","个",1]
[33,"铸铁管管件","1.种类:承插单支盘三通\n2.材质及规格:球墨铸铁 DN300×80 P=1.0MPa；","个",1]
["二","到工检测试验费",null,"项",1]
["注：（1）管材及管件均应符合《水及燃气管道用球墨铸铁管、管件及附件》（GB/T 13295-2008）要求；\n（2）管道采用K9级球墨铸铁管，T型接口，橡胶圈连接（SBR），且包含在投标报价中。橡胶圈符合国家供水行业规定标准，\n使用寿命不低于铸铁管道使用寿命。供货方供货时需提供相应的行业质量检测报告。\n（3）管件及附件采用K12级球墨铸铁，管道、管件及附件材料要求应符合《生活饮用水输配水设备及防护材料的安全性评价标准》（GB/T 17219）的规定；其它详见技术条款。\n（4）球墨铸铁管厂家需足额提供管材转换处配套螺栓螺母。"]
[null,null,"                                 投标人：(盖单位章)"]
[null,null,"                                               法定代表人(或委托代理人)：(签名)"]
[null,null,"                                         年     月     日"]