{"text_format":"3","workbook":"xls","n_sheets":22,"sheets":["扉页","投标报价汇总表","3.1 表-08 分部分项工程和单价措施项目清单与计价表","3.2 表-11 总价措施项目清单与计价表","3.3 表-12 其他项目清单与计价汇总表","3.9 表-13 规费、税金项目计价表","4.1 表-08 分部分项工程和单价措施项目清单与计价表","4.2 表-11 总价措施项目清单与计价表","4.3 表-12 其他项目清单与计价汇总表","4.9 表-13 规费、税金项目计价表","5.1 表-08 分部分项工程和单价措施项目清单与计价表","5.2 表-11 总价措施项目清单与计价表","5.3 表-12 其他项目清单与计价汇总表","5.9 表-13 规费、税金项目计价表","6.1 表-08 分部分项工程和单价措施项目清单与计价表","6.2 表-11 总价措施项目清单与计价表","6.3 表-12 其他项目清单与计价汇总表","6.9 表-13 规费、税金项目计价表","7.1 表-08 分部分项工程和单价措施项目清单与计价表","7.2 表-11 总价措施项目清单与计价表","7.3 表-12 其他项目清单与计价汇总表","7.9 表-13 规费、税金项目计价表"],"not_rendered":{"external_links":1,"defined_names":19},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"扉页","index":0,"n_rows":10,"n_cols":6,"rows_kept":10,"merged":[[0,0,0,6],[1,0,1,6],[2,1,2,2],[2,5,2,6],[3,1,3,3],[3,5,3,6],[4,1,4,3],[4,5,4,6],[5,1,5,3],[5,5,5,6],[6,1,6,3],[6,5,6,6],[7,1,7,3],[7,5,7,6],[8,1,8,3],[8,5,8,6],[9,1,9,3],[9,5,9,6],[10,0,10,1],[10,2,10,5]],"flags":["formulas_cached_only"]}
["邳州市城区部分道路路面积水整治工程"]
["招 标 工 程 量 清 单"]
[]
["招  标  人：",{"$nulls":3},"造价咨询人："]
[null,"（单位盖章）",{"$nulls":3},"(单位资质专用章)"]
["法定代表人  \n\n或其授权人：",{"$nulls":3},"法定代表人  \n\n  或其授权人："]
[null,"(签字或盖章)",{"$nulls":3},"(签字或盖章)"]
["编  制  人：",{"$nulls":3},"复  核  人："]
[null,"(造价人员签字盖专用章)",{"$nulls":3},"(造价工程师签字盖专用章)"]
["编 制 时 间：  ",{"$nulls":3},"复 核 时 间："]

{"sheet":"投标报价汇总表","index":1,"n_rows":21,"n_cols":8,"rows_kept":21,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,5],[1,6,1,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,2,7],[3,3,3,4],[3,5,3,6],[4,3,4,4],[4,5,4,6],[5,3,5,4],[5,5,5,6],[6,3,6,4],[6,5,6,6],[7,3,7,4],[7,5,7,6],[8,3,8,4],[8,5,8,6],[9,3,9,4],[9,5,9,6],[10,3,10,4],[10,5,10,6],[11,3,11,4],[11,5,11,6],[12,3,12,4],[12,5,12,6],[13,3,13,4],[13,5,13,6],[14,3,14,4],[14,5,14,6],[15,3,15,4],[15,5,15,6],[16,3,16,4],[16,5,16,6],[17,3,17,4],[17,5,17,6],[18,3,18,4],[18,5,18,6],[19,3,19,4],[19,5,19,6],[20,0,20,1],[20,3,20,4],[20,5,20,6],[21,0,21,3],[21,4,21,5],[21,6,21,7]],"flags":["formulas_cached_only"]}
["投标报价汇总表"]
["工程名称：邳州市城区部分道路路面积水整治工程",{"$nulls":5},"第 1 页  共 1 页"]
["序号","单项工程名称","金额（元）","其中: （元）"]
[{"$nulls":3},"暂估价",null,"安全文明施工费",null,"规费"]
["1","邳新路～瑞兴南路路面积水整治工程"]
[2,"三汊河路（瑞兴南路-六保河）路面积水整治工程"]
[3,"三汊河路（东兴路-李口大沟）路面积水整治工程"]
[4,"乐园街-人民路路面积水整治工程"]
[5,"民主路（大榆树街-花园路）路面积水整治工程"]
{"$rows_empty":11}
["合计"]

{"sheet":"3.1 表-08 分部分项工程和单价措施项目清单与计价表","index":2,"n_rows":140,"n_cols":12,"rows_kept":140,"merged":[[0,0,0,11],[1,0,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,7],[2,8,2,11],[3,8,4,9],[3,10,4,10],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,7],[5,8,6,9],[5,10,6,10],[5,11,6,11],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,7],[7,8,8,9],[7,10,8,10],[7,11,8,11],[9,5,9,7],[9,8,9,9],[10,5,10,7],[10,8,10,9],[11,0,13,0],[11,1,13,1],[11,2,13,2],[11,3,13,3],[11,4,13,4],[11,5,13,7],[11,8,13,9],[11,10,13,10],[11,11,13,11],[14,0,16,0],[14,1,16,1],[14,2,16,2],[14,3,16,3],[14,4,16,4],[14,5,16,7],[14,8,16,9],[14,10,16,10],[14,11,16,11],[17,5,17,7],[17,8,17,9],[18,5,18,7],[18,8,18,9],[19,0,19,9],[21,4,21,11],[22,0,22,11],[23,0,23,5],[23,6,23,8],[23,9,23,11],[24,0,26,0],[24,1,26,1],[24,2,26,2],[24,3,26,3],[24,4,26,4],[24,5,26,7],[24,8,24,11],[25,8,26,9],[25,10,26,10],[27,0,29,0],[27,1,29,1],[27,2,29,2],[27,3,29,3],[27,4,29,4],[27,5,29,7],[27,8,29,9],[27,10,29,10],[27,11,29,11],[30,5,30,7],[30,8,30,9],[31,5,31,7],[31,8,31,9],[32,0,34,0],[32,1,34,1],[32,2,34,2],[32,3,34,3],[32,4,34,4],[32,5,34,7],[32,8,34,9],[32,10,34,10],[32,11,34,11],[35,5,35,7],[35,8,35,9],[36,5,36,7],[36,8,36,9],[37,5,37,7],[37,8,37,9],[38,5,38,7],[38,8,38,9],[39,5,39,7],[39,8,39,9],[40,5,40,7],[40,8,40,9],[41,5,41,7],[41,8,41,9],[42,5,42,7],[42,8,42,9],[43,5,43,7],[43,8,43,9],[44,0,44,9],[46,4,46,11],[47,0,47,11],[48,0,48,5],[48,6,48,8],[48,9,48,11],[49,0,51,0],[49,1,51,1],[49,2,51,2],[49,3,51,3],[49,4,51,4],[49,5,51,7],[49,8,49,11],[50,8,51,9],[50,10,51,10],[52,0,54,0],[52,1,54,1],[52,2,54,2],[52,3,54,3],[52,4,54,4],[52,5,54,7],[52,8,54,9],[52,10,54,10],[52,11,54,11],[55,0,57,0],[55,1,57,1],[55,2,57,2],[55,3,57,3],[55,4,57,4],[55,5,57,7],[55,8,57,9],[55,10,57,10],[55,11,57,11],[58,0,60,0],[58,1,60,1],[58,2,60,2],[58,3,60,3],[58,4,60,4],[58,5,60,7],[58,8,60,9],[58,10,60,10],[58,11,60,11],[61,5,61,7],[61,8,61,9],[62,5,62,7],[62,8,62,9],[63,5,63,7],[63,8,63,9],[64,5,64,7],[64,8,64,9],[65,5,65,7],[65,8,65,9],[66,5,66,7],[66,8,66,9],[67,0,67,9],[69,4,69,11],[70,0,70,11],[71,0,71,5],[71,6,71,8],[71,9,71,11],[72,0,74,0],[72,1,74,1],[72,2,74,2],[72,3,74,3],[72,4,74,4],[72,5,74,7],[72,8,72,11],[73,8,74,9],[73,10,74,10],[75,0,77,0],[75,1,77,1],[75,2,77,2],[75,3,77,3],[75,4,77,4],[75,5,77,7],[75,8,77,9],[75,10,77,10],[75,11,77,11],[78,0,80,0],[78,1,80,1],[78,2,80,2],[78,3,80,3],[78,4,80,4],[78,5,80,7],[78,8,80,9],[78,10,80,10],[78,11,80,11],[81,0,82,0],[81,1,82,1],[81,2,82,2],[81,3,82,3],[81,4,82,4],[81,5,82,7],[81,8,82,9],[81,10,82,10],[81,11,82,11],[83,0,85,0],[83,1,85,1],[83,2,85,2],[83,3,85,3],[83,4,85,4],[83,5,85,7],[83,8,85,9],[83,10,85,10],[83,11,85,11],[86,5,86,7],[86,8,86,9],[87,0,87,9],[89,4,89,11],[90,0,90,11],[91,0,91,5],[91,6,91,8],[91,9,91,11],[92,0,94,0],[92,1,94,1],[92,2,94,2],[92,3,94,3],[92,4,94,4],[92,5,94,7],[92,8,92,11],[93,8,94,9],[93,10,94,10],[95,5,95,7],[95,8,95,9],[96,0,97,0],[96,1,97,1],[96,2,97,2],[96,3,97,3],[96,4,97,4],[96,5,97,7],[96,8,97,9],[96,10,97,10],[96,11,97,11],[98,5,98,7],[98,8,98,9],[99,0,101,0],[99,1,101,1],[99,2,101,2],[99,3,101,3],[99,4,101,4],[99,5,101,7],[99,8,101,9],[99,10,101,10],[99,11,101,11],[102,0,103,0],[102,1,103,1],[102,2,103,2],[102,3,103,3],[102,4,103,4],[102,5,103,7],[102,8,103,9],[102,10,103,10],[102,11,103,11],[104,5,104,7],[104,8,104,9],[105,5,105,7],[105,8,105,9],[106,5,106,7],[106,8,106,9],[107,5,107,7],[107,8,107,9],[108,5,108,7],[108,8,108,9],[109,5,109,7],[109,8,109,9],[110,0,110,9],[112,4,112,11],[113,0,113,11],[114,0,114,5],[114,6,114,8],[114,9,114,11],[115,0,117,0],[115,1,117,1],[115,2,117,2],[115,3,117,3],[115,4,117,4],[115,5,117,7],[115,8,115,11],[116,8,117,9],[116,10,117,10],[118,5,118,7],[118,8,118,9],[119,5,119,7],[119,8,119,9],[120,5,120,7],[120,8,120,9],[121,5,121,7],[121,8,121,9],[122,5,122,7],[122,8,122,9],[123,5,123,7],[123,8,123,9],[124,5,124,7],[124,8,124,9],[125,2,125,3],[125,5,125,7],[125,8,125,9],[126,5,126,7],[126,8,126,9],[127,5,127,7],[127,8,127,9],[128,5,128,7],[128,8,128,9],[129,5,129,7],[129,8,129,9],[130,5,130,7],[130,8,130,9],[131,2,131,3],[131,5,131,7],[131,8,131,9],[132,5,132,7],[132,8,132,9],[133,5,133,7],[133,8,133,9],[134,5,134,7],[134,8,134,9],[135,5,135,7],[135,8,135,9],[136,0,136,9],[137,0,137,9],[139,4,139,11]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第1页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["1","040101002006","挖沟槽土方","1、机械挖土人工清理\n2、土壤类别：三类土\n3、挖土深度：4M内\n4、土方堆放：投标方自行考虑","m3","8743"]
[]
["2","040103001016","回填土方","1、密实度要求：按设计要求\n2、填方材料品种：土方\n3、填方来源、运距：符合要求的原状土、运距投标方自行考虑","m3","1605"]
[]
["3","040103002001","余方弃置","1、废弃料品种：外运废方\n2、余方外运：20KM","m3","7138"]
["4","040103001017","回填方 6%灰土","1、密实度要求：按设计要求\n2、填方材料品种：6%灰土，原土利用","m3","3411"]
["5","040501001003","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用90°-C20砼基础\n3、规格：d300钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","42"]
[]
[]
["6","040501001001","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用135°-C20砼基础\n3、规格：d600钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","20"]
[]
[]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第2页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["7","040501001002","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d1000钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","262"]
[]
[]
["8","040306004002","钢筋砼箱涵","1、管涵类型：钢筋砼箱涵\n2、尺寸：BXH=3.0X2.0m\n3、其他按设计图纸要求","m","232"]
["9","040306004001","破修现状箱涵","1、管涵类型：钢筋砼箱涵\n2、尺寸：BXH=1.0X1.7m\n3、破除及修复","m","8"]
["10","040504009001","雨水口","1、收水井采用偏沟式砖砌单篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","14"]
{"$rows_empty":11}
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第3页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["11","040504009002","雨水口","1、收水井采用偏沟式砖砌双篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","2"]
[]
[]
["12","040504001015","砌筑井","1、盖板式砖砌圆形1500排水检查井\n2、规格：1500\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","7"]
[]
[]
["13","040504001006","砌筑井","1、砖砌圆矩形1650×1650排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、成品预制砼井筒\n5、井筒内均应设置防坠落板（质量符合设计要求）","座","2"]
{"$rows_empty":8}
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第4页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["14","040504002015","混凝土井","1、1800×1100钢筋砼矩形排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、成品预制砼井筒\n5、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["15","040504002014","混凝土井","1、1300×1000钢筋砼矩形排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、成品预制砼井筒\n5、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["16","040504001016","沟上排水检查井","1、沟上排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","8"]
[]
["17","040504001017","检查井","1、破坏修复现状排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","2"]
[]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第5页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["18","040602031001","截污闸","1、B=3.0m截污闸\n2、具体做法详见施工图","座","1"]
["19","040602031002","闸门安装","1、铸铁镶铜闸门SFZ3000×2000\n2、启闭机选用单吊点手电两用启闭机，与闸门配套安装\n3、其他具体要求按施工图纸","座","1"]
[]
["20","040602035002","单吊点手电两用启闭机","1、单吊点手电两用启闭机\n2、与闸门SFZ3000X2000配套","台","1"]
["21","040504002016","混凝土井","1、2000×1500钢筋砼矩形闸门井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、成品预制砼井筒\n5、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["22","040602031003","闸门安装","1、铸铁镶铜闸门SYZ600\n2、启闭机选用手电两用启闭机，与闸门配套安装\n3、其他具体要求按施工图纸","座","1"]
[]
["23","040602035001","QDA-45型单吊点手电两用启闭机","QDA-45型单吊点手电两用启闭机","台","1"]
["24","041001002002","破修现状路面","1、现状路面破除\n2、施工结束后原状恢复","m2","1965"]
["25","041001002003","拆除及修复人行道","1、现状人行道破除\n2、施工结束后原状恢复","m2","300"]
["26","041001001010","破坏及修复现状绿化","1、破除现状绿化\n2、施工结束后原状恢复","m2","300"]
["27","041001005001","拆除及修复现状路牙石","1、现状路牙石破除\n2、施工结束后原状恢复","m","594"]
["28","040203007002","拆除及恢复公交站台","1、现状公交站台拆除\n2、施工结束后原状恢复","座","1"]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第6页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["29","041001007003","现状钢筋砼挡墙拆除及修复","1、现状钢筋砼挡墙破除\n2、施工结束后原状恢复","m2","16"]
["30","040303002002","管道包封混凝土基础","1、管道包封\n2、混凝土强度等级：C25商品混凝土","m3","8.8"]
["31","040901001001","管道包封现浇构件钢筋","1、钢筋种类：10以内\n2、其他按设计要求","t","0.183"]
["32","040305001001","管道包封 碎石垫层","1、材料品种、规格：碎石","m3","1.5"]
["33","040201022001","污水导流","1、污水导流时间为施工期；\n2、流量 1000m3/d。","项","1"]
["34","010202006003","钢板桩","1、钢板桩类型：拉森钢板桩SP-III\n2、桩长：10m内","t","900"]
["35","041001010002","现状（给水、弱电、燃气等）管线支护保护","现状（给水、弱电、燃气等）管线支护保护","处","2"]
[null,null,"分部分项合计",null,null,""]
["1","041107002005","轻型井点降水",null,"m","522"]
["2","041107002006","汛期应急排水（投标方自行考虑，需满足汛期应急排水要求）","1、汛期应急排水\n2、费用由投标方自行考虑","项","1"]
["3","041103001001","围堰（草袋围堰）",null,"m3","320"]
["4","041107002003","排水",null,"项",1]
["5","041106001001","大型机械设备进出场及安拆",null,"项","1"]
[null,null,"单价措施合计",null,null,""]
[]
[]
[]
[]
["本页小计"]
["合    计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"3.2 表-11 总价措施项目清单与计价表","index":3,"n_rows":57,"n_cols":12,"rows_kept":57,"merged":[[0,0,0,12],[1,0,1,6],[1,7,1,8],[1,9,1,12],[2,2,2,3],[2,6,2,8],[2,11,2,12],[3,2,3,3],[3,6,3,8],[3,11,3,12],[4,2,4,3],[4,6,4,8],[4,11,4,12],[5,2,5,3],[5,6,5,8],[5,11,5,12],[6,2,6,3],[6,6,6,8],[6,11,6,12],[7,2,7,3],[7,6,7,8],[7,11,7,12],[8,2,8,3],[8,6,8,8],[8,11,8,12],[9,2,9,3],[9,6,9,8],[9,11,9,12],[10,2,10,3],[10,6,10,8],[10,11,10,12],[11,2,11,3],[11,6,11,8],[11,11,11,12],[12,2,12,3],[12,6,12,8],[12,11,12,12],[13,2,13,3],[13,6,13,8],[13,11,13,12],[14,2,14,3],[14,6,14,8],[14,11,14,12],[15,2,15,3],[15,6,15,8],[15,11,15,12],[16,0,16,12],[17,5,17,12],[18,0,18,2],[18,8,18,11],[19,0,19,12],[20,0,20,6],[20,7,20,8],[20,9,20,12],[21,2,21,3],[21,6,21,8],[21,11,21,12],[22,2,22,3],[22,6,22,8],[22,11,22,12],[23,2,23,3],[23,6,23,8],[23,11,23,12],[24,2,24,3],[24,6,24,8],[24,11,24,12],[25,2,25,3],[25,6,25,8],[25,11,25,12],[26,2,26,3],[26,6,26,8],[26,11,26,12],[27,2,27,3],[27,6,27,8],[27,11,27,12],[28,2,28,3],[28,6,28,8],[28,11,28,12],[29,2,29,3],[29,6,29,8],[29,11,29,12],[30,2,30,3],[30,6,30,8],[30,11,30,12],[31,2,31,3],[31,6,31,8],[31,11,31,12],[32,2,32,3],[32,6,32,8],[32,11,32,12],[33,2,33,3],[33,6,33,8],[33,11,33,12],[34,2,34,3],[34,6,34,8],[34,11,34,12],[35,2,35,3],[35,6,35,8],[35,11,35,12],[36,2,36,3],[36,6,36,8],[36,11,36,12],[37,2,37,3],[37,6,37,8],[37,11,37,12],[38,2,38,3],[38,6,38,8],[38,11,38,12],[39,2,39,3],[39,6,39,8],[39,11,39,12],[40,2,40,3],[40,6,40,8],[40,11,40,12],[41,2,41,3],[41,6,41,8],[41,11,41,12],[42,2,42,3],[42,6,42,8],[42,11,42,12],[43,2,43,3],[43,6,43,8],[43,11,43,12],[44,2,44,3],[44,6,44,8],[44,11,44,12],[45,2,45,3],[45,6,45,8],[45,11,45,12],[46,2,46,3],[46,6,46,8],[46,11,46,12],[47,2,47,3],[47,6,47,8],[47,11,47,12],[48,2,48,3],[48,6,48,8],[48,11,48,12],[49,2,49,3],[49,6,49,8],[49,11,49,12],[50,2,50,3],[50,6,50,8],[50,11,50,12],[51,2,51,3],[51,6,51,8],[51,11,51,12],[52,2,52,3],[52,6,52,8],[52,11,52,12],[53,2,53,3],[53,6,53,8],[53,11,53,12],[54,0,54,12],[55,5,55,12],[56,0,56,2],[56,8,56,11]],"flags":["formulas_cached_only"]}
["总价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":6},"标段：",null,"第1页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["1","041109001001","安全文明施工费",null,null,""]
["1.1",null,"基本费",null,"分部分项合计+单价措施项目合计-除税工程设备费","1.500"]
["1.2",null,"增加费",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["2","041109002001","夜间施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["3","041109003001","二次搬运",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["4","041109004001","冬雨季施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["5","041109005001","行车、行人干扰",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["6","041109006001","地上、地下设施、建筑物的临时保护设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["7","041109007001","已完工程及设备保护",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["8","041109008001","临时设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["9","041109009001","赶工措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
[]
[]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]
["总价措施项目清单与计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":6},"标段：",null,"第2页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["10","041109010001","工程按质论价",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["11","041109011001","扬尘防治专项措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
{"$rows_empty":31}
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]

{"sheet":"3.3 表-12 其他项目清单与计价汇总表","index":4,"n_rows":43,"n_cols":8,"rows_kept":43,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,5],[1,6,1,7],[2,3,2,6],[3,3,3,6],[4,3,4,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,3,11,6],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[23,3,23,6],[24,3,24,6],[25,3,25,6],[26,3,26,6],[27,3,27,6],[28,3,28,6],[29,3,29,6],[30,3,30,6],[31,3,31,6],[32,3,32,6],[33,3,33,6],[34,3,34,6],[35,3,35,6],[36,3,36,6],[37,3,37,6],[38,3,38,6],[39,3,39,6],[40,0,40,1],[40,3,40,6],[42,5,42,7]],"flags":["formulas_cached_only"]}
["其他项目清单与计价汇总表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":3},"标段：",null,"第1页 共1页"]
["序号","项目名称","金额(元)","结算金额(元)",{"$nulls":3},"备注"]
["1","暂列金额",""]
["2","暂估价",""]
["2.1","材料暂估价",""]
["2.2","专业工程暂估价",""]
["3","计日工",""]
["4","总承包服务费",""]
{"$rows_empty":31}
["合  计",null,""]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"3.9 表-13 规费、税金项目计价表","index":5,"n_rows":34,"n_cols":10,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,6],[1,7,1,10],[2,2,2,5],[2,6,2,7],[2,9,2,10],[3,2,3,5],[3,6,3,7],[3,9,3,10],[4,2,4,5],[4,6,4,7],[4,9,4,10],[5,2,5,5],[5,6,5,7],[5,9,5,10],[6,2,6,5],[6,6,6,7],[6,9,6,10],[7,2,7,5],[7,6,7,7],[7,9,7,10],[8,2,8,5],[8,6,8,7],[8,9,8,10],[9,2,9,5],[9,6,9,7],[9,9,9,10],[10,2,10,5],[10,6,10,7],[10,9,10,10],[11,2,11,5],[11,6,11,7],[11,9,11,10],[12,2,12,5],[12,6,12,7],[12,9,12,10],[13,2,13,5],[13,6,13,7],[13,9,13,10],[14,2,14,5],[14,6,14,7],[14,9,14,10],[15,2,15,5],[15,6,15,7],[15,9,15,10],[16,2,16,5],[16,6,16,7],[16,9,16,10],[17,2,17,5],[17,6,17,7],[17,9,17,10],[18,2,18,5],[18,6,18,7],[18,9,18,10],[19,2,19,5],[19,6,19,7],[19,9,19,10],[20,2,20,5],[20,6,20,7],[20,9,20,10],[21,2,21,5],[21,6,21,7],[21,9,21,10],[22,2,22,5],[22,6,22,7],[22,9,22,10],[23,2,23,5],[23,6,23,7],[23,9,23,10],[24,2,24,5],[24,6,24,7],[24,9,24,10],[25,2,25,5],[25,6,25,7],[25,9,25,10],[26,2,26,5],[26,6,26,7],[26,9,26,10],[27,2,27,5],[27,6,27,7],[27,9,27,10],[28,2,28,5],[28,6,28,7],[28,9,28,10],[30,0,30,8],[30,9,30,10],[32,5,32,10],[33,0,33,2],[33,5,33,9]],"flags":["formulas_cached_only"]}
["规费、税金项目计价表"]
["工程名称：邳新路～瑞兴南路路面积水整治工程",{"$nulls":3},"标段：",null,null,"第1页 共1页"]
["序号","项目名称","计算基础",{"$nulls":3},"计算基数(元)",null,"计算费率(％)","金额(元)"]
["1","规费","工程排污费+社会保险费+住房公积金",{"$nulls":5},"100.000"]
["1.1","社会保险费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"2.000"]
["1.2","住房公积金","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"0.340"]
["1.3","工程排污费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},""]
["2","税金","分部分项工程费+措施项目费+其他项目费+规费-除税甲供材料和甲供设备费/1.01",{"$nulls":5},"11.000"]
{"$rows_empty":22}
["合  计"]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":4},"复核人（造价工程师）："]

{"sheet":"4.1 表-08 分部分项工程和单价措施项目清单与计价表","index":6,"n_rows":169,"n_cols":12,"rows_kept":169,"merged":[[0,0,0,11],[1,0,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,7],[2,8,2,11],[3,8,4,9],[3,10,4,10],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,7],[5,8,6,9],[5,10,6,10],[5,11,6,11],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,7],[7,8,8,9],[7,10,8,10],[7,11,8,11],[9,5,9,7],[9,8,9,9],[10,5,10,7],[10,8,10,9],[11,0,13,0],[11,1,13,1],[11,2,13,2],[11,3,13,3],[11,4,13,4],[11,5,13,7],[11,8,13,9],[11,10,13,10],[11,11,13,11],[14,0,16,0],[14,1,16,1],[14,2,16,2],[14,3,16,3],[14,4,16,4],[14,5,16,7],[14,8,16,9],[14,10,16,10],[14,11,16,11],[17,0,17,9],[19,4,19,11],[20,0,20,11],[21,0,21,5],[21,6,21,8],[21,9,21,11],[22,0,24,0],[22,1,24,1],[22,2,24,2],[22,3,24,3],[22,4,24,4],[22,5,24,7],[22,8,22,11],[23,8,24,9],[23,10,24,10],[25,0,27,0],[25,1,27,1],[25,2,27,2],[25,3,27,3],[25,4,27,4],[25,5,27,7],[25,8,27,9],[25,10,27,10],[25,11,27,11],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[28,5,30,7],[28,8,30,9],[28,10,30,10],[28,11,30,11],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[31,5,33,7],[31,8,33,9],[31,10,33,10],[31,11,33,11],[34,5,34,7],[34,8,34,9],[35,5,35,7],[35,8,35,9],[36,5,36,7],[36,8,36,9],[37,5,37,7],[37,8,37,9],[38,0,38,9],[40,4,40,11],[41,0,41,11],[42,0,42,5],[42,6,42,8],[42,9,42,11],[43,0,45,0],[43,1,45,1],[43,2,45,2],[43,3,45,3],[43,4,45,4],[43,5,45,7],[43,8,43,11],[44,8,45,9],[44,10,45,10],[46,0,48,0],[46,1,48,1],[46,2,48,2],[46,3,48,3],[46,4,48,4],[46,5,48,7],[46,8,48,9],[46,10,48,10],[46,11,48,11],[49,0,51,0],[49,1,51,1],[49,2,51,2],[49,3,51,3],[49,4,51,4],[49,5,51,7],[49,8,51,9],[49,10,51,10],[49,11,51,11],[52,0,54,0],[52,1,54,1],[52,2,54,2],[52,3,54,3],[52,4,54,4],[52,5,54,7],[52,8,54,9],[52,10,54,10],[52,11,54,11],[55,5,55,7],[55,8,55,9],[56,5,56,7],[56,8,56,9],[57,5,57,7],[57,8,57,9],[58,0,58,9],[60,4,60,11],[61,0,61,11],[62,0,62,5],[62,6,62,8],[62,9,62,11],[63,0,65,0],[63,1,65,1],[63,2,65,2],[63,3,65,3],[63,4,65,4],[63,5,65,7],[63,8,63,11],[64,8,65,9],[64,10,65,10],[66,0,68,0],[66,1,68,1],[66,2,68,2],[66,3,68,3],[66,4,68,4],[66,5,68,7],[66,8,68,9],[66,10,68,10],[66,11,68,11],[69,0,71,0],[69,1,71,1],[69,2,71,2],[69,3,71,3],[69,4,71,4],[69,5,71,7],[69,8,71,9],[69,10,71,10],[69,11,71,11],[72,0,74,0],[72,1,74,1],[72,2,74,2],[72,3,74,3],[72,4,74,4],[72,5,74,7],[72,8,74,9],[72,10,74,10],[72,11,74,11],[75,5,75,7],[75,8,75,9],[76,5,76,7],[76,8,76,9],[77,5,77,7],[77,8,77,9],[78,5,78,7],[78,8,78,9],[79,0,79,9],[81,4,81,11],[82,0,82,11],[83,0,83,5],[83,6,83,8],[83,9,83,11],[84,0,86,0],[84,1,86,1],[84,2,86,2],[84,3,86,3],[84,4,86,4],[84,5,86,7],[84,8,84,11],[85,8,86,9],[85,10,86,10],[87,0,89,0],[87,1,89,1],[87,2,89,2],[87,3,89,3],[87,4,89,4],[87,5,89,7],[87,8,89,9],[87,10,89,10],[87,11,89,11],[90,0,92,0],[90,1,92,1],[90,2,92,2],[90,3,92,3],[90,4,92,4],[90,5,92,7],[90,8,92,9],[90,10,92,10],[90,11,92,11],[93,5,93,7],[93,8,93,9],[94,5,94,7],[94,8,94,9],[95,5,95,7],[95,8,95,9],[96,5,96,7],[96,8,96,9],[97,5,97,7],[97,8,97,9],[98,5,98,7],[98,8,98,9],[99,5,99,7],[99,8,99,9],[100,5,100,7],[100,8,100,9],[101,0,101,9],[103,4,103,11],[104,0,104,11],[105,0,105,5],[105,6,105,8],[105,9,105,11],[106,0,108,0],[106,1,108,1],[106,2,108,2],[106,3,108,3],[106,4,108,4],[106,5,108,7],[106,8,106,11],[107,8,108,9],[107,10,108,10],[109,5,109,7],[109,8,109,9],[110,5,110,7],[110,8,110,9],[111,5,111,7],[111,8,111,9],[112,5,112,7],[112,8,112,9],[113,5,113,7],[113,8,113,9],[114,5,114,7],[114,8,114,9],[115,5,115,7],[115,8,115,9],[116,5,116,7],[116,8,116,9],[117,5,117,7],[117,8,117,9],[118,5,118,7],[118,8,118,9],[119,5,119,7],[119,8,119,9],[120,5,120,7],[120,8,120,9],[121,5,121,7],[121,8,121,9],[122,5,122,7],[122,8,122,9],[123,2,123,3],[123,5,123,7],[123,8,123,9],[124,5,124,7],[124,8,124,9],[125,5,125,7],[125,8,125,9],[126,0,126,9],[127,4,127,11],[128,0,128,11],[129,0,129,5],[129,6,129,8],[129,9,129,11],[130,0,132,0],[130,1,132,1],[130,2,132,2],[130,3,132,3],[130,4,132,4],[130,5,132,7],[130,8,130,11],[131,8,132,9],[131,10,132,10],[133,5,133,7],[133,8,133,9],[134,5,134,7],[134,8,134,9],[135,5,135,7],[135,8,135,9],[136,2,136,3],[136,5,136,7],[136,8,136,9],[137,5,137,7],[137,8,137,9],[138,5,138,7],[138,8,138,9],[139,5,139,7],[139,8,139,9],[140,5,140,7],[140,8,140,9],[141,5,141,7],[141,8,141,9],[142,5,142,7],[142,8,142,9],[143,5,143,7],[143,8,143,9],[144,5,144,7],[144,8,144,9],[145,5,145,7],[145,8,145,9],[146,5,146,7],[146,8,146,9],[147,5,147,7],[147,8,147,9],[148,5,148,7],[148,8,148,9],[149,5,149,7],[149,8,149,9],[150,5,150,7],[150,8,150,9],[151,5,151,7],[151,8,151,9],[152,5,152,7],[152,8,152,9],[153,5,153,7],[153,8,153,9],[154,5,154,7],[154,8,154,9],[155,5,155,7],[155,8,155,9],[156,5,156,7],[156,8,156,9],[157,5,157,7],[157,8,157,9],[158,5,158,7],[158,8,158,9],[159,5,159,7],[159,8,159,9],[160,5,160,7],[160,8,160,9],[161,5,161,7],[161,8,161,9],[162,5,162,7],[162,8,162,9],[163,5,163,7],[163,8,163,9],[164,5,164,7],[164,8,164,9],[165,0,165,9],[166,0,166,9],[168,4,168,11]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第1页 共7页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["1","040101002006","挖沟槽土方","1、机械挖土人工清理\n2、土壤类别：三类土\n3、挖土深度：4M内\n4、土方堆放：投标方自行考虑","m3","11860"]
[]
["2","040103001016","回填土方","1、密实度要求：按设计要求\n2、填方材料品种：土方\n3、填方来源、运距：符合要求的原状土、运距投标方自行考虑","m3","4750"]
[]
["3","040103002001","余方弃置","1、废弃料品种：外运废方\n2、余方外运：20KM","m3","9005"]
["4","040103001017","回填方 6%灰土","1、密实度要求：按设计要求\n2、填方材料品种：6%灰土，原土利用","m3","5350"]
["5","040501001003","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用90°-C20砼基础\n3、规格：d300钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","150"]
[]
[]
["6","040501001001","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d800钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","28"]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第2页 共7页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["7","040501001002","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d1000钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","866"]
[]
[]
["8","040501001004","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d1500钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","171"]
[]
[]
["9","040504009001","雨水口","1、收水井采用偏沟式砖砌单篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","47"]
[]
[]
[]
[]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第3页 共7页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["10","040504009002","雨水口","1、收水井采用偏沟式砖砌双篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","4"]
[]
[]
["11","040504001018","砌筑井","1、盖板式砖砌圆形1250排水检查井\n2、规格：1250\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","7"]
[]
[]
["12","040504001015","砌筑井","1、盖板式砖砌砖砌圆形1500排水检查井\n2、规格：1500\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","21"]
[]
[]
[]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第4页 共7页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["13","040504001019","砌筑井","1、砖砌1100X1300矩形雨水检查井\n2、规格：1100X1300\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","9"]
[]
[]
["14","040504001020","砌筑井","1、砖砌1100X1800矩形雨水检查井\n2、规格：1100X1800\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","5"]
[]
[]
["15","040504001021","砌筑井","1、砖砌2200X2200矩形雨水检查井\n2、规格：2200X2200\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","2"]
[]
[]
[]
[]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第5页 共7页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["16","040504001017","破修现状检查井","1、破坏修复现状排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","4"]
[]
[]
["17","040504002016","混凝土井","1、2000X1500钢筋砼矩形闸门井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、成品预制砼井筒\n5、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["18","040602031003","闸门安装","1、铸铁镶铜闸门SYZ1000\n2、其他具体要求按施工图纸","座","1"]
["19","040602035001","QDA-45型单吊点手电两用启闭机","QDA-45型单吊点手电两用启闭机","台","1"]
["20","040504006002","石砌八字式出水口","1、M10石砌八字式 H×L1(1.58×2.75m以内) 管径1000mm","座","1"]
["21","041001002002","破修现状沥青路面","1、现状沥青路面破除\n2、施工结束后原状恢复","m2","3267"]
["22","041001002003","拆除及修复人行道","1、现状人行道破除\n2、施工结束后原标准恢复","m2","250"]
["23","041001005001","拆除及修复现状路牙石","1、现状路牙石破除\n2、施工结束后原状恢复","m","750"]
["24","041001001010","破坏及修复现状绿化","1、破除现状绿化\n2、施工结束后原状恢复","m2","90"]
["25","041001007003","现状围墙拆除及修复","1、现状围墙拆除\n2、施工结束后原状恢复","m2","24"]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第6页 共7页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["26","041001010001","迁移弱电线杆","迁移弱电线杆","根","1"]
["27","041001006033","破坏修复现状污水管道 DN1500","破坏修复现状污水管道 DN1500","m","8"]
["28","041001006032","破坏修复现状污水管道 DN1000","破坏修复现状污水管道 DN1000","m","6"]
["29","041001006002","破修现状管道 DN800","破坏修复现状污水管道 DN800","m","6"]
["30","041001006031","现状盖板沟合流管清淤疏通、检测修复","现状盖板沟合流管清淤疏通、检测修复（检测采用声呐或CCTV）","m","65"]
["31","041001006034","现状d1500合流管清淤疏通、检测修复","现状d1500合流管清淤疏通、检测修复（检测采用声呐或CCTV）","m","700"]
["32","041001006035","现状d1000合流管清淤疏通、检测修复","现状d1000合流管清淤疏通、检测修复（检测采用声呐或CCTV）","m","18"]
["33","041001006036","现状d800合流管清淤疏通、检测修复","现状d800合流管清淤疏通、检测修复（检测采用声呐或CCTV）","m","18"]
["34","041001006037","现状排水沟清淤疏浚","现状排水沟清淤疏浚","m3","6123"]
["35","010512008001","更换现状雨水检查井井盖、井座","更换现状雨水检查井井盖、井座（轻型球墨铸铁材质、含防坠落板）","块(套)","15"]
["36","040201022001","污水导流","1、污水导流时间为施工期；\n2、流量 1000m3/d。","项","1"]
["37","041001007004","现状石砌挡墙拆除及修复","1、现状石砌挡墙拆除\n2、施工结束后原状恢复","项",1]
["38","010202006003","钢板桩","1、钢板桩类型：拉森钢板桩SP-III\n2、桩长：10m内","t","900"]
["39","041001010002","现状（给水、弱电、燃气等）管线支护保护","现状（给水、弱电、燃气等）管线支护保护","处","5"]
[null,null,"分部分项合计",null,null,""]
["1","041107002005","轻型井点降水",null,"m","1037"]
["2","041107002006","汛期应急排水（投标方自行考虑，需满足汛期应急排水要求）","1、汛期应急排水\n2、费用由投标方自行考虑","项","1"]
["本页小计"]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第7页 共7页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["3","041103001001","围堰（草袋围堰）",null,"m3","1680"]
["4","041107002003","排水",null,"项","1"]
["5","041106001001","大型机械设备进出场及安拆",null,"项","1"]
[null,null,"单价措施合计",null,null,""]
{"$rows_empty":28}
["本页小计"]
["合    计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"4.2 表-11 总价措施项目清单与计价表","index":7,"n_rows":56,"n_cols":12,"rows_kept":56,"merged":[[0,0,0,12],[1,0,1,6],[1,7,1,8],[1,9,1,12],[2,2,2,3],[2,6,2,8],[2,11,2,12],[3,2,3,3],[3,6,3,8],[3,11,3,12],[4,2,4,3],[4,6,4,8],[4,11,4,12],[5,2,5,3],[5,6,5,8],[5,11,5,12],[6,2,6,3],[6,6,6,8],[6,11,6,12],[7,2,7,3],[7,6,7,8],[7,11,7,12],[8,2,8,3],[8,6,8,8],[8,11,8,12],[9,2,9,3],[9,6,9,8],[9,11,9,12],[10,2,10,3],[10,6,10,8],[10,11,10,12],[11,2,11,3],[11,6,11,8],[11,11,11,12],[12,2,12,3],[12,6,12,8],[12,11,12,12],[13,2,13,3],[13,6,13,8],[13,11,13,12],[14,2,14,3],[14,6,14,8],[14,11,14,12],[15,0,15,12],[16,5,16,12],[17,0,17,2],[17,8,17,11],[18,0,18,12],[19,0,19,6],[19,7,19,8],[19,9,19,12],[20,2,20,3],[20,6,20,8],[20,11,20,12],[21,2,21,3],[21,6,21,8],[21,11,21,12],[22,2,22,3],[22,6,22,8],[22,11,22,12],[23,2,23,3],[23,6,23,8],[23,11,23,12],[24,2,24,3],[24,6,24,8],[24,11,24,12],[25,2,25,3],[25,6,25,8],[25,11,25,12],[26,2,26,3],[26,6,26,8],[26,11,26,12],[27,2,27,3],[27,6,27,8],[27,11,27,12],[28,2,28,3],[28,6,28,8],[28,11,28,12],[29,2,29,3],[29,6,29,8],[29,11,29,12],[30,2,30,3],[30,6,30,8],[30,11,30,12],[31,2,31,3],[31,6,31,8],[31,11,31,12],[32,2,32,3],[32,6,32,8],[32,11,32,12],[33,2,33,3],[33,6,33,8],[33,11,33,12],[34,2,34,3],[34,6,34,8],[34,11,34,12],[35,2,35,3],[35,6,35,8],[35,11,35,12],[36,2,36,3],[36,6,36,8],[36,11,36,12],[37,2,37,3],[37,6,37,8],[37,11,37,12],[38,2,38,3],[38,6,38,8],[38,11,38,12],[39,2,39,3],[39,6,39,8],[39,11,39,12],[40,2,40,3],[40,6,40,8],[40,11,40,12],[41,2,41,3],[41,6,41,8],[41,11,41,12],[42,2,42,3],[42,6,42,8],[42,11,42,12],[43,2,43,3],[43,6,43,8],[43,11,43,12],[44,2,44,3],[44,6,44,8],[44,11,44,12],[45,2,45,3],[45,6,45,8],[45,11,45,12],[46,2,46,3],[46,6,46,8],[46,11,46,12],[47,2,47,3],[47,6,47,8],[47,11,47,12],[48,2,48,3],[48,6,48,8],[48,11,48,12],[49,2,49,3],[49,6,49,8],[49,11,49,12],[50,2,50,3],[50,6,50,8],[50,11,50,12],[51,2,51,3],[51,6,51,8],[51,11,51,12],[52,2,52,3],[52,6,52,8],[52,11,52,12],[53,0,53,12],[54,8,54,12],[55,0,55,2],[55,8,55,11]],"flags":["formulas_cached_only"]}
["总价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":6},"标段：",null,"第1页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["1","041109001001","安全文明施工费",null,null,""]
["1.1",null,"基本费",null,"分部分项合计+单价措施项目合计-除税工程设备费","1.500"]
["1.2",null,"增加费",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["2","041109002001","夜间施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["3","041109003001","二次搬运",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["4","041109004001","冬雨季施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["5","041109005001","行车、行人干扰",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["6","041109006001","地上、地下设施、建筑物的临时保护设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["7","041109007001","已完工程及设备保护",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["8","041109008001","临时设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["9","041109009001","赶工措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
[]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]
["总价措施项目清单与计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":6},"标段：",null,"第2页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["10","041109010001","工程按质论价",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["11","041109011001","扬尘防治专项措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
{"$rows_empty":31}
[{"$nulls":8},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]

{"sheet":"4.3 表-12 其他项目清单与计价汇总表","index":8,"n_rows":43,"n_cols":8,"rows_kept":43,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,5],[1,6,1,7],[2,3,2,6],[3,3,3,6],[4,3,4,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,3,11,6],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[23,3,23,6],[24,3,24,6],[25,3,25,6],[26,3,26,6],[27,3,27,6],[28,3,28,6],[29,3,29,6],[30,3,30,6],[31,3,31,6],[32,3,32,6],[33,3,33,6],[34,3,34,6],[35,3,35,6],[36,3,36,6],[37,3,37,6],[38,3,38,6],[39,3,39,6],[40,0,40,1],[40,3,40,6],[42,5,42,7]],"flags":["formulas_cached_only"]}
["其他项目清单与计价汇总表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":3},"标段：",null,"第1页 共1页"]
["序号","项目名称","金额(元)","结算金额(元)",{"$nulls":3},"备注"]
["1","暂列金额",""]
["2","暂估价",""]
["2.1","材料暂估价",""]
["2.2","专业工程暂估价",""]
["3","计日工",""]
["4","总承包服务费",""]
{"$rows_empty":31}
["合  计",null,""]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"4.9 表-13 规费、税金项目计价表","index":9,"n_rows":34,"n_cols":10,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,6],[1,7,1,10],[2,2,2,5],[2,6,2,7],[2,9,2,10],[3,2,3,5],[3,6,3,7],[3,9,3,10],[4,2,4,5],[4,6,4,7],[4,9,4,10],[5,2,5,5],[5,6,5,7],[5,9,5,10],[6,2,6,5],[6,6,6,7],[6,9,6,10],[7,2,7,5],[7,6,7,7],[7,9,7,10],[8,2,8,5],[8,6,8,7],[8,9,8,10],[9,2,9,5],[9,6,9,7],[9,9,9,10],[10,2,10,5],[10,6,10,7],[10,9,10,10],[11,2,11,5],[11,6,11,7],[11,9,11,10],[12,2,12,5],[12,6,12,7],[12,9,12,10],[13,2,13,5],[13,6,13,7],[13,9,13,10],[14,2,14,5],[14,6,14,7],[14,9,14,10],[15,2,15,5],[15,6,15,7],[15,9,15,10],[16,2,16,5],[16,6,16,7],[16,9,16,10],[17,2,17,5],[17,6,17,7],[17,9,17,10],[18,2,18,5],[18,6,18,7],[18,9,18,10],[19,2,19,5],[19,6,19,7],[19,9,19,10],[20,2,20,5],[20,6,20,7],[20,9,20,10],[21,2,21,5],[21,6,21,7],[21,9,21,10],[22,2,22,5],[22,6,22,7],[22,9,22,10],[23,2,23,5],[23,6,23,7],[23,9,23,10],[24,2,24,5],[24,6,24,7],[24,9,24,10],[25,2,25,5],[25,6,25,7],[25,9,25,10],[26,2,26,5],[26,6,26,7],[26,9,26,10],[27,2,27,5],[27,6,27,7],[27,9,27,10],[28,2,28,5],[28,6,28,7],[28,9,28,10],[30,0,30,8],[30,9,30,10],[32,5,32,10],[33,0,33,2],[33,5,33,9]],"flags":["formulas_cached_only"]}
["规费、税金项目计价表"]
["工程名称：三汊河路（瑞兴南路-六保河）路面积水整治工程",{"$nulls":3},"标段：",null,null,"第1页 共1页"]
["序号","项目名称","计算基础",{"$nulls":3},"计算基数(元)",null,"计算费率(％)","金额(元)"]
["1","规费","工程排污费+社会保险费+住房公积金",{"$nulls":5},"100.000"]
["1.1","社会保险费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"2.000"]
["1.2","住房公积金","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"0.340"]
["1.3","工程排污费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},""]
["2","税金","分部分项工程费+措施项目费+其他项目费+规费-除税甲供材料和甲供设备费/1.01",{"$nulls":5},"11.000"]
{"$rows_empty":22}
["合  计"]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":4},"复核人（造价工程师）："]

{"sheet":"5.1 表-08 分部分项工程和单价措施项目清单与计价表","index":10,"n_rows":127,"n_cols":12,"rows_kept":127,"merged":[[0,0,0,11],[1,0,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,7],[2,8,2,11],[3,8,4,9],[3,10,4,10],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,7],[5,8,6,9],[5,10,6,10],[5,11,6,11],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,7],[7,8,8,9],[7,10,8,10],[7,11,8,11],[9,5,9,7],[9,8,9,9],[10,5,10,7],[10,8,10,9],[11,0,13,0],[11,1,13,1],[11,2,13,2],[11,3,13,3],[11,4,13,4],[11,5,13,7],[11,8,13,9],[11,10,13,10],[11,11,13,11],[14,0,16,0],[14,1,16,1],[14,2,16,2],[14,3,16,3],[14,4,16,4],[14,5,16,7],[14,8,16,9],[14,10,16,10],[14,11,16,11],[17,5,17,7],[17,8,17,9],[18,0,18,9],[20,4,20,11],[21,0,21,11],[22,0,22,5],[22,6,22,8],[22,9,22,11],[23,0,25,0],[23,1,25,1],[23,2,25,2],[23,3,25,3],[23,4,25,4],[23,5,25,7],[23,8,23,11],[24,8,25,9],[24,10,25,10],[26,5,26,7],[26,8,26,9],[27,5,27,7],[27,8,27,9],[28,5,28,7],[28,8,28,9],[29,0,31,0],[29,1,31,1],[29,2,31,2],[29,3,31,3],[29,4,31,4],[29,5,31,7],[29,8,31,9],[29,10,31,10],[29,11,31,11],[32,0,34,0],[32,1,34,1],[32,2,34,2],[32,3,34,3],[32,4,34,4],[32,5,34,7],[32,8,34,9],[32,10,34,10],[32,11,34,11],[35,5,35,7],[35,8,35,9],[36,5,36,7],[36,8,36,9],[37,5,37,7],[37,8,37,9],[38,5,38,7],[38,8,38,9],[39,0,39,9],[41,4,41,11],[42,0,42,11],[43,0,43,5],[43,6,43,8],[43,9,43,11],[44,0,46,0],[44,1,46,1],[44,2,46,2],[44,3,46,3],[44,4,46,4],[44,5,46,7],[44,8,44,11],[45,8,46,9],[45,10,46,10],[47,0,48,0],[47,1,48,1],[47,2,48,2],[47,3,48,3],[47,4,48,4],[47,5,48,7],[47,8,48,9],[47,10,48,10],[47,11,48,11],[49,0,51,0],[49,1,51,1],[49,2,51,2],[49,3,51,3],[49,4,51,4],[49,5,51,7],[49,8,51,9],[49,10,51,10],[49,11,51,11],[52,5,52,7],[52,8,52,9],[53,0,54,0],[53,1,54,1],[53,2,54,2],[53,3,54,3],[53,4,54,4],[53,5,54,7],[53,8,54,9],[53,10,54,10],[53,11,54,11],[55,5,55,7],[55,8,55,9],[56,0,58,0],[56,1,58,1],[56,2,58,2],[56,3,58,3],[56,4,58,4],[56,5,58,7],[56,8,58,9],[56,10,58,10],[56,11,58,11],[59,0,59,9],[61,4,61,11],[62,0,62,11],[63,0,63,5],[63,6,63,8],[63,9,63,11],[64,0,66,0],[64,1,66,1],[64,2,66,2],[64,3,66,3],[64,4,66,4],[64,5,66,7],[64,8,64,11],[65,8,66,9],[65,10,66,10],[67,5,67,7],[67,8,67,9],[68,5,68,7],[68,8,68,9],[69,5,69,7],[69,8,69,9],[70,5,70,7],[70,8,70,9],[71,5,71,7],[71,8,71,9],[72,5,72,7],[72,8,72,9],[73,5,73,7],[73,8,73,9],[74,5,74,7],[74,8,74,9],[75,5,75,7],[75,8,75,9],[76,5,76,7],[76,8,76,9],[77,5,77,7],[77,8,77,9],[78,5,78,7],[78,8,78,9],[79,5,79,7],[79,8,79,9],[80,2,80,3],[80,5,80,7],[80,8,80,9],[81,5,81,7],[81,8,81,9],[82,5,82,7],[82,8,82,9],[83,5,83,7],[83,8,83,9],[84,0,84,9],[86,4,86,11],[87,0,87,11],[88,0,88,5],[88,6,88,8],[88,9,88,11],[89,0,91,0],[89,1,91,1],[89,2,91,2],[89,3,91,3],[89,4,91,4],[89,5,91,7],[89,8,89,11],[90,8,91,9],[90,10,91,10],[92,5,92,7],[92,8,92,9],[93,5,93,7],[93,8,93,9],[94,5,94,7],[94,8,94,9],[95,2,95,3],[95,5,95,7],[95,8,95,9],[96,5,96,7],[96,8,96,9],[97,5,97,7],[97,8,97,9],[98,5,98,7],[98,8,98,9],[99,5,99,7],[99,8,99,9],[100,5,100,7],[100,8,100,9],[101,5,101,7],[101,8,101,9],[102,5,102,7],[102,8,102,9],[103,5,103,7],[103,8,103,9],[104,5,104,7],[104,8,104,9],[105,5,105,7],[105,8,105,9],[106,5,106,7],[106,8,106,9],[107,5,107,7],[107,8,107,9],[108,5,108,7],[108,8,108,9],[109,5,109,7],[109,8,109,9],[110,5,110,7],[110,8,110,9],[111,5,111,7],[111,8,111,9],[112,5,112,7],[112,8,112,9],[113,5,113,7],[113,8,113,9],[114,5,114,7],[114,8,114,9],[115,5,115,7],[115,8,115,9],[116,5,116,7],[116,8,116,9],[117,5,117,7],[117,8,117,9],[118,5,118,7],[118,8,118,9],[119,5,119,7],[119,8,119,9],[120,5,120,7],[120,8,120,9],[121,5,121,7],[121,8,121,9],[122,5,122,7],[122,8,122,9],[123,0,123,9],[124,0,124,9],[126,4,126,11]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第1页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["1","040101002006","挖沟槽土方","1、机械挖土人工清理\n2、土壤类别：三类土\n3、挖土深度：4M内\n4、土方堆放：投标方自行考虑","m3","10098"]
[]
["2","040103001016","回填土方","1、密实度要求：按设计要求\n2、填方材料品种：土方\n3、填方来源、运距：符合要求的原状土、运距投标方自行考虑","m3","1093"]
[]
["3","040103002001","余方弃置","1、废弃料品种：外运废方\n2、余方外运：20KM","m3","7110"]
["4","040103001017","回填方 6%灰土","1、密实度要求：按设计要求\n2、填方材料品种：6%灰土，原土利用","m3","5870"]
["5","040501001003","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用90°-C20砼基础\n3、规格：d300钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","54"]
[]
[]
["6","040501001002","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d1000钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","6"]
[]
[]
["7","041001006035","现状d1000合流管清淤疏通、检测修复","现状d1000合流管清淤疏通、检测修复（检测采用声呐或CCTV）","m","262"]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第2页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["8","040306004002","钢筋砼箱涵","1、管涵类型：钢筋砼箱涵\n2、尺寸：BXH=3.0X2.0m\n3、其他按设计图纸要求","m","340"]
["9","040306004001","破修现状箱涵","1、管涵类型：钢筋砼箱涵\n2、尺寸：BXH=1.8X1.5m\n3、破除及修复","m","4"]
["10","040306004003","破修现状箱涵","1、管涵类型：钢筋砼箱涵\n2、尺寸：BXH=2.5X1.8m\n3、破除及修复","m","4"]
["11","040504009001","雨水口","1、收水井采用偏沟式砖砌单篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","20"]
[]
[]
["12","040504009002","雨水口","1、收水井采用偏沟式砖砌双篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","2"]
[]
[]
[]
[]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第3页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["13","040504001016","沟上排水检查井","1、沟上排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","12"]
[]
["14","040504001017","破修现状检查井","1、破坏修复现状排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["15","040602031001","截污闸","1、B=3.0m截污闸\n2、具体做法详见施工图","座","1"]
["16","040602031002","闸门安装","1、铸铁镶铜闸门SFZ3000X2000\n2、启闭机选用单吊点手电两用启闭机，与闸门配套安装\n3、其他具体要求按施工图纸","座","1"]
[]
["17","040602035002","单吊点手电两用启闭机","1、单吊点手电两用启闭机\n2、与闸门SFZ3000X2000配套","台","1"]
["18","040504002016","混凝土井","1、2000X1500钢筋砼矩形闸门井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、成品预制砼井筒\n5、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第4页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["19","040602031003","闸门安装","1、铸铁镶铜闸门SYZ1000\n2、其他具体要求按施工图纸","座","1"]
["20","040602035001","QDA-45型单吊点手电两用启闭机","QDA-45型单吊点手电两用启闭机","台","1"]
["21","041001002002","破修现状路面","破修现状路面","m2","2040"]
["22","041001002003","拆除及修复人行道","1、现状人行道破除\n2、施工结束后原状恢复","m2","168"]
["23","041001001010","破坏及修复现状绿化","1、破除现状绿化\n2、施工结束后原状恢复","m2","20"]
["24","041001005001","拆除及修复现状路牙石（条石）","1、现状路牙石（条石）破除\n2、施工结束后原状恢复","m","360"]
["25","041001007004","现状石砌挡墙拆除及修复","1、现状石砌挡墙拆除\n2、施工结束后原状恢复","项",1]
["26","010202006003","钢板桩","1、钢板桩类型：拉森钢板桩SP-III\n2、桩长：10m内","t","900"]
["27","040201022001","污水导流","1、污水导流时间施工期；\n2、流量 500m3/d。","项","1"]
["28","010512008001","更换现状雨水检查井井盖、井座","更换现状雨水检查井井盖、井座（轻型球墨铸铁材质、含防坠落板）","块(套)","12"]
["29","041001006002","破修现状管道 DN400","破坏修复现状管道 DN400","m","30"]
["30","041001010002","现状给水（燃气）管线支护","现状给水（燃气）管线支护","处","4"]
["31","041001010001","路灯杆线迁移","路灯杆线迁移","处","1"]
[null,null,"分部分项合计",null,null,""]
["1","041107002005","轻型井点降水",null,"m","346"]
["2","041107002006","汛期应急排水（投标方自行考虑，需满足汛期应急排水要求）","1、汛期应急排水\n2、费用由投标方自行考虑","项","1"]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第5页 共5页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["3","041103001001","围堰（草袋围堰）",null,"m3","720"]
["4","041107002003","排水",null,"项",1]
["5","041106001001","大型机械设备进出场及安拆",null,"项","1"]
[null,null,"单价措施合计",null,null,""]
{"$rows_empty":27}
["本页小计"]
["合    计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"5.2 表-11 总价措施项目清单与计价表","index":11,"n_rows":53,"n_cols":12,"rows_kept":53,"merged":[[0,0,0,12],[1,0,1,6],[1,7,1,8],[1,9,1,12],[2,2,2,3],[2,6,2,8],[2,11,2,12],[3,2,3,3],[3,6,3,8],[3,11,3,12],[4,2,4,3],[4,6,4,8],[4,11,4,12],[5,2,5,3],[5,6,5,8],[5,11,5,12],[6,2,6,3],[6,6,6,8],[6,11,6,12],[7,2,7,3],[7,6,7,8],[7,11,7,12],[8,2,8,3],[8,6,8,8],[8,11,8,12],[9,2,9,3],[9,6,9,8],[9,11,9,12],[10,2,10,3],[10,6,10,8],[10,11,10,12],[11,2,11,3],[11,6,11,8],[11,11,11,12],[12,2,12,3],[12,6,12,8],[12,11,12,12],[13,2,13,3],[13,6,13,8],[13,11,13,12],[14,2,14,3],[14,6,14,8],[14,11,14,12],[15,0,15,12],[16,5,16,12],[17,0,17,2],[17,8,17,11],[18,0,18,12],[19,0,19,6],[19,7,19,8],[19,9,19,12],[20,2,20,3],[20,6,20,8],[20,11,20,12],[21,2,21,3],[21,6,21,8],[21,11,21,12],[22,2,22,3],[22,6,22,8],[22,11,22,12],[23,2,23,3],[23,6,23,8],[23,11,23,12],[24,2,24,3],[24,6,24,8],[24,11,24,12],[25,2,25,3],[25,6,25,8],[25,11,25,12],[26,2,26,3],[26,6,26,8],[26,11,26,12],[27,2,27,3],[27,6,27,8],[27,11,27,12],[28,2,28,3],[28,6,28,8],[28,11,28,12],[29,2,29,3],[29,6,29,8],[29,11,29,12],[30,2,30,3],[30,6,30,8],[30,11,30,12],[31,2,31,3],[31,6,31,8],[31,11,31,12],[32,2,32,3],[32,6,32,8],[32,11,32,12],[33,2,33,3],[33,6,33,8],[33,11,33,12],[34,2,34,3],[34,6,34,8],[34,11,34,12],[35,2,35,3],[35,6,35,8],[35,11,35,12],[36,2,36,3],[36,6,36,8],[36,11,36,12],[37,2,37,3],[37,6,37,8],[37,11,37,12],[38,2,38,3],[38,6,38,8],[38,11,38,12],[39,2,39,3],[39,6,39,8],[39,11,39,12],[40,2,40,3],[40,6,40,8],[40,11,40,12],[41,2,41,3],[41,6,41,8],[41,11,41,12],[42,2,42,3],[42,6,42,8],[42,11,42,12],[43,2,43,3],[43,6,43,8],[43,11,43,12],[44,2,44,3],[44,6,44,8],[44,11,44,12],[45,2,45,3],[45,6,45,8],[45,11,45,12],[46,2,46,3],[46,6,46,8],[46,11,46,12],[47,2,47,3],[47,6,47,8],[47,11,47,12],[48,2,48,3],[48,6,48,8],[48,11,48,12],[49,2,49,3],[49,6,49,8],[49,11,49,12],[50,0,50,12],[51,5,51,12],[52,0,52,2],[52,8,52,11]],"flags":["formulas_cached_only"]}
["总价措施项目清单与计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":6},"标段：",null,"第1页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["1","041109001001","安全文明施工费",null,null,""]
["1.1",null,"基本费",null,"分部分项合计+单价措施项目合计-除税工程设备费","1.500"]
["1.2",null,"增加费",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["2","041109002001","夜间施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["3","041109003001","二次搬运",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["4","041109004001","冬雨季施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["5","041109005001","行车、行人干扰",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["6","041109006001","地上、地下设施、建筑物的临时保护设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["7","041109007001","已完工程及设备保护",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["8","041109008001","临时设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["9","041109009001","赶工措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
[]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]
["总价措施项目清单与计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":6},"标段：",null,"第2页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["10","041109010001","工程按质论价",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["11","041109011001","扬尘防治专项措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
{"$rows_empty":28}
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]

{"sheet":"5.3 表-12 其他项目清单与计价汇总表","index":12,"n_rows":42,"n_cols":8,"rows_kept":42,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,5],[1,6,1,7],[2,3,2,6],[3,3,3,6],[4,3,4,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,3,11,6],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[23,3,23,6],[24,3,24,6],[25,3,25,6],[26,3,26,6],[27,3,27,6],[28,3,28,6],[29,3,29,6],[30,3,30,6],[31,3,31,6],[32,3,32,6],[33,3,33,6],[34,3,34,6],[35,3,35,6],[36,3,36,6],[37,3,37,6],[38,3,38,6],[39,0,39,1],[39,3,39,6],[41,5,41,7]],"flags":["formulas_cached_only"]}
["其他项目清单与计价汇总表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":3},"标段：",null,"第1页 共1页"]
["序号","项目名称","金额(元)","结算金额(元)",{"$nulls":3},"备注"]
["1","暂列金额",""]
["2","暂估价",""]
["2.1","材料暂估价",""]
["2.2","专业工程暂估价",""]
["3","计日工",""]
["4","总承包服务费",""]
{"$rows_empty":30}
["合  计",null,""]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"5.9 表-13 规费、税金项目计价表","index":13,"n_rows":36,"n_cols":10,"rows_kept":36,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,6],[1,7,1,10],[2,2,2,5],[2,6,2,7],[2,9,2,10],[3,2,3,5],[3,6,3,7],[3,9,3,10],[4,2,4,5],[4,6,4,7],[4,9,4,10],[5,2,5,5],[5,6,5,7],[5,9,5,10],[6,2,6,5],[6,6,6,7],[6,9,6,10],[7,2,7,5],[7,6,7,7],[7,9,7,10],[8,2,8,5],[8,6,8,7],[8,9,8,10],[9,2,9,5],[9,6,9,7],[9,9,9,10],[10,2,10,5],[10,6,10,7],[10,9,10,10],[11,2,11,5],[11,6,11,7],[11,9,11,10],[12,2,12,5],[12,6,12,7],[12,9,12,10],[13,2,13,5],[13,6,13,7],[13,9,13,10],[14,2,14,5],[14,6,14,7],[14,9,14,10],[15,2,15,5],[15,6,15,7],[15,9,15,10],[16,2,16,5],[16,6,16,7],[16,9,16,10],[17,2,17,5],[17,6,17,7],[17,9,17,10],[18,2,18,5],[18,6,18,7],[18,9,18,10],[19,2,19,5],[19,6,19,7],[19,9,19,10],[20,2,20,5],[20,6,20,7],[20,9,20,10],[21,2,21,5],[21,6,21,7],[21,9,21,10],[22,2,22,5],[22,6,22,7],[22,9,22,10],[23,2,23,5],[23,6,23,7],[23,9,23,10],[24,2,24,5],[24,6,24,7],[24,9,24,10],[25,2,25,5],[25,6,25,7],[25,9,25,10],[26,2,26,5],[26,6,26,7],[26,9,26,10],[27,2,27,5],[27,6,27,7],[27,9,27,10],[28,2,28,5],[28,6,28,7],[28,9,28,10],[29,2,29,5],[29,6,29,7],[29,9,29,10],[30,2,30,5],[30,6,30,7],[30,9,30,10],[32,0,32,8],[32,9,32,10],[34,5,34,10],[35,0,35,2],[35,5,35,9]],"flags":["formulas_cached_only"]}
["规费、税金项目计价表"]
["工程名称：三汊河路（东兴路-李口大沟）路面积水整治工程",{"$nulls":3},"标段：",null,null,"第1页 共1页"]
["序号","项目名称","计算基础",{"$nulls":3},"计算基数(元)",null,"计算费率(％)","金额(元)"]
["1","规费","工程排污费+社会保险费+住房公积金",{"$nulls":5},"100.000"]
["1.1","社会保险费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"2.000"]
["1.2","住房公积金","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"0.340"]
["1.3","工程排污费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},""]
["2","税金","分部分项工程费+措施项目费+其他项目费+规费-除税甲供材料和甲供设备费/1.01",{"$nulls":5},"11.000"]
{"$rows_empty":24}
["合  计"]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":4},"复核人（造价工程师）："]

{"sheet":"6.1 表-08 分部分项工程和单价措施项目清单与计价表","index":14,"n_rows":88,"n_cols":12,"rows_kept":88,"merged":[[0,0,0,11],[1,0,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,7],[2,8,2,11],[3,8,4,9],[3,10,4,10],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,7],[5,8,6,9],[5,10,6,10],[5,11,6,11],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,7],[7,8,8,9],[7,10,8,10],[7,11,8,11],[9,5,9,7],[9,8,9,9],[10,5,10,7],[10,8,10,9],[11,0,13,0],[11,1,13,1],[11,2,13,2],[11,3,13,3],[11,4,13,4],[11,5,13,7],[11,8,13,9],[11,10,13,10],[11,11,13,11],[14,0,16,0],[14,1,16,1],[14,2,16,2],[14,3,16,3],[14,4,16,4],[14,5,16,7],[14,8,16,9],[14,10,16,10],[14,11,16,11],[17,5,17,7],[17,8,17,9],[18,0,18,9],[19,4,19,11],[20,0,20,11],[21,0,21,5],[21,6,21,8],[21,9,21,11],[22,0,24,0],[22,1,24,1],[22,2,24,2],[22,3,24,3],[22,4,24,4],[22,5,24,7],[22,8,22,11],[23,8,24,9],[23,10,24,10],[25,0,27,0],[25,1,27,1],[25,2,27,2],[25,3,27,3],[25,4,27,4],[25,5,27,7],[25,8,27,9],[25,10,27,10],[25,11,27,11],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[28,5,30,7],[28,8,30,9],[28,10,30,10],[28,11,30,11],[31,0,32,0],[31,1,32,1],[31,2,32,2],[31,3,32,3],[31,4,32,4],[31,5,32,7],[31,8,32,9],[31,10,32,10],[31,11,32,11],[33,5,33,7],[33,8,33,9],[34,5,34,7],[34,8,34,9],[35,5,35,7],[35,8,35,9],[36,5,36,7],[36,8,36,9],[37,5,37,7],[37,8,37,9],[38,5,38,7],[38,8,38,9],[39,0,39,9],[41,4,41,11],[42,0,42,11],[43,0,43,5],[43,6,43,8],[43,9,43,11],[44,0,46,0],[44,1,46,1],[44,2,46,2],[44,3,46,3],[44,4,46,4],[44,5,46,7],[44,8,44,11],[45,8,46,9],[45,10,46,10],[47,0,49,0],[47,1,49,1],[47,2,49,2],[47,3,49,3],[47,4,49,4],[47,5,49,7],[47,8,49,9],[47,10,49,10],[47,11,49,11],[50,0,52,0],[50,1,52,1],[50,2,52,2],[50,3,52,3],[50,4,52,4],[50,5,52,7],[50,8,52,9],[50,10,52,10],[50,11,52,11],[53,0,55,0],[53,1,55,1],[53,2,55,2],[53,3,55,3],[53,4,55,4],[53,5,55,7],[53,8,55,9],[53,10,55,10],[53,11,55,11],[56,5,56,7],[56,8,56,9],[57,5,57,7],[57,8,57,9],[58,5,58,7],[58,8,58,9],[59,0,59,9],[61,4,61,11],[62,0,62,11],[63,0,63,5],[63,6,63,8],[63,9,63,11],[64,0,66,0],[64,1,66,1],[64,2,66,2],[64,3,66,3],[64,4,66,4],[64,5,66,7],[64,8,64,11],[65,8,66,9],[65,10,66,10],[67,5,67,7],[67,8,67,9],[68,5,68,7],[68,8,68,9],[69,5,69,7],[69,8,69,9],[70,5,70,7],[70,8,70,9],[71,5,71,7],[71,8,71,9],[72,5,72,7],[72,8,72,9],[73,5,73,7],[73,8,73,9],[74,5,74,7],[74,8,74,9],[75,5,75,7],[75,8,75,9],[76,5,76,7],[76,8,76,9],[77,5,77,7],[77,8,77,9],[78,5,78,7],[78,8,78,9],[79,5,79,7],[79,8,79,9],[80,2,80,3],[80,5,80,7],[80,8,80,9],[81,5,81,7],[81,8,81,9],[82,5,82,7],[82,8,82,9],[83,5,83,7],[83,8,83,9],[84,2,84,3],[84,5,84,7],[84,8,84,9],[85,0,85,9],[86,0,86,9],[87,4,87,11]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第1页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["1","040101002006","挖沟槽土方","1、机械挖土人工清理\n2、土壤类别：三类土\n3、挖土深度：4M内\n4、土方堆放：投标方自行考虑","m3","2580"]
[]
["2","040103001016","回填土方","1、密实度要求：按设计要求\n2、填方材料品种：土方\n3、填方来源、运距：符合要求的原状土、运距投标方自行考虑","m3","930"]
[]
["3","040103002001","余方弃置","1、废弃料品种：外运废方\n2、余方外运：20KM","m3","1650"]
["4","040103001017","回填方 6%灰土","1、密实度要求：按设计要求\n2、填方材料品种：6%灰土，原土利用","m3","1410"]
["5","040501001003","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用90°-C20砼基础\n3、规格：d300钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","89"]
[]
[]
["6","040501001002","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d1000钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","279"]
[]
[]
[]
["本页小计"]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第2页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["7","040504001015","砌筑井","1、盖板式砖砌圆形1500排水检查井\n2、规格：1500\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","9"]
[]
[]
["8","040504001019","砌筑井","1、砖砌1100X1300矩形雨水检查井\n2、规格：1100X1300\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["9","040504001016","沟上排水检查井","1、沟上排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
{"$rows_empty":7}
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第3页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["10","040504009001","雨水口","1、收水井采用偏沟式砖砌单篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","19"]
[]
[]
["11","040504009002","雨水口","1、收水井采用偏沟式砖砌双篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","2"]
[]
[]
["12","040504001017","破修现状检查井","1、破坏修复现状排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","1"]
[]
[]
["13","041001002004","破修现状沥青路面","1、现状沥青路面破除\n2、施工结束后原状恢复","m2","370"]
["14","041001002003","拆除及修复人行道","1、现状人行道破除\n2、施工结束后原状恢复","m2","80"]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":5},"标段：",null,null,"第4页 共4页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["15","041001002005","拆除及修复停车场","1、现状停车场破除\n2、施工结束后原状恢复","m2","765"]
["16","041001001010","破坏及修复现状绿化","1、破除现状绿化\n2、施工结束后原状恢复","m2","32"]
["17","041001005002","拆除及修复现状路牙石","1、现状路牙石破除\n2、施工结束后原状恢复","m","30"]
["18","010202006003","钢板桩","1、钢板桩类型：拉森钢板桩SP-III\n2、桩长：10m内","t","216"]
["19","041001006002","破修现状污水管道 DN600","破坏修复现状污水管道 DN600","m","6"]
["20","041001006003","废除现状污水管道 DN600","废除现状污水管道 DN600","m","9"]
["21","041001006004","破修现状1200×1700暗涵","破修现状1200X1700暗涵","m","6"]
["22","041001006034","现状1250×900暗涵清淤疏通、检测修复","现状1250X900暗涵清淤疏通、检测修复（检测采用声呐或CCTV）","m","140"]
["23","041001006036","现状d600合流管清淤疏通、检测修复","现状d600合流管清淤疏通、检测修复（检测采用声呐或CCTV）","m","410"]
["24","040201022001","污水导流","1、污水导流时间为施工期；\n2、流量 500m3/d。","项","1"]
["25","010512008001","更换现状雨水检查井井盖、井座","更换现状雨水检查井井盖、井座（重型球墨铸铁材质、含防坠落板）","块(套)","18"]
["26","041001010003","现状（给水、弱电、燃气等）管线支护保护","现状（给水、弱电、燃气等）管线支护保护","处","5"]
["27","041001010001","路灯杆线迁移","路灯杆线迁移","处","1"]
[null,null,"分部分项合计",null,null,""]
["1","041107002005","轻型井点降水",null,"m","279"]
["2","041107002006","汛期应急排水（投标方自行考虑，需满足汛期应急排水要求）","1、汛期应急排水\n2、费用由投标方自行考虑","项","1"]
["3","041106001001","大型机械设备进出场及安拆",null,"项","1"]
[null,null,"单价措施合计",null,null,""]
["本页小计"]
["合    计"]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"6.2 表-11 总价措施项目清单与计价表","index":15,"n_rows":54,"n_cols":12,"rows_kept":54,"merged":[[0,0,0,12],[1,0,1,6],[1,7,1,8],[1,9,1,12],[2,2,2,3],[2,6,2,8],[2,11,2,12],[3,2,3,3],[3,6,3,8],[3,11,3,12],[4,2,4,3],[4,6,4,8],[4,11,4,12],[5,2,5,3],[5,6,5,8],[5,11,5,12],[6,2,6,3],[6,6,6,8],[6,11,6,12],[7,2,7,3],[7,6,7,8],[7,11,7,12],[8,2,8,3],[8,6,8,8],[8,11,8,12],[9,2,9,3],[9,6,9,8],[9,11,9,12],[10,2,10,3],[10,6,10,8],[10,11,10,12],[11,2,11,3],[11,6,11,8],[11,11,11,12],[12,2,12,3],[12,6,12,8],[12,11,12,12],[13,2,13,3],[13,6,13,8],[13,11,13,12],[14,2,14,3],[14,6,14,8],[14,11,14,12],[15,0,15,12],[16,5,16,12],[17,0,17,2],[17,8,17,11],[18,0,18,12],[19,0,19,6],[19,7,19,8],[19,9,19,12],[20,2,20,3],[20,6,20,8],[20,11,20,12],[21,2,21,3],[21,6,21,8],[21,11,21,12],[22,2,22,3],[22,6,22,8],[22,11,22,12],[23,2,23,3],[23,6,23,8],[23,11,23,12],[24,2,24,3],[24,6,24,8],[24,11,24,12],[25,2,25,3],[25,6,25,8],[25,11,25,12],[26,2,26,3],[26,6,26,8],[26,11,26,12],[27,2,27,3],[27,6,27,8],[27,11,27,12],[28,2,28,3],[28,6,28,8],[28,11,28,12],[29,2,29,3],[29,6,29,8],[29,11,29,12],[30,2,30,3],[30,6,30,8],[30,11,30,12],[31,2,31,3],[31,6,31,8],[31,11,31,12],[32,2,32,3],[32,6,32,8],[32,11,32,12],[33,2,33,3],[33,6,33,8],[33,11,33,12],[34,2,34,3],[34,6,34,8],[34,11,34,12],[35,2,35,3],[35,6,35,8],[35,11,35,12],[36,2,36,3],[36,6,36,8],[36,11,36,12],[37,2,37,3],[37,6,37,8],[37,11,37,12],[38,2,38,3],[38,6,38,8],[38,11,38,12],[39,2,39,3],[39,6,39,8],[39,11,39,12],[40,2,40,3],[40,6,40,8],[40,11,40,12],[41,2,41,3],[41,6,41,8],[41,11,41,12],[42,2,42,3],[42,6,42,8],[42,11,42,12],[43,2,43,3],[43,6,43,8],[43,11,43,12],[44,2,44,3],[44,6,44,8],[44,11,44,12],[45,2,45,3],[45,6,45,8],[45,11,45,12],[46,2,46,3],[46,6,46,8],[46,11,46,12],[47,2,47,3],[47,6,47,8],[47,11,47,12],[48,2,48,3],[48,6,48,8],[48,11,48,12],[49,2,49,3],[49,6,49,8],[49,11,49,12],[50,2,50,3],[50,6,50,8],[50,11,50,12],[51,0,51,12],[52,5,52,12],[53,0,53,2],[53,8,53,11]],"flags":["formulas_cached_only"]}
["总价措施项目清单与计价表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":6},"标段：",null,"第1页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["1","041109001001","安全文明施工费",null,null,""]
["1.1",null,"基本费",null,"分部分项合计+单价措施项目合计-除税工程设备费","1.500"]
["1.2",null,"增加费",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["2","041109002001","夜间施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["3","041109003001","二次搬运",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["4","041109004001","冬雨季施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["5","041109005001","行车、行人干扰",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["6","041109006001","地上、地下设施、建筑物的临时保护设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["7","041109007001","已完工程及设备保护",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["8","041109008001","临时设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["9","041109009001","赶工措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
[]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]
["总价措施项目清单与计价表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":6},"标段：",null,"第2页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["10","041109010001","工程按质论价",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["11","041109011001","扬尘防治专项措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
{"$rows_empty":29}
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]

{"sheet":"6.3 表-12 其他项目清单与计价汇总表","index":16,"n_rows":44,"n_cols":8,"rows_kept":44,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,5],[1,6,1,7],[2,3,2,6],[3,3,3,6],[4,3,4,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,3,11,6],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[23,3,23,6],[24,3,24,6],[25,3,25,6],[26,3,26,6],[27,3,27,6],[28,3,28,6],[29,3,29,6],[30,3,30,6],[31,3,31,6],[32,3,32,6],[33,3,33,6],[34,3,34,6],[35,3,35,6],[36,3,36,6],[37,3,37,6],[38,3,38,6],[39,3,39,6],[40,3,40,6],[41,0,41,1],[41,3,41,6],[43,5,43,7]],"flags":["formulas_cached_only"]}
["其他项目清单与计价汇总表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":3},"标段：",null,"第1页 共1页"]
["序号","项目名称","金额(元)","结算金额(元)",{"$nulls":3},"备注"]
["1","暂列金额",""]
["2","暂估价",""]
["2.1","材料暂估价",""]
["2.2","专业工程暂估价",""]
["3","计日工",""]
["4","总承包服务费",""]
{"$rows_empty":32}
["合  计",null,""]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"6.9 表-13 规费、税金项目计价表","index":17,"n_rows":34,"n_cols":10,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,6],[1,7,1,10],[2,2,2,5],[2,6,2,7],[2,9,2,10],[3,2,3,5],[3,6,3,7],[3,9,3,10],[4,2,4,5],[4,6,4,7],[4,9,4,10],[5,2,5,5],[5,6,5,7],[5,9,5,10],[6,2,6,5],[6,6,6,7],[6,9,6,10],[7,2,7,5],[7,6,7,7],[7,9,7,10],[8,2,8,5],[8,6,8,7],[8,9,8,10],[9,2,9,5],[9,6,9,7],[9,9,9,10],[10,2,10,5],[10,6,10,7],[10,9,10,10],[11,2,11,5],[11,6,11,7],[11,9,11,10],[12,2,12,5],[12,6,12,7],[12,9,12,10],[13,2,13,5],[13,6,13,7],[13,9,13,10],[14,2,14,5],[14,6,14,7],[14,9,14,10],[15,2,15,5],[15,6,15,7],[15,9,15,10],[16,2,16,5],[16,6,16,7],[16,9,16,10],[17,2,17,5],[17,6,17,7],[17,9,17,10],[18,2,18,5],[18,6,18,7],[18,9,18,10],[19,2,19,5],[19,6,19,7],[19,9,19,10],[20,2,20,5],[20,6,20,7],[20,9,20,10],[21,2,21,5],[21,6,21,7],[21,9,21,10],[22,2,22,5],[22,6,22,7],[22,9,22,10],[23,2,23,5],[23,6,23,7],[23,9,23,10],[24,2,24,5],[24,6,24,7],[24,9,24,10],[25,2,25,5],[25,6,25,7],[25,9,25,10],[26,2,26,5],[26,6,26,7],[26,9,26,10],[27,2,27,5],[27,6,27,7],[27,9,27,10],[28,2,28,5],[28,6,28,7],[28,9,28,10],[30,0,30,8],[30,9,30,10],[32,5,32,10],[33,0,33,2],[33,5,33,9]],"flags":["formulas_cached_only"]}
["规费、税金项目计价表"]
["工程名称：乐园街-人民路路面积水整治工程",{"$nulls":3},"标段：",null,null,"第1页 共1页"]
["序号","项目名称","计算基础",{"$nulls":3},"计算基数(元)",null,"计算费率(％)","金额(元)"]
["1","规费","工程排污费+社会保险费+住房公积金",{"$nulls":5},"100.000"]
["1.1","社会保险费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"2.000"]
["1.2","住房公积金","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"0.340"]
["1.3","工程排污费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},""]
["2","税金","分部分项工程费+措施项目费+其他项目费+规费-除税甲供材料和甲供设备费/1.01",{"$nulls":5},"11.000"]
{"$rows_empty":22}
["合  计"]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":4},"复核人（造价工程师）："]

{"sheet":"7.1 表-08 分部分项工程和单价措施项目清单与计价表","index":18,"n_rows":135,"n_cols":12,"rows_kept":135,"merged":[[0,0,0,11],[1,0,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,7],[2,8,2,11],[3,8,4,9],[3,10,4,10],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,7],[5,8,6,9],[5,10,6,10],[5,11,6,11],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,7],[7,8,8,9],[7,10,8,10],[7,11,8,11],[9,5,9,7],[9,8,9,9],[10,5,10,7],[10,8,10,9],[11,0,13,0],[11,1,13,1],[11,2,13,2],[11,3,13,3],[11,4,13,4],[11,5,13,7],[11,8,13,9],[11,10,13,10],[11,11,13,11],[14,0,16,0],[14,1,16,1],[14,2,16,2],[14,3,16,3],[14,4,16,4],[14,5,16,7],[14,8,16,9],[14,10,16,10],[14,11,16,11],[17,5,17,7],[17,8,17,9],[18,0,18,9],[20,4,20,11],[21,0,21,11],[22,0,22,5],[22,6,22,8],[22,9,22,11],[23,0,25,0],[23,1,25,1],[23,2,25,2],[23,3,25,3],[23,4,25,4],[23,5,25,7],[23,8,23,11],[24,8,25,9],[24,10,25,10],[26,0,28,0],[26,1,28,1],[26,2,28,2],[26,3,28,3],[26,4,28,4],[26,5,28,7],[26,8,28,9],[26,10,28,10],[26,11,28,11],[29,0,31,0],[29,1,31,1],[29,2,31,2],[29,3,31,3],[29,4,31,4],[29,5,31,7],[29,8,31,9],[29,10,31,10],[29,11,31,11],[32,0,34,0],[32,1,34,1],[32,2,34,2],[32,3,34,3],[32,4,34,4],[32,5,34,7],[32,8,34,9],[32,10,34,10],[32,11,34,11],[35,5,35,7],[35,8,35,9],[36,5,36,7],[36,8,36,9],[37,5,37,7],[37,8,37,9],[38,0,38,9],[40,4,40,11],[41,0,41,11],[42,0,42,5],[42,6,42,8],[42,9,42,11],[43,0,45,0],[43,1,45,1],[43,2,45,2],[43,3,45,3],[43,4,45,4],[43,5,45,7],[43,8,43,11],[44,8,45,9],[44,10,45,10],[46,0,48,0],[46,1,48,1],[46,2,48,2],[46,3,48,3],[46,4,48,4],[46,5,48,7],[46,8,48,9],[46,10,48,10],[46,11,48,11],[49,0,51,0],[49,1,51,1],[49,2,51,2],[49,3,51,3],[49,4,51,4],[49,5,51,7],[49,8,51,9],[49,10,51,10],[49,11,51,11],[52,0,53,0],[52,1,53,1],[52,2,53,2],[52,3,53,3],[52,4,53,4],[52,5,53,7],[52,8,53,9],[52,10,53,10],[52,11,53,11],[54,5,54,7],[54,8,54,9],[55,5,55,7],[55,8,55,9],[56,5,56,7],[56,8,56,9],[57,5,57,7],[57,8,57,9],[58,5,58,7],[58,8,58,9],[59,5,59,7],[59,8,59,9],[60,0,60,9],[62,4,62,11],[63,0,63,11],[64,0,64,5],[64,6,64,8],[64,9,64,11],[65,0,67,0],[65,1,67,1],[65,2,67,2],[65,3,67,3],[65,4,67,4],[65,5,67,7],[65,8,65,11],[66,8,67,9],[66,10,67,10],[68,0,70,0],[68,1,70,1],[68,2,70,2],[68,3,70,3],[68,4,70,4],[68,5,70,7],[68,8,70,9],[68,10,70,10],[68,11,70,11],[71,0,73,0],[71,1,73,1],[71,2,73,2],[71,3,73,3],[71,4,73,4],[71,5,73,7],[71,8,73,9],[71,10,73,10],[71,11,73,11],[74,0,76,0],[74,1,76,1],[74,2,76,2],[74,3,76,3],[74,4,76,4],[74,5,76,7],[74,8,76,9],[74,10,76,10],[74,11,76,11],[77,5,77,7],[77,8,77,9],[78,5,78,7],[78,8,78,9],[79,5,79,7],[79,8,79,9],[80,5,80,7],[80,8,80,9],[81,5,81,7],[81,8,81,9],[82,5,82,7],[82,8,82,9],[83,0,83,9],[85,4,85,11],[86,0,86,11],[87,0,87,5],[87,6,87,8],[87,9,87,11],[88,0,90,0],[88,1,90,1],[88,2,90,2],[88,3,90,3],[88,4,90,4],[88,5,90,7],[88,8,88,11],[89,8,90,9],[89,10,90,10],[91,0,93,0],[91,1,93,1],[91,2,93,2],[91,3,93,3],[91,4,93,4],[91,5,93,7],[91,8,93,9],[91,10,93,10],[91,11,93,11],[94,0,96,0],[94,1,96,1],[94,2,96,2],[94,3,96,3],[94,4,96,4],[94,5,96,7],[94,8,96,9],[94,10,96,10],[94,11,96,11],[97,0,99,0],[97,1,99,1],[97,2,99,2],[97,3,99,3],[97,4,99,4],[97,5,99,7],[97,8,99,9],[97,10,99,10],[97,11,99,11],[100,5,100,7],[100,8,100,9],[101,5,101,7],[101,8,101,9],[102,5,102,7],[102,8,102,9],[103,5,103,7],[103,8,103,9],[104,5,104,7],[104,8,104,9],[105,0,105,9],[106,4,106,11],[107,0,107,11],[108,0,108,5],[108,6,108,8],[108,9,108,11],[109,0,111,0],[109,1,111,1],[109,2,111,2],[109,3,111,3],[109,4,111,4],[109,5,111,7],[109,8,109,11],[110,8,111,9],[110,10,111,10],[112,5,112,7],[112,8,112,9],[113,5,113,7],[113,8,113,9],[114,5,114,7],[114,8,114,9],[115,5,115,7],[115,8,115,9],[116,5,116,7],[116,8,116,9],[117,5,117,7],[117,8,117,9],[118,5,118,7],[118,8,118,9],[119,5,119,7],[119,8,119,9],[120,5,120,7],[120,8,120,9],[121,5,121,7],[121,8,121,9],[122,5,122,7],[122,8,122,9],[123,5,123,7],[123,8,123,9],[124,5,124,7],[124,8,124,9],[125,5,125,7],[125,8,125,9],[126,2,126,3],[126,5,126,7],[126,8,126,9],[127,5,127,7],[127,8,127,9],[128,5,128,7],[128,8,128,9],[129,5,129,7],[129,8,129,9],[130,2,130,3],[130,5,130,7],[130,8,130,9],[131,0,131,9],[132,0,132,9],[134,4,134,11]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第1页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["1","040101002006","挖沟槽土方","1、机械挖土人工清理\n2、土壤类别：三类土\n3、挖土深度：4M内\n4、土方堆放：投标方自行考虑","m3","24656"]
[]
["2","040103001016","回填土方","1、密实度要求：按设计要求\n2、填方材料品种：土方\n3、填方来源、运距：符合要求的原状土、运距投标方自行考虑","m3","3293"]
[]
["3","040103002001","余方弃置","1、废弃料品种：外运废方\n2、余方外运：20KM","m3","21363"]
["4","040103001017","回填方 6%灰土","1、密实度要求：按设计要求\n2、填方材料品种：6%灰土，原土利用","m3","13426"]
["5","040501001003","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用90°-C20砼基础\n3、规格：d300钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求","m","500"]
[]
[]
["6","041001006038","混凝土管（污水）","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用135°-C20砼基础\n3、规格：d400钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","350"]
[]
[]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第2页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["7","041001006003","混凝土管（污水）","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用135°-C20砼基础\n3、规格：d500钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","1500"]
[]
[]
["8","040501001005","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d1000钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求","m","145"]
[]
[]
["9","040501001004","混凝土管","1、垫层、基础材质及厚度：碎石垫层\n2、管座材质：管道基础采用180°-C20砼基础\n3、规格：d1500钢筋砼Ⅱ级承插管\n4、接口方式：承插式橡胶接口\n5、铺设深度：按设计要求\n6、管道检验及试验要求：按规范要求\n7、闭水试验","m","145"]
[]
[]
["10","040306004001","2.0X2.0m箱涵","1、管涵类型：钢筋砼箱涵\n2、尺寸：BXH=2.0X2.0m\n3、其他按设计图纸要求","m","660"]
["11","040306004002","2.5X2.0m箱涵","1、管涵类型：钢筋砼箱涵\n2、尺寸：BXH=2.5X2.0m\n3、其他按设计图纸要求","m","350"]
[]
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第3页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["12","040504009001","雨水口","1、收水井采用偏沟式砖砌单篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","102"]
[]
[]
["13","040504009002","雨水口","1、收水井采用偏沟式砖砌双篦收水井\n2、收水井井盖及井座采用球墨铸铁QT500-7，球化率需达到3级以上，抗拉强度不小于450MPa，屈服强度不小于300MPa，材料尚应符合《球墨铸铁件》（GB1348-2009）规定。收水井井盖的承载等级采用D400。\n3、其他按设计及规范要求。","座","8"]
[]
[]
["14","040504001016","沟上排水检查井","1、沟上排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","35"]
{"$rows_empty":7}
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第4页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["15","040504001018","砌筑井","1、盖板式砖砌圆形1000污水检查井\n2、规格：1000\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","53"]
[]
[]
["16","040504001015","砌筑井","1、盖板式砖砌砖砌圆形1500排水检查井\n2、规格：1500\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","4"]
[]
[]
["17","040504001019","砌筑井","1、砖砌1650X1650矩形雨水检查井\n2、规格：1650X1650\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","3"]
{"$rows_empty":8}
["本页小计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第5页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["18","040504001020","砌筑井","1、砖砌1100X1800矩形雨水检查井\n2、规格：1100X1800\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","5"]
[]
[]
["19","040504001021","砌筑井","1、砖砌2200X2200矩形雨水检查井\n2、规格：2200X2200\n3、构造：详见设计图纸\n4、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n5、成品预制砼井筒\n6、井筒内均应设置防坠落板（质量符合设计要求）","座","2"]
[]
[]
["20","040504001017","破修现状检查井","1、破坏修复现状排水检查井\n2、具体做法详见施工图\n3、直径700mm球墨铸铁井盖、井座（防响、防跳、防坠落、防位移），井盖上须有“排”字样\n4、井筒内均应设置防坠落板（质量符合设计要求）","座","6"]
[]
[]
["21","041001002004","破修现状路面","破修现状路面","m2","7578"]
["22","041001002005","拆除及修复人行道","1、现状人行道破除\n2、施工结束后原状恢复","m2","368"]
["23","041001005002","拆除及修复现状路牙石（条石）","1、现状路牙石（条石）破除\n2、施工结束后原状恢复","m","1300"]
["24","040201022002","污水导流","1、污水导流时间为施工期；\n2、流量 500m3/d。","项","15"]
["25","010202006003","钢板桩","1、钢板桩类型：拉森钢板桩SP-III\n2、桩长：10m内","t","3240"]
["本页小计"]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":5},"标段：",null,null,"第6页 共6页"]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量",null,null,"金额（元）"]
[{"$nulls":8},"综合单价",null,"合价","其中"]
[{"$nulls":11},"暂估价"]
["26","041001006039","破修现状管道 DN600","破坏修复现状管道 DN600","m","12"]
["27","041001006002","破修现状管道 DN800","破坏修复现状管道 DN800","m","20"]
["28","041001006032","破坏修复现状管道 DN1000","破坏修复现状管道 DN1000","m","88"]
["29","041001006033","破坏修复现状盖板沟","破坏修复现状盖板沟","m","68"]
["30","041001006035","现状d1000合流管清淤疏通、检测修复","现状d1000合流管清淤疏通、检测修复（检测采用声呐或CCTV）","m","1352"]
["31","041001006034","现状BXH=1.0×1.6m暗涵清淤疏通、检测修复","现状BXH=1.0X1.6m暗涵清淤疏通、检测修复（检测采用声呐或CCTV）","m","376"]
["32","041001006004","破修现状1200×1600暗涵","破修现状1200X1600暗涵","m","8"]
["33","041001006041","破修现状1250×900暗涵","破修现状1250X900暗涵","m","8"]
["34","010512008001","更换现状雨水检查井井盖、井座","更换现状雨水检查井井盖、井座（轻型球墨铸铁材质、含防坠落板）","块(套)","67"]
["35","040303002002","管道包封混凝土基础","1、d400管道包封\n2、混凝土强度等级：C25商品混凝土","m3","4.91"]
["36","040901001001","管道包封现浇构件钢筋","1、钢筋种类：10以内\n2、其他按设计要求","t","0.102"]
["37","040305001001","管道包封 碎石垫层","1、材料品种、规格：碎石","m3","0.88"]
["38","041001006040","废除现状污水管道 DN600","废除现状污水管道 DN600","m","1006"]
["39","041001010002","现状给水（燃气）管线支护","现状给水（燃气）管线支护","处","14"]
[null,null,"分部分项合计",null,null,""]
["1","041107002005","轻型井点降水",null,"m","1440"]
["2","041107002006","汛期应急排水（投标方自行考虑，需满足汛期应急排水要求）","1、汛期应急排水\n2、费用由投标方自行考虑","项","1"]
["3","041106001001","大型机械设备进出场及安拆",null,"项","1"]
[null,null,"单价措施合计",null,null,""]
["本页小计"]
["合    计"]
[]
[{"$nulls":4},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"7.2 表-11 总价措施项目清单与计价表","index":19,"n_rows":51,"n_cols":12,"rows_kept":51,"merged":[[0,0,0,12],[1,0,1,6],[1,7,1,8],[1,9,1,12],[2,2,2,3],[2,6,2,8],[2,11,2,12],[3,2,3,3],[3,6,3,8],[3,11,3,12],[4,2,4,3],[4,6,4,8],[4,11,4,12],[5,2,5,3],[5,6,5,8],[5,11,5,12],[6,2,6,3],[6,6,6,8],[6,11,6,12],[7,2,7,3],[7,6,7,8],[7,11,7,12],[8,2,8,3],[8,6,8,8],[8,11,8,12],[9,2,9,3],[9,6,9,8],[9,11,9,12],[10,2,10,3],[10,6,10,8],[10,11,10,12],[11,2,11,3],[11,6,11,8],[11,11,11,12],[12,2,12,3],[12,6,12,8],[12,11,12,12],[13,2,13,3],[13,6,13,8],[13,11,13,12],[14,2,14,3],[14,6,14,8],[14,11,14,12],[15,0,15,12],[16,5,16,12],[17,0,17,2],[17,8,17,11],[18,0,18,12],[19,0,19,6],[19,7,19,8],[19,9,19,12],[20,2,20,3],[20,6,20,8],[20,11,20,12],[21,2,21,3],[21,6,21,8],[21,11,21,12],[22,2,22,3],[22,6,22,8],[22,11,22,12],[23,2,23,3],[23,6,23,8],[23,11,23,12],[24,2,24,3],[24,6,24,8],[24,11,24,12],[25,2,25,3],[25,6,25,8],[25,11,25,12],[26,2,26,3],[26,6,26,8],[26,11,26,12],[27,2,27,3],[27,6,27,8],[27,11,27,12],[28,2,28,3],[28,6,28,8],[28,11,28,12],[29,2,29,3],[29,6,29,8],[29,11,29,12],[30,2,30,3],[30,6,30,8],[30,11,30,12],[31,2,31,3],[31,6,31,8],[31,11,31,12],[32,2,32,3],[32,6,32,8],[32,11,32,12],[33,2,33,3],[33,6,33,8],[33,11,33,12],[34,2,34,3],[34,6,34,8],[34,11,34,12],[35,2,35,3],[35,6,35,8],[35,11,35,12],[36,2,36,3],[36,6,36,8],[36,11,36,12],[37,2,37,3],[37,6,37,8],[37,11,37,12],[38,2,38,3],[38,6,38,8],[38,11,38,12],[39,2,39,3],[39,6,39,8],[39,11,39,12],[40,2,40,3],[40,6,40,8],[40,11,40,12],[41,2,41,3],[41,6,41,8],[41,11,41,12],[42,2,42,3],[42,6,42,8],[42,11,42,12],[43,2,43,3],[43,6,43,8],[43,11,43,12],[44,2,44,3],[44,6,44,8],[44,11,44,12],[45,2,45,3],[45,6,45,8],[45,11,45,12],[46,2,46,3],[46,6,46,8],[46,11,46,12],[47,2,47,3],[47,6,47,8],[47,11,47,12],[48,0,48,12],[49,5,49,12],[50,0,50,2],[50,8,50,11]],"flags":["formulas_cached_only"]}
["总价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":6},"标段：",null,"第1页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["1","041109001001","安全文明施工费",null,null,""]
["1.1",null,"基本费",null,"分部分项合计+单价措施项目合计-除税工程设备费","1.500"]
["1.2",null,"增加费",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["2","041109002001","夜间施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["3","041109003001","二次搬运",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["4","041109004001","冬雨季施工",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["5","041109005001","行车、行人干扰",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["6","041109006001","地上、地下设施、建筑物的临时保护设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["7","041109007001","已完工程及设备保护",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["8","041109008001","临时设施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["9","041109009001","赶工措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
[]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]
["总价措施项目清单与计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":6},"标段：",null,"第2页 共2页"]
["序号","项目编码","项目名称",null,"计算基础","费率（%）","金额（元）",null,null,"调整\n费率（%）","调整后\n金额（元）","备注"]
["10","041109010001","工程按质论价",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
["11","041109011001","扬尘防治专项措施",null,"分部分项合计+单价措施项目合计-除税工程设备费",""]
{"$rows_empty":26}
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":7},"复核人（造价工程师）："]

{"sheet":"7.3 表-12 其他项目清单与计价汇总表","index":20,"n_rows":44,"n_cols":8,"rows_kept":44,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,5],[1,6,1,7],[2,3,2,6],[3,3,3,6],[4,3,4,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,3,11,6],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[23,3,23,6],[24,3,24,6],[25,3,25,6],[26,3,26,6],[27,3,27,6],[28,3,28,6],[29,3,29,6],[30,3,30,6],[31,3,31,6],[32,3,32,6],[33,3,33,6],[34,3,34,6],[35,3,35,6],[36,3,36,6],[37,3,37,6],[38,3,38,6],[39,3,39,6],[40,3,40,6],[41,0,41,1],[41,3,41,6],[43,5,43,7]],"flags":["formulas_cached_only"]}
["其他项目清单与计价汇总表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":3},"标段：",null,"第1页 共1页"]
["序号","项目名称","金额(元)","结算金额(元)",{"$nulls":3},"备注"]
["1","暂列金额",""]
["2","暂估价",""]
["2.1","材料暂估价",""]
["2.2","专业工程暂估价",""]
["3","计日工",""]
["4","总承包服务费",""]
{"$rows_empty":32}
["合  计",null,""]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]

{"sheet":"7.9 表-13 规费、税金项目计价表","index":21,"n_rows":37,"n_cols":10,"rows_kept":37,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,6],[1,7,1,10],[2,2,2,5],[2,6,2,7],[2,9,2,10],[3,2,3,5],[3,6,3,7],[3,9,3,10],[4,2,4,5],[4,6,4,7],[4,9,4,10],[5,2,5,5],[5,6,5,7],[5,9,5,10],[6,2,6,5],[6,6,6,7],[6,9,6,10],[7,2,7,5],[7,6,7,7],[7,9,7,10],[8,2,8,5],[8,6,8,7],[8,9,8,10],[9,2,9,5],[9,6,9,7],[9,9,9,10],[10,2,10,5],[10,6,10,7],[10,9,10,10],[11,2,11,5],[11,6,11,7],[11,9,11,10],[12,2,12,5],[12,6,12,7],[12,9,12,10],[13,2,13,5],[13,6,13,7],[13,9,13,10],[14,2,14,5],[14,6,14,7],[14,9,14,10],[15,2,15,5],[15,6,15,7],[15,9,15,10],[16,2,16,5],[16,6,16,7],[16,9,16,10],[17,2,17,5],[17,6,17,7],[17,9,17,10],[18,2,18,5],[18,6,18,7],[18,9,18,10],[19,2,19,5],[19,6,19,7],[19,9,19,10],[20,2,20,5],[20,6,20,7],[20,9,20,10],[21,2,21,5],[21,6,21,7],[21,9,21,10],[22,2,22,5],[22,6,22,7],[22,9,22,10],[23,2,23,5],[23,6,23,7],[23,9,23,10],[24,2,24,5],[24,6,24,7],[24,9,24,10],[25,2,25,5],[25,6,25,7],[25,9,25,10],[26,2,26,5],[26,6,26,7],[26,9,26,10],[27,2,27,5],[27,6,27,7],[27,9,27,10],[28,2,28,5],[28,6,28,7],[28,9,28,10],[29,2,29,5],[29,6,29,7],[29,9,29,10],[30,2,30,5],[30,6,30,7],[30,9,30,10],[31,2,31,5],[31,6,31,7],[31,9,31,10],[33,0,33,8],[33,9,33,10],[35,5,35,10],[36,0,36,2],[36,5,36,9]],"flags":["formulas_cached_only"]}
["规费、税金项目计价表"]
["工程名称：民主路（大榆树街-花园路）路面积水整治工程",{"$nulls":3},"标段：",null,null,"第1页 共1页"]
["序号","项目名称","计算基础",{"$nulls":3},"计算基数(元)",null,"计算费率(％)","金额(元)"]
["1","规费","工程排污费+社会保险费+住房公积金",{"$nulls":5},"100.000"]
["1.1","社会保险费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"2.000"]
["1.2","住房公积金","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},"0.340"]
["1.3","工程排污费","分部分项工程费+措施项目费+其他项目费-除税工程设备费",{"$nulls":5},""]
["2","税金","分部分项工程费+措施项目费+其他项目费+规费-除税甲供材料和甲供设备费/1.01",{"$nulls":5},"11.000"]
{"$rows_empty":25}
["合  计"]
[]
[{"$nulls":5},"【新点2013清单造价江苏版 V10.3.2】"]
["编制人（造价人员）：",{"$nulls":4},"复核人（造价工程师）："]