{"text_format":"3","workbook":"xls","n_sheets":6,"sheets":["汇总表","阿湖镇","草桥镇","马陵山镇","棋盘镇","双塘镇"],"not_rendered":{"external_links":1,"defined_names":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"汇总表","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"merged":[[0,0,0,3],[9,0,9,1],[11,0,11,1],[12,0,12,1],[13,1,13,2]],"flags":["formulas_cached_only"]}
["新沂市2018年度小型农田水利重点县项目A标段（土建及安装工程）  \n投标报价汇总表"]
["组号","分组名称","投标报价\n（元）","备注"]
["1","阿湖镇高效节水灌溉"]
["2","草桥镇高效节水灌溉"]
["3","马陵山镇高效节水灌溉"]
["4","棋盘镇高效节水灌溉"]
["5","双塘镇高效节水灌溉"]
["6","安全文明措施费",{"v":60000,"d":"60000.00"}]
["7","备用金",{"v":100000,"d":"100000.00"}]
["1～7项合计"]
[]
["投标人：",null,null,"(盖章)"]
["法定代表人或委托代理人：",null,null,"(签字)"]
[null,"                年             月             日"]

{"sheet":"阿湖镇","index":1,"n_rows":135,"n_cols":7,"rows_kept":135,"merged":[[0,0,0,6],[1,2,1,3],[1,4,1,6],[130,0,130,2],[132,0,132,2],[132,3,132,5],[133,0,133,2],[134,3,134,5]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：",1,"分组名称：",null,"阿湖镇高效节水灌溉"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":8632.199999999999,"d":"8632.20"}]
[2,"土方回填压实","m3",{"v":6038.7,"d":"6038.70"}]
["二","管道安装工程"]
["（一）","小管出流"]
[1,"干管埋设(PVC-U 0.8Mpa)DN315","m",{"v":1020,"d":"1020.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN200","m",{"v":1120,"d":"1120.00"}]
[3,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":4155,"d":"4155.00"}]
[4,"干管埋设(PVC-U 0.8Mpa)DN63","m",{"v":3285,"d":"3285.00"}]
[5,"出地管(PE63 0.8Mpa)DN50","m",{"v":486,"d":"486.00"}]
[6,"PE毛管(PE63 0.8Mpa)DN25","m",{"v":202913,"d":"202913.00"}]
[7,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":11595,"d":"11595.00"}]
[8,"PE毛管DN4","m",{"v":169094,"d":"169094.00"}]
["（二）","管道灌溉"]
[1,"干管埋设(PVC-U 0.8Mpa)DN315","m",{"v":1450,"d":"1450.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":5570,"d":"5570.00"}]
[3,"出地管(PE63 0.8Mpa)DN50","m",{"v":285,"d":"285.00"}]
[4,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":5570,"d":"5570.00"}]
["三","管件及其他材料购置与安装工程"]
["（一）","小管出流"]
[1,"0.4级1.6Mpa压力表","块",{"v":4,"d":"4.00"}]
[2,"可拆卸螺翼式干式冷水表DN315","个",{"v":2,"d":"2.00"}]
[3,"可拆卸螺翼式干式冷水表DN200","个",{"v":2,"d":"2.00"}]
[4,"微阻缓闭止回阀DN315","个",{"v":1,"d":"1.00"}]
[5,"微阻缓闭止回阀DN200","个",{"v":1,"d":"1.00"}]
[6,"进排气阀(2寸)","个",{"v":4,"d":"4.00"}]
[7,"PVC-U异径三通DN200-63","个",{"v":19,"d":"19.00"}]
[8,"PVC-U异径三通DN315-90","个",{"v":16,"d":"16.00"}]
[9,"PVC-U正三通DN200-200","个",{"v":2,"d":"2.00"}]
[10,"PVC-U90°弯头DN315","个",{"v":3,"d":"3.00"}]
[11,"PVC-U90°弯头DN200","个",{"v":1,"d":"1.00"}]
[12,"PVC-U90°弯头DN90","个",{"v":1,"d":"1.00"}]
[13,"PVC-U90°弯头DN63","个",{"v":3,"d":"3.00"}]
[14,"支管阀门井","座",{"v":38,"d":"38.00"}]
[15,"支管控制阀DN90（铸铁蝶阀）","个",{"v":16,"d":"16.00"}]
[16,"支管控制阀DN63（铸铁蝶阀）","个",{"v":22,"d":"22.00"}]
[17,"泄水井","座",{"v":38,"d":"38.00"}]
[18,"泄水阀DN90（铸铁蝶阀）","个",{"v":16,"d":"16.00"}]
[19,"泄水阀DN63（铸铁蝶阀）","个",{"v":22,"d":"22.00"}]
[20,"田间阀门井","座",{"v":162,"d":"162.00"}]
[21,"PE球阀DN50","个",{"v":162,"d":"162.00"}]
[22,"PE90°弯头DN50","个",{"v":162,"d":"162.00"}]
[23,"PE正三通DN50","个",{"v":162,"d":"162.00"}]
[24,"PVC-U异径三通DN63-50","个",{"v":66,"d":"66.00"}]
[25,"PVC-U异径三通DN90-50","个",{"v":96,"d":"96.00"}]
[26,"PVC-U内螺纹接头DN50×1\"","个",{"v":324,"d":"324.00"}]
[27,"PE快接外螺纹接头DN50×1\"","个",{"v":324,"d":"324.00"}]
[28,"PE快接堵头DN50","个",{"v":324,"d":"324.00"}]
[29,"PE快接异径三通DN50-25","个",{"v":2899,"d":"2899.00"}]
[30,"PE堵头DN25","个",{"v":2899,"d":"2899.00"}]
[31,"稳流器(10L/h)","个",{"v":169094,"d":"169094.00"}]
[32,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
[33,"支墩","个",{"v":48,"d":"48.00"}]
[34,"镇墩","个",{"v":24,"d":"24.00"}]
[35,"过路","处",{"v":16,"d":"16.00"}]
[36,"过沟","处",{"v":12,"d":"12.00"}]
["（二）","管道灌溉"]
[1,"0.4级1.6Mpa压力表","块",{"v":2,"d":"2.00"}]
[2,"可拆卸螺翼式干式冷水表DN315","个",{"v":3,"d":"3.00"}]
[3,"微阻缓闭止回阀DN315","个",{"v":1,"d":"1.00"}]
[4,"进排气阀(2寸)","个",{"v":8,"d":"8.00"}]
[5,"PVC-U异径三通DN315-90","个",{"v":12,"d":"12.00"}]
[6,"PVC-U正三通DN90-90","个",{"v":2,"d":"2.00"}]
[7,"PVC-U90°弯头DN315","个",{"v":4,"d":"4.00"}]
[8,"PVC-U90°弯头DN90","个",{"v":6,"d":"6.00"}]
[9,"支管阀门井","座",{"v":14,"d":"14.00"}]
[10,"支管控制阀DN90（铸铁蝶阀）","个",{"v":14,"d":"14.00"}]
[11,"泄水井","座",{"v":14,"d":"14.00"}]
[12,"泄水阀DN90（铸铁蝶阀）","个",{"v":14,"d":"14.00"}]
[13,"田间阀门井","座",{"v":95,"d":"95.00"}]
[14,"PE球阀DN50","个",{"v":95,"d":"95.00"}]
[15,"PE球阀DN32","个",{"v":1857,"d":"1857.00"}]
[16,"PE90°弯头DN50","个",{"v":95,"d":"95.00"}]
[17,"PE正三通DN50","个",{"v":95,"d":"95.00"}]
[18,"PVC-U异径三通DN90-50","个",{"v":95,"d":"95.00"}]
[19,"PVC-U内螺纹接头DN50×1\"","个",{"v":95,"d":"95.00"}]
[20,"PE快接外螺纹接头DN50×1\"","个",{"v":95,"d":"95.00"}]
[21,"PE快接堵头DN50","个",{"v":190,"d":"190.00"}]
[22,"PE快接异径三通DN50-32","个",{"v":1857,"d":"1857.00"}]
[23,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
[24,"支墩","个",{"v":24,"d":"24.00"}]
[25,"镇墩","个",{"v":12,"d":"12.00"}]
[26,"过路","处",{"v":20,"d":"20.00"}]
[27,"过沟","处",{"v":16,"d":"16.00"}]
["四","混凝土工程"]
["（一）","一体化泵站1（1座）"]
[1,"C25砼垫层封底","m3",3.24]
[2,"C25砼进水池底板","m3",{"v":7.3,"d":"7.30"}]
[3,"C25砼进水池墙","m3",{"v":11.1,"d":"11.10"}]
[4,"C25砼一体式泵房基础","m3",4.11]
[5,"钢筋制作安装","t",1.66]
[6,"不锈钢栏杆","m",{"v":6.4,"d":"6.40"}]
[7,"MPIS100/30S20M一体化智能泵站15kW电机","座",{"v":1,"d":"1.00"},null,null,"详见图纸"]
["（二）","一体化泵站2（1座）"]
[1,"C25砼垫层封底","m3",3.63]
[2,"C25砼进水池底板","m3",{"v":7.3,"d":"7.30"}]
[3,"C25砼进水池墙","m3",{"v":11.1,"d":"11.10"}]
[4,"C25砼一体式泵房基础","m3",5.18]
[5,"钢筋制作安装","t",1.74]
[6,"不锈钢栏杆","m",{"v":6.4,"d":"6.40"}]
[7,"MPIS150/28S20M一体化智能泵站30kW电机","座",{"v":1,"d":"1.00"},null,null,"详见图纸"]
["（三）","地表水泵站（1座）"]
[1,"C25砼垫层封底","m3",0.84]
[2,"C25砼进水池底板","m3",3.11]
[3,"C25砼进水池墙","m3",6.43]
[4,"C25砼进水池顶板","m3",0.29]
[5,"C30砼盖板","m3",0.21]
[6,"C25砼镇墩","m3",0.13]
[7,"钢筋制作安装","t",0.72]
[8,"地表水泵站管理房屋","m2",{"v":21.5625,"d":"21.56"}]
["五","机电设备及安装工程"]
["（一）","地表水泵站（1座）"]
[1,"WQ2290-4134-150潜水泵（30kW电机）含配套钢管","台套",{"v":1,"d":"1.00"}]
[2,"砂石过滤器SL-S30(3)+网式过滤器4\"(5)","台套",{"v":1,"d":"1.00"}]
[3,"一体化钢制施肥罐(100L)","台套",{"v":1,"d":"1.00"}]
[4,"变频恒压开关控制柜COCON-PU 30 DV","台套",{"v":1,"d":"1.00"}]
[5,"低压电缆YJV-0.6/1KV 1(4×25+1×16)MM2 SC65 ","m",{"v":20,"d":"20.00"}]
[6,"防水电缆JHS-0.6/1KV 1(4×16)MM2 SC50 ","m",{"v":40,"d":"40.00"}]
[7,"控制电缆KVVR-450/750-8×1 SC40","m",{"v":40,"d":"40.00"}]
[8,"其他辅助配材费用","项",{"v":1,"d":"1.00"},null,null,"总价，见地表水泵房管件布置示意图"]
["六","金属结构及安装工程"]
[1,"拦污栅","t",{"v":3,"d":"3.00"}]
["七","临时工程"]
["1","施工围堰填筑拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
["2","施工排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
["3","施工房屋工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["4","其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]
[]
["投标人：",{"$nulls":5},"(盖章)"]
["法定代表人或委托代理人：",{"$nulls":5},"(签字)"]
[{"$nulls":3},"                     年        月        日"]

{"sheet":"草桥镇","index":2,"n_rows":97,"n_cols":7,"rows_kept":97,"merged":[[0,0,0,6],[1,2,1,3],[1,4,1,6],[92,0,92,2],[94,0,94,2],[94,3,94,5],[95,0,95,2],[96,3,96,5]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：",2,"分组名称：",null,"草桥镇高效节水灌溉"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":9040,"d":"9040.00"}]
[2,"土方回填压实","m3",{"v":6163.6,"d":"6163.60"}]
["二","管道安装工程"]
["（一）","喷灌"]
[1,"干管埋设(PVC-U 0.8Mpa)DN200","m",{"v":580,"d":"580.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN160","m",{"v":1010,"d":"1010.00"}]
[3,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":5600,"d":"5600.00"}]
["（二）","微灌"]
[1,"干管埋设(PVC-U 0.8Mpa)DN200","m",{"v":580,"d":"580.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":2400,"d":"2400.00"}]
[3,"PE管(PE63 0.8Mpa)DN32","m",{"v":19200,"d":"19200.00"}]
[4,"PE管(PE63 0.8Mpa)DN25","m",{"v":10800,"d":"10800.00"}]
["三","管件及其他材料购置与安装工程"]
["（一）","喷灌"]
[1,"0.4级1.6Mpa压力表","块",{"v":2,"d":"2.00"}]
[2,"可拆卸螺翼式干式冷水表DN200","个",{"v":1,"d":"1.00"}]
[3,"微阻缓闭止回阀DN200","个",{"v":1,"d":"1.00"}]
[4,"进排气阀(2寸)","个",{"v":2,"d":"2.00"}]
[5,"PVC-U异径三通DN200-160","个",{"v":4,"d":"4.00"}]
[6,"PVC-U异径三通DN160-50","个",{"v":60,"d":"60.00"}]
[7,"PVC-U异径三通DN90-25","个",{"v":320,"d":"320.00"}]
[8,"PVC-U正三通DN200-200","个",{"v":1,"d":"1.00"}]
[9,"PVC-U90°弯头DN200","个",{"v":5,"d":"5.00"}]
[10,"支管阀门井","座",{"v":7,"d":"7.00"}]
[11,"支管控制阀DN160（铸铁蝶阀）","个",{"v":7,"d":"7.00"}]
[12,"泄水井","座",{"v":7,"d":"7.00"}]
[13,"泄水阀DN160（铸铁蝶阀）","个",{"v":7,"d":"7.00"}]
[14,"田间阀门井","座",{"v":60,"d":"60.00"}]
[15,"PVC-U球阀DN90","个",{"v":60,"d":"60.00"}]
[16,"PVC-U快接堵头DN90","个",{"v":60,"d":"60.00"}]
[17,"热镀锌钢管DN25","m",{"v":800,"d":"800.00"}]
[18,"20PY2-30°金属摇臂式喷头","套",{"v":320,"d":"320.00"}]
[19,"闸阀DN25","个",{"v":320,"d":"320.00"}]
[20,"钢制三角支架","套",{"v":320,"d":"320.00"}]
[21,"支墩","个",{"v":5,"d":"5.00"}]
[22,"镇墩","个",{"v":5,"d":"5.00"}]
[23,"过路","处",{"v":5,"d":"5.00"}]
[24,"过沟","处",{"v":6,"d":"6.00"}]
[25,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["（二）","微灌"]
[1,"0.4级1.6Mpa压力表","块",{"v":2,"d":"2.00"}]
[2,"可拆卸螺翼式干式冷水表DN200","个",{"v":1,"d":"1.00"}]
[3,"微阻缓闭止回阀DN200","个",{"v":1,"d":"1.00"}]
[4,"进排气阀(2寸)","个",{"v":1,"d":"1.00"}]
[5,"PVC-U异径三通DN200-90","个",{"v":3,"d":"3.00"}]
[6,"PVC-U异径三通DN90-32","个",{"v":528,"d":"528.00"}]
[7,"PVC-U异径三通DN90-25","个",{"v":360,"d":"360.00"}]
[8,"PVC-U正三通DN200-200","个",{"v":2,"d":"2.00"}]
[9,"PVC-U正三通DN90-90","个",{"v":40,"d":"40.00"}]
[10,"PVC-U90°弯头DN200","个",{"v":4,"d":"4.00"}]
[11,"PVC-U90°弯头DN90","个",{"v":40,"d":"40.00"}]
[12,"支管阀门井","座",{"v":6,"d":"6.00"}]
[13,"支管控制阀DN90（铸铁蝶阀）","个",{"v":6,"d":"6.00"}]
[14,"泄水井","座",{"v":6,"d":"6.00"}]
[15,"泄水阀DN90（铸铁蝶阀）","个",{"v":6,"d":"6.00"}]
[16,"田间阀门井","座",{"v":40,"d":"40.00"}]
[17,"PE球阀DN90","个",{"v":40,"d":"40.00"}]
[18,"PE旁通阀DN32","个",{"v":528,"d":"528.00"}]
[19,"PE旁通阀DN25","个",{"v":360,"d":"360.00"}]
[20,"PE90°弯头DN32","个",{"v":528,"d":"528.00"}]
[21,"PE90°弯头DN25","个",{"v":360,"d":"360.00"}]
[22,"PVC-U内螺纹接头DN32×1″","个",{"v":528,"d":"528.00"}]
[23,"PE快接外螺纹接头DN32×1″","个",{"v":528,"d":"528.00"}]
[24,"PVC-U内螺纹接头DN25×1″","个",{"v":360,"d":"360.00"}]
[25,"PE快接外螺纹接头DN25×1″","个",{"v":360,"d":"360.00"}]
[26,"PE快接堵头DN32","个",{"v":528,"d":"528.00"}]
[27,"PE快接堵头DN25","个",{"v":360,"d":"360.00"}]
[28,"悬挂防滴双侧旋转式微喷头","个",{"v":4800,"d":"4800.00"}]
[29,"稳流器(10L/h)","个",{"v":11250,"d":"11250.00"}]
[30,"4爪小滴剑","个",{"v":11250,"d":"11250.00"}]
[31,"支墩","个",{"v":20,"d":"20.00"}]
[32,"镇墩","个",{"v":20,"d":"20.00"}]
[33,"过路","处",{"v":12,"d":"12.00"}]
[34,"过沟","处",{"v":12,"d":"12.00"}]
[35,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["四","机电设备购置及安装工程"]
[1,"深井潜水泵（含配套电机、防水电缆）","台套",{"v":2,"d":"2.00"}]
[2,"液位传感器","台套",{"v":2,"d":"2.00"}]
[3,"扬水管","m",{"v":160,"d":"160.00"}]
[4,"4吋离心式过滤器+4吋网式过滤器","台套",{"v":2,"d":"2.00"}]
[5,"一体化钢制施肥罐(100L)","台套",{"v":2,"d":"2.00"}]
[6,"变频恒压开关控制柜COCON-PU 15 DV","台套",{"v":2,"d":"2.00"}]
[7,"控制电缆KVVR-450/750-8×1 SC40","m",{"v":140,"d":"140.00"}]
[8,"低压电缆YJV-0.6/1KV 1(5×10)MM2 SC40 ","m",{"v":40,"d":"40.00"}]
[9,"其他辅助配材费用","项",{"v":1,"d":"1.00"},null,null,"总价，见井房布置图"]
["五","临时工程"]
["1","施工房屋工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["2","其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]
[]
["投标人：",{"$nulls":5},"(盖章)"]
["法定代表人或委托代理人：",{"$nulls":5},"(签字)"]
[{"$nulls":3},"                     年        月        日"]

{"sheet":"马陵山镇","index":3,"n_rows":200,"n_cols":7,"rows_kept":200,"merged":[[0,0,0,6],[1,2,1,3],[1,4,1,6],[195,0,195,2],[197,0,197,2],[197,3,197,5],[198,0,198,2],[199,3,199,5]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：",3,"分组名称：",null,"马陵山镇高效节水灌溉"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":19125,"d":"19125.00"}]
[2,"土方回填压实","m3",{"v":15300,"d":"15300.00"}]
["二","管道安装工程"]
["（一）","滴灌"]
[1,"干管埋设(PVC-U 0.8Mpa)DN315","m",{"v":1670,"d":"1670.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":340,"d":"340.00"}]
[3,"干管埋设(PVC-U 0.8Mpa)DN160","m",{"v":5390,"d":"5390.00"}]
[4,"干管埋设(PVC-U 0.8Mpa)DN63","m",{"v":1040,"d":"1040.00"}]
[5,"出地管(PE63 0.8Mpa)DN50","m",{"v":402,"d":"402.00"}]
[6,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":7470,"d":"7470.00"}]
["（二）","微喷灌"]
[1,"干管埋设(PVC-U 0.8Mpa)DN315","m",{"v":1870,"d":"1870.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN110","m",{"v":180,"d":"180.00"}]
[3,"干管埋设(PVC-U 0.8Mpa)DN160","m",{"v":5220,"d":"5220.00"}]
[4,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":780,"d":"780.00"}]
[5,"出地管(PE63 0.8Mpa)DN50","m",{"v":375,"d":"375.00"}]
[6,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":6000,"d":"6000.00"}]
["（三）","小管出流"]
[1,"干管埋设(PVC-U 0.8Mpa)DN160","m",{"v":510,"d":"510.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":3940,"d":"3940.00"}]
[3,"干管埋设(PVC-U 0.8Mpa)DN63","m",{"v":16050,"d":"16050.00"}]
[4,"出地管(PE63 0.8Mpa)DN50","m",{"v":1332,"d":"1332.00"}]
[5,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":27660,"d":"27660.00"}]
[6,"PE毛管(PE63 0.8Mpa)DN25","m",{"v":346350,"d":"346350.00"}]
[7,"PE毛管DN4","m",{"v":173175,"d":"173175.00"}]
["三","管件及其他材料购置与安装工程"]
["（一）","滴灌"]
[1,"0.4级1.6Mpa压力表","块",{"v":4,"d":"4.00"}]
[2,"可拆卸螺翼式干式冷水表DN315","个",{"v":3,"d":"3.00"}]
[3,"可拆卸螺翼式干式冷水表DN90","个",{"v":3,"d":"3.00"}]
[4,"微阻缓闭止回阀DN315","个",{"v":1,"d":"1.00"}]
[5,"微阻缓闭止回阀DN90","个",{"v":1,"d":"1.00"}]
[6,"进排气阀(2寸)","个",{"v":10,"d":"10.00"}]
[7,"PVC-U异径三通DN315-160","个",{"v":25,"d":"25.00"}]
[8,"PVC-U异径三通DN90-63","个",{"v":6,"d":"6.00"}]
[9,"PVC-U正三通DN160-160","个",{"v":3,"d":"3.00"}]
[10,"PVC-U正三通DN90-90","个",{"v":1,"d":"1.00"}]
[11,"PVC-U90°弯头DN315","个",{"v":3,"d":"3.00"}]
[12,"PVC-U90°弯头DN63","个",{"v":2,"d":"2.00"}]
[13,"支管阀门井","座",{"v":36,"d":"36.00"}]
[14,"支管控制阀DN160（铸铁蝶阀）","个",{"v":28,"d":"28.00"}]
[15,"支管控制阀DN63（铸铁蝶阀）","个",{"v":8,"d":"8.00"}]
[16,"泄水井","座",{"v":36,"d":"36.00"}]
[17,"泄水阀DN160（铸铁蝶阀）","个",{"v":28,"d":"28.00"}]
[18,"泄水阀DN63（铸铁蝶阀）","个",{"v":8,"d":"8.00"}]
[19,"田间阀门井","座",{"v":134,"d":"134.00"}]
[20,"PE球阀DN50","个",{"v":134,"d":"134.00"}]
[21,"PE90°弯头DN50","个",{"v":134,"d":"134.00"}]
[22,"PE正三通DN50","个",{"v":134,"d":"134.00"}]
[23,"PVC-U异径三通DN160-50","个",{"v":134,"d":"134.00"}]
[24,"PVC-U内螺纹接头DN50×1\"","个",{"v":158,"d":"158.00"}]
[25,"PE快接外螺纹接头DN50×1\"","个",{"v":158,"d":"158.00"}]
[26,"PE快接堵头DN50","个",{"v":268,"d":"268.00"}]
[27,"PE快接异径三通DN50-16","个",{"v":4236,"d":"4236.00"}]
[28,"PE旁通阀DN16","个",{"v":4236,"d":"4236.00"}]
[29,"PE壁厚0.4mm贴片式滴灌带DN16","m",{"v":276480,"d":"276480.00"}]
[30,"PE堵头DN16","个",{"v":4236,"d":"4236.00"}]
[31,"支墩","个",{"v":30,"d":"30.00"}]
[32,"镇墩","个",{"v":18,"d":"18.00"}]
[33,"过路","处",{"v":24,"d":"24.00"}]
[34,"过沟","处",{"v":18,"d":"18.00"}]
[35,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["（二）","微喷灌"]
[1,"0.4级1.6Mpa压力表","块",{"v":6,"d":"6.00"}]
[2,"可拆卸螺翼式干式冷水表DN315","个",{"v":6,"d":"6.00"}]
[3,"可拆卸螺翼式干式冷水表DN90","个",{"v":2,"d":"2.00"}]
[4,"微阻缓闭止回阀DN315","个",{"v":2,"d":"2.00"}]
[5,"微阻缓闭止回阀DN90","个",{"v":1,"d":"1.00"}]
[6,"进排气阀(2寸)","个",{"v":14,"d":"14.00"}]
[7,"PVC-U异径三通DN110-90","个",{"v":3,"d":"3.00"}]
[8,"PVC-U异径三通DN315-160","个",{"v":41,"d":"41.00"}]
[9,"PVC-U正三通DN160-160","个",{"v":1,"d":"1.00"}]
[10,"PVC-U正三通DN110-110","个",{"v":2,"d":"2.00"}]
[11,"PVC-U90°弯头DN315","个",{"v":5,"d":"5.00"}]
[12,"PVC-U90°弯头DN160","个",{"v":3,"d":"3.00"}]
[13,"PVC-U90°弯头DN90","个",{"v":2,"d":"2.00"}]
[14,"支管阀门井","座",{"v":45,"d":"45.00"}]
[15,"支管控制阀DN160（铸铁蝶阀）","个",{"v":40,"d":"40.00"}]
[16,"支管控制阀DN90（铸铁蝶阀）","个",{"v":5,"d":"5.00"}]
[17,"泄水井","座",{"v":45,"d":"45.00"}]
[18,"泄水阀DN160（铸铁蝶阀）","个",{"v":40,"d":"40.00"}]
[19,"泄水阀DN90（铸铁蝶阀）","个",{"v":5,"d":"5.00"}]
[20,"田间阀门井","座",{"v":125,"d":"125.00"}]
[21,"PE球阀DN50","个",{"v":125,"d":"125.00"}]
[22,"PE90°弯头DN50","个",{"v":125,"d":"125.00"}]
[23,"PE正三通DN50","个",{"v":125,"d":"125.00"}]
[24,"PVC-U异径三通DN160-50","个",{"v":50,"d":"50.00"}]
[25,"PVC-U异径三通DN90-50","个",{"v":75,"d":"75.00"}]
[26,"PVC-U内螺纹接头DN50×1\"","个",{"v":125,"d":"125.00"}]
[27,"PE快接外螺纹接头DN50×1\"","个",{"v":125,"d":"125.00"}]
[28,"PE快接堵头DN50","个",{"v":250,"d":"250.00"}]
[29,"PE快接异径三通DN50-25","个",{"v":1686,"d":"1686.00"}]
[30,"PE旁通阀DN25","个",{"v":1686,"d":"1686.00"}]
[31,"PE斜三孔微喷带DN25","m",{"v":15600,"d":"15600.00"}]
[32,"PE堵头DN25","个",{"v":195,"d":"195.00"}]
[33,"支墩","个",{"v":46,"d":"46.00"}]
[34,"镇墩","个",{"v":23,"d":"23.00"}]
[35,"过路","处",{"v":23,"d":"23.00"}]
[36,"过沟","处",{"v":14,"d":"14.00"}]
[37,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["（三）","小管出流"]
[1,"0.4级1.6Mpa压力表","块",{"v":32,"d":"32.00"}]
[2,"可拆卸螺翼式干式冷水表DN90","个",{"v":30,"d":"30.00"}]
[3,"可拆卸螺翼式干式冷水表DN160","个",{"v":2,"d":"2.00"}]
[4,"微阻缓闭止回阀DN90","个",{"v":15,"d":"15.00"}]
[5,"微阻缓闭止回阀DN160","个",{"v":1,"d":"1.00"}]
[6,"进排气阀(2寸)","个",{"v":32,"d":"32.00"}]
[7,"PVC-U异径三通DN160-63","个",{"v":6,"d":"6.00"}]
[8,"PVC-U异径三通DN90-63","个",{"v":66,"d":"66.00"}]
[9,"PVC-U正三通DN90-90","个",{"v":20,"d":"20.00"}]
[10,"PVC-U正三通DN160-160","个",{"v":1,"d":"1.00"}]
[11,"PVC-U90°弯头DN160","个",{"v":3,"d":"3.00"}]
[12,"PVC-U90°弯头DN90","个",{"v":6,"d":"6.00"}]
[13,"PVC-U90°弯头DN63","个",{"v":32,"d":"32.00"}]
[14,"支管阀门井","座",{"v":106,"d":"106.00"}]
[15,"支管控制阀DN63（铸铁蝶阀）","个",{"v":106,"d":"106.00"}]
[16,"泄水井","座",{"v":106,"d":"106.00"}]
[17,"泄水阀DN63（铸铁蝶阀）","个",{"v":106,"d":"106.00"}]
[18,"田间阀门井","座",{"v":444,"d":"444.00"}]
[19,"PE球阀DN50","个",{"v":444,"d":"444.00"}]
[20,"PE90°弯头DN50","个",{"v":444,"d":"444.00"}]
[21,"PE正三通DN50","个",{"v":444,"d":"444.00"}]
[22,"PVC-U异径三通DN63-50","个",{"v":444,"d":"444.00"}]
[23,"PVC-U内螺纹接头DN50×1\"","个",{"v":888,"d":"888.00"}]
[24,"PE快接外螺纹接头DN50×1\"","个",{"v":888,"d":"888.00"}]
[25,"PE快接堵头DN50","个",{"v":888,"d":"888.00"}]
[26,"PE快接异径三通DN50-25","个",{"v":6915,"d":"6915.00"}]
[27,"PE堵头DN25","个",{"v":6915,"d":"6915.00"}]
[28,"稳流器(10L/h)","个",{"v":173175,"d":"173175.00"}]
[29,"支墩","个",{"v":96,"d":"96.00"}]
[30,"镇墩","个",{"v":48,"d":"48.00"}]
[31,"过路","处",{"v":48,"d":"48.00"}]
[32,"过沟","处",{"v":32,"d":"32.00"}]
[33,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["四","混凝土工程"]
["（一）","地表水泵站（4座）"]
[1,"C25砼垫层封底","m3",3.36]
[2,"C25砼进水池底板","m3",12.44]
[3,"C25砼进水池墙","m3",25.72]
[4,"C25砼进水池顶板","m3",1.16]
[5,"C30砼盖板","m3",0.84]
[6,"C25砼镇墩","m3",0.52]
[7,"钢筋制作安装","t",2.88]
[8,"地表水泵站管理房屋","m2",{"v":80,"d":"80.00"}]
["（二）","深水井（17眼）"]
[1,"Φ30cm灌溉井成井","m",{"v":1360,"d":"1360.00"}]
[2,"井房","m2",{"v":204,"d":"204.00"}]
["五","机电设备及安装工程"]
["（一）","地表水泵站（4座）"]
[1,"WQ2290-4170-150潜水泵（45kW电机）含配套钢管","台套",{"v":1,"d":"1.00"}]
[2,"变频恒压开关控制柜COCON-PU 45 DV","台套",{"v":1,"d":"1.00"}]
[3,"低压电缆YJV-0.6/1KV 1(4×50+1×25)MM2 SC80 ","m",{"v":20,"d":"20.00"}]
[4,"防水电缆JHS-0.6/1KV 1(4×25)MM2 SC65","m",{"v":40,"d":"40.00"}]
[5,"WQ2260-2124-100潜水泵（22kW电机）含配套钢管","台套",{"v":1,"d":"1.00"}]
[6,"变频恒压开关控制柜COCON-PU 22 DV","台套",{"v":1,"d":"1.00"}]
[7,"低压电缆YJV-0.6/1KV 1(5×16)MM2 SC50","m",{"v":20,"d":"20.00"}]
[8,"防水电缆JHS-0.6/1KV 1(4×10)MM2 SC40","m",{"v":40,"d":"40.00"}]
[9,"WQ2290-2131-100潜水泵（30kW电机）含配套钢管","台套",{"v":1,"d":"1.00"}]
[10,"变频恒压开关控制柜COCON-PU 30 DV","台套",{"v":1,"d":"1.00"}]
[11,"低压电缆YJV-0.6/1KV 1(4×25+1×16)MM2 SC65 ","m",{"v":20,"d":"20.00"}]
[12,"防水电缆JHS-0.6/1KV 1(4×16)MM2 SC50 ","m",{"v":40,"d":"40.00"}]
[13,"WQ2210-2111-65潜水泵（11kW电机）含配套钢管","台套",{"v":1,"d":"1.00"}]
[14,"变频恒压开关控制柜COCON-PU 11 DV","台套",{"v":1,"d":"1.00"}]
[15,"低压电缆YJV-0.6/1KV 1(5×6)MM2 SC40","m",{"v":20,"d":"20.00"}]
[16,"防水电缆JHS-0.6/1KV 1(4×4)MM2 SC40","m",{"v":40,"d":"40.00"}]
[17,"砂石过滤器SL-S30(4)+网式过滤器4\"(8)","台套",{"v":1,"d":"1.00"}]
[18,"砂石过滤器SL-S30(1)+网式过滤器4\"(3)","台套",{"v":1,"d":"1.00"}]
[19,"砂石过滤器SL-S30(3)+网式过滤器4\"(5)","台套",{"v":1,"d":"1.00"}]
[20,"砂石过滤器SL-S30(1)+网式过滤器4\"(1)","台套",{"v":1,"d":"1.00"}]
[21,"一体化钢制施肥罐(100L)","台套",{"v":4,"d":"4.00"}]
[22,"控制电缆KVVR-450/750-8×1 SC40","m",{"v":160,"d":"160.00"}]
[23,"其他辅助配材费用","项",{"v":1,"d":"1.00"},null,null,"总价，见地表水泵房管件布置示意图"]
["（二）","深水井（17眼）"]
[1,"深井潜水泵（含配套电机、防水电缆）","台套",{"v":17,"d":"17.00"}]
[2,"液位传感器","台套",{"v":17,"d":"17.00"}]
[3,"扬水管","m",{"v":1190,"d":"1190.00"}]
[4,"4吋离心式过滤器+4吋网式过滤器","台套",{"v":17,"d":"17.00"}]
[5,"一体化钢制施肥罐(100L)","台套",{"v":17,"d":"17.00"}]
[6,"变频恒压开关控制柜COCON-PU 5.5 DV","台套",{"v":10,"d":"10.00"}]
[7,"变频恒压开关控制柜COCON-PU 7.5 DV","台套",{"v":6,"d":"6.00"}]
[8,"变频恒压开关控制柜COCON-PU 11 DV","台套",{"v":1,"d":"1.00"}]
[9,"低压电缆YJV-0.6/1KV 1(5×6)MM2 SC40","m",{"v":340,"d":"340.00"}]
[10,"控制电缆KVVR-450/750-8×1 SC40","m",{"v":1190,"d":"1190.00"}]
[11,"其他辅助配材费用","项",{"v":1,"d":"1.00"},null,null,"总价，见井房布置图"]
["六","金属结构及安装工程"]
[1,"拦污栅","t",{"v":4,"d":"4.00"}]
["七","临时工程"]
["1","施工围堰填筑拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
["2","施工排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
["3","施工房屋工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["4","其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]
[]
["投标人：",{"$nulls":5},"(盖章)"]
["法定代表人或委托代理人：",{"$nulls":5},"(签字)"]
[{"$nulls":3},"                     年        月        日"]

{"sheet":"棋盘镇","index":4,"n_rows":179,"n_cols":7,"rows_kept":179,"merged":[[0,0,0,6],[1,2,1,3],[1,4,1,6],[174,0,174,2],[176,0,176,2],[176,3,176,5],[177,0,177,2],[178,3,178,5]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：",4,"分组名称：",null,"棋盘镇高效节水灌溉"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":20980,"d":"20980.00"}]
[2,"土方回填压实","m3",{"v":14749.3,"d":"14749.30"}]
["二","管道安装工程"]
["（一）","滴灌"]
[1,"干管埋设(PVC-U 0.8Mpa)DN160","m",{"v":870,"d":"870.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN63","m",{"v":3910,"d":"3910.00"}]
[3,"出地管(PE63 0.8Mpa)DN50","m",{"v":432,"d":"432.00"}]
[4,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":7820,"d":"7820.00"}]
["（二）","管道灌溉"]
[1,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":90,"d":"90.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN63","m",{"v":750,"d":"750.00"}]
[3,"出地管(PE63 0.8Mpa)DN32","m",{"v":750,"d":"750.00"}]
["（三）","小管出流"]
[1,"干管埋设(PVC-U 0.8Mpa)DN200","m",{"v":320,"d":"320.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN160","m",{"v":2805,"d":"2805.00"}]
[3,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":4915,"d":"4915.00"}]
[4,"干管埋设(PVC-U 0.8Mpa)DN63","m",{"v":25120,"d":"25120.00"}]
[5,"出地管(PE63 0.8Mpa)DN50","m",{"v":1908,"d":"1908.00"}]
[6,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":47020,"d":"47020.00"}]
[7,"PE毛管(PE63 0.8Mpa)DN25","m",{"v":600400,"d":"600400.00"}]
[8,"PE毛管DN4","m",{"v":300200,"d":"300200.00"}]
["三","管件及其他材料购置与安装工程"]
["（一）","滴灌"]
[1,"0.4级1.6Mpa压力表","块",{"v":6,"d":"6.00"}]
[2,"可拆卸螺翼式干式冷水表DN90","个",{"v":6,"d":"6.00"}]
[3,"可拆卸螺翼式干式冷水表DN160","个",{"v":3,"d":"3.00"}]
[4,"微阻缓闭止回阀DN90","个",{"v":2,"d":"2.00"}]
[5,"微阻缓闭止回阀DN160","个",{"v":1,"d":"1.00"}]
[6,"进排气阀(2寸)","个",{"v":10,"d":"10.00"}]
[7,"PVC-U异径三通DN160-63","个",{"v":6,"d":"6.00"}]
[8,"PVC-U异径三通DN90-63","个",{"v":4,"d":"4.00"}]
[9,"PVC-U正三通DN160-160","个",{"v":1,"d":"1.00"}]
[10,"PVC-U正三通DN90-90","个",{"v":2,"d":"2.00"}]
[11,"PVC-U正三通DN63-63","个",{"v":6,"d":"6.00"}]
[12,"PVC-U90°弯头DN63","个",{"v":4,"d":"4.00"}]
[13,"支管阀门井","座",{"v":24,"d":"24.00"}]
[14,"支管控制阀DN63（铸铁蝶阀）","个",{"v":24,"d":"24.00"}]
[15,"泄水井","座",{"v":24,"d":"24.00"}]
[16,"泄水阀DN63（铸铁蝶阀）","个",{"v":24,"d":"24.00"}]
[17,"田间阀门井","座",{"v":144,"d":"144.00"}]
[18,"PE球阀DN50","个",{"v":144,"d":"144.00"}]
[19,"PE90°弯头DN50","个",{"v":144,"d":"144.00"}]
[20,"PE正三通DN50","个",{"v":144,"d":"144.00"}]
[21,"PE异径三通DN63-50","个",{"v":144,"d":"144.00"}]
[22,"PVC-U内螺纹接头DN50×1\"","个",{"v":144,"d":"144.00"}]
[23,"PE快接外螺纹接头DN50×1\"","个",{"v":144,"d":"144.00"}]
[24,"PE快接堵头DN50","个",{"v":288,"d":"288.00"}]
[25,"PE快接异径三通DN50-16","个",{"v":3910,"d":"3910.00"}]
[26,"PE壁厚0.4mm贴片式滴灌带DN16","m",{"v":211500,"d":"211500.00"}]
[27,"PE旁通阀DN16","个",{"v":3910,"d":"3910.00"}]
[28,"PE堵头DN16","个",{"v":3910,"d":"3910.00"}]
[29,"支墩","个",{"v":32,"d":"32.00"}]
[30,"镇墩","个",{"v":32,"d":"32.00"}]
[31,"过路","处",{"v":14,"d":"14.00"}]
[32,"过沟","处",{"v":9,"d":"9.00"}]
[33,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["（二）","管道灌溉"]
[1,"0.4级1.6Mpa压力表","块",{"v":2,"d":"2.00"}]
[2,"可拆卸螺翼式干式冷水表DN90","个",{"v":2,"d":"2.00"}]
[3,"微阻缓闭止回阀DN90","个",{"v":1,"d":"1.00"}]
[4,"进排气阀(2寸)","个",{"v":2,"d":"2.00"}]
[5,"PVC-U异径三通DN90-63","个",{"v":2,"d":"2.00"}]
[6,"PVC-U正三通DN90-90","个",{"v":1,"d":"1.00"}]
[7,"PVC-U90°弯头DN63","个",{"v":2,"d":"2.00"}]
[8,"支管阀门井","座",{"v":4,"d":"4.00"}]
[9,"支管控制阀DN63（铸铁蝶阀）","个",{"v":4,"d":"4.00"}]
[10,"泄水井","座",{"v":4,"d":"4.00"}]
[11,"泄水阀DN63（铸铁蝶阀）","个",{"v":4,"d":"4.00"}]
[12,"PE球阀DN32","个",{"v":250,"d":"250.00"}]
[13,"PE90°弯头DN32","个",{"v":250,"d":"250.00"}]
[14,"PVC-U异径三通DN63-32","个",{"v":250,"d":"250.00"}]
[15,"PVC-U内螺纹接头DN32×1\"","个",{"v":250,"d":"250.00"}]
[16,"PE快接外螺纹接头DN32×1\"","个",{"v":250,"d":"250.00"}]
[17,"支墩","个",{"v":5,"d":"5.00"}]
[18,"镇墩","个",{"v":3,"d":"3.00"}]
[19,"过路","处",{"v":5,"d":"5.00"}]
[20,"过沟","处",{"v":1,"d":"1.00"}]
[21,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["（三）","小管出流"]
[1,"0.4级1.6Mpa压力表","块",{"v":36,"d":"36.00"}]
[2,"可拆卸螺翼式干式冷水表DN200","个",{"v":1,"d":"1.00"}]
[3,"可拆卸螺翼式干式冷水表DN160","个",{"v":10,"d":"10.00"}]
[4,"可拆卸螺翼式干式冷水表DN90","个",{"v":29,"d":"29.00"}]
[5,"微阻缓闭止回阀DN200","个",{"v":1,"d":"1.00"}]
[6,"微阻缓闭止回阀DN160","个",{"v":2,"d":"2.00"}]
[7,"微阻缓闭止回阀DN90","个",{"v":15,"d":"15.00"}]
[8,"进排气阀(2寸)","个",{"v":40,"d":"40.00"}]
[9,"PVC-U异径三通DN200-160","个",{"v":1,"d":"1.00"}]
[10,"PVC-U异径三通DN160-63","个",{"v":16,"d":"16.00"}]
[11,"PVC-U异径三通DN160-90","个",{"v":8,"d":"8.00"}]
[12,"PVC-U异径三通DN90-63","个",{"v":77,"d":"77.00"}]
[13,"PVC-U正三通DN90-90","个",{"v":14,"d":"14.00"}]
[14,"PVC-U正三通DN160-160","个",{"v":1,"d":"1.00"}]
[15,"PVC-U90°弯头DN160","个",{"v":12,"d":"12.00"}]
[16,"PVC-U90°弯头DN90","个",{"v":2,"d":"2.00"}]
[17,"PVC-U90°弯头DN63","个",{"v":37,"d":"37.00"}]
[18,"支管阀门井","座",{"v":136,"d":"136.00"}]
[19,"支管控制阀DN63（铸铁蝶阀）","个",{"v":136,"d":"136.00"}]
[20,"泄水井","座",{"v":136,"d":"136.00"}]
[21,"泄水阀DN63（铸铁蝶阀）","个",{"v":136,"d":"136.00"}]
[22,"田间阀门井","座",{"v":636,"d":"636.00"}]
[23,"PE球阀DN50","个",{"v":636,"d":"636.00"}]
[24,"PE90°弯头DN50","个",{"v":636,"d":"636.00"}]
[25,"PE正三通DN50","个",{"v":636,"d":"636.00"}]
[26,"PVC-U异径三通DN63-50","个",{"v":636,"d":"636.00"}]
[27,"PVC-U内螺纹接头DN50×1\"","个",{"v":1188,"d":"1188.00"}]
[28,"PE快接外螺纹接头DN50×1\"","个",{"v":1188,"d":"1188.00"}]
[29,"PE快接堵头DN50","个",{"v":1272,"d":"1272.00"}]
[30,"PE快接异径三通DN50-25","个",{"v":11755,"d":"11755.00"}]
[31,"PE堵头DN25","个",{"v":11755,"d":"11755.00"}]
[32,"稳流器(10L/h)","个",{"v":300200,"d":"300200.00"}]
[33,"支墩","个",{"v":156,"d":"156.00"}]
[34,"镇墩","个",{"v":111,"d":"111.00"}]
[35,"过路","处",{"v":86,"d":"86.00"}]
[36,"过沟","处",{"v":40,"d":"40.00"}]
[37,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["四","混凝土工程"]
["（一）","一体化泵站1（1座）"]
[1,"C25砼垫层封底","m3",3.24]
[2,"C25砼进水池底板","m3",{"v":7.3,"d":"7.30"}]
[3,"C25砼进水池墙","m3",{"v":11.1,"d":"11.10"}]
[4,"C25砼一体式泵房基础","m3",4.11]
[5,"钢筋制作安装","t",1.66]
[6,"不锈钢栏杆","m",{"v":6.4,"d":"6.40"}]
[7,"MPIS100/30S20M一体化智能泵站15kW电机","座",{"v":1,"d":"1.00"},null,null,"详见图纸"]
["（三）","地表水泵站（3座）"]
[1,"C25砼垫层封底","m3",2.52]
[2,"C25砼进水池底板","m3",9.33]
[3,"C25砼进水池墙","m3",19.29]
[4,"C25砼进水池顶板","m3",{"v":0.8699999999999999,"d":"0.87"}]
[5,"C30砼盖板","m3",0.63]
[6,"C25砼镇墩","m3",0.39]
[7,"钢筋制作安装","t",2.16]
[8,"地表水泵站管理房屋","m2",{"v":45.5625,"d":"45.56"}]
["（二）","深水井（新打7眼）"]
[1,"Φ30cm灌溉井成井","m",{"v":560,"d":"560.00"}]
[2,"井房","m2",{"v":84,"d":"84.00"}]
["五","机电设备及安装工程"]
["（三）","地表水泵站（3座）"]
[1,"WQ2260-2124-100潜水泵（22kW电机）含配套钢管","台套",{"v":1,"d":"1.00"}]
[2,"变频恒压开关控制柜COCON-PU 22 DV","台套",{"v":1,"d":"1.00"}]
[3,"低压电缆YJV-0.6/1KV 1(5×16)MM2 SC50","m",{"v":20,"d":"20.00"}]
[4,"防水电缆JHS-0.6/1KV 1(4×10)MM2 SC40","m",{"v":40,"d":"40.00"}]
[5,"WQ2210-2115-80潜水泵（11kW电机）含配套钢管","台套",{"v":2,"d":"2.00"}]
[6,"变频恒压开关控制柜COCON-PU 11 DV","台套",{"v":2,"d":"2.00"}]
[7,"低压电缆YJV-0.6/1KV 1(5×6)MM2 SC40","m",{"v":40,"d":"40.00"}]
[8,"防水电缆JHS-0.6/1KV 1(4×4)MM2 SC40","m",{"v":80,"d":"80.00"}]
[9,"砂石过滤器SL-S30(1)+网式过滤器4\"(1)","台套",{"v":2,"d":"2.00"}]
[10,"砂石过滤器SL-S30(2)+网式过滤器4\"(4)","台套",{"v":1,"d":"1.00"}]
[11,"一体化钢制施肥罐(100L)","台套",{"v":3,"d":"3.00"}]
[12,"控制电缆KVVR-450/750-8×1 SC40","m",{"v":120,"d":"120.00"}]
[13,"其他辅助配材费用","项",{"v":1,"d":"1.00"},null,null,"总价，见地表水泵房管件布置示意图"]
["（二）","深水井（18眼）"]
[1,"深井潜水泵（含配套电机、防水电缆）","台套",{"v":18,"d":"18.00"}]
[2,"液位传感器","台套",{"v":18,"d":"18.00"}]
[3,"扬水管","m",{"v":1260,"d":"1260.00"}]
[4,"4吋离心式过滤器+4吋网式过滤器","台套",{"v":18,"d":"18.00"}]
[5,"一体化钢制施肥罐(100L)","台套",{"v":18,"d":"18.00"}]
[6,"变频恒压开关控制柜COCON-PU 5.5 DV","台套",{"v":13,"d":"13.00"}]
[7,"变频恒压开关控制柜COCON-PU 7.5 DV","台套",{"v":5,"d":"5.00"}]
[8,"低压电缆YJV-0.6/1KV 1(5×6)MM2 SC40","m",{"v":360,"d":"360.00"}]
[9,"控制电缆KVVR-450/750-8×1 SC40","m",{"v":1260,"d":"1260.00"}]
[10,"其他辅助配材费用","项",{"v":1,"d":"1.00"},null,null,"总价，见井房布置图"]
["六","金属结构及安装工程"]
[1,"拦污栅","t",{"v":3,"d":"3.00"}]
["七","临时工程"]
["1","施工围堰填筑拆除","项",{"v":1,"d":"1.00"},null,null,"总价"]
["2","施工排水","项",{"v":1,"d":"1.00"},null,null,"总价"]
["3","施工房屋工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["4","其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]
[]
["投标人：",{"$nulls":5},"(盖章)"]
["法定代表人或委托代理人：",{"$nulls":5},"(签字)"]
[{"$nulls":3},"             年             月             日"]

{"sheet":"双塘镇","index":5,"n_rows":67,"n_cols":7,"rows_kept":67,"merged":[[0,0,0,6],[1,2,1,3],[1,4,1,6],[62,0,62,2],[64,0,64,2],[64,3,64,5],[65,0,65,2],[66,3,66,5]],"flags":["formulas_cached_only"]}
["分组工程量清单"]
["组号：",5,"分组名称：",null,"双塘镇高效节水灌溉"]
["序号","项目名称","单位","数量","单价（元）","合价（元）","备注"]
["一","土方工程"]
[1,"土方开挖","m3",{"v":10672.300000000001,"d":"10672.30"}]
[2,"土方回填压实","m3",{"v":7275.2,"d":"7275.20"}]
["二","管道安装工程"]
["（一）","滴灌"]
[1,"干管埋设(PVC-U 0.8Mpa)DN90","m",{"v":4630,"d":"4630.00"}]
[2,"干管埋设(PVC-U 0.8Mpa)DN63","m",{"v":15121,"d":"15121.00"}]
[3,"出地管(PE63 0.8Mpa)DN50","m",{"v":1647,"d":"1647.00"}]
[4,"PE辅管(PE63 0.8Mpa)DN50","m",{"v":27912,"d":"27912.00"}]
["三","管件及其他材料购置与安装工程"]
["（一）","滴灌"]
[1,"0.4级1.6Mpa压力表","块",{"v":42,"d":"42.00"}]
[2,"可拆卸螺翼式干式冷水表DN90","个",{"v":63,"d":"63.00"}]
[3,"微阻缓闭止回阀DN90","个",{"v":21,"d":"21.00"}]
[4,"进排气阀(2寸)","个",{"v":42,"d":"42.00"}]
[5,"PVC-U异径三通DN90-63","个",{"v":73,"d":"73.00"}]
[6,"PVC-U正三通DN90-90","个",{"v":19,"d":"19.00"}]
[7,"PVC-U90°弯头DN90","个",{"v":2,"d":"2.00"}]
[8,"PVC-U90°弯头DN63","个",{"v":40,"d":"40.00"}]
[9,"支管阀门井","座",{"v":112,"d":"112.00"}]
[10,"支管控制阀DN63（铸铁蝶阀）","个",{"v":112,"d":"112.00"}]
[11,"泄水井","座",{"v":112,"d":"112.00"}]
[12,"支管泄水阀DN63（铸铁蝶阀）","个",{"v":112,"d":"112.00"}]
[13,"田间阀门井","座",{"v":549,"d":"549.00"}]
[14,"PE球阀DN50","个",{"v":549,"d":"549.00"}]
[15,"PE90°弯头DN50","个",{"v":549,"d":"549.00"}]
[16,"PE正三通DN50","个",{"v":549,"d":"549.00"}]
[17,"PVC-U异径三通DN63-50","个",{"v":549,"d":"549.00"}]
[18,"PVC-U内螺纹接头DN50×1\"","个",{"v":1098,"d":"1098.00"}]
[19,"PE快接外螺纹接头DN50×1\"","个",{"v":1098,"d":"1098.00"}]
[20,"PE快接堵头DN50","个",{"v":1098,"d":"1098.00"}]
[21,"PE快接异径三通DN50-16","个",{"v":11316,"d":"11316.00"}]
[22,"PE旁通阀DN16","个",{"v":11316,"d":"11316.00"}]
[23,"PE壁厚0.4mm贴片式滴灌带DN16","m",{"v":601816,"d":"601816.00"}]
[24,"PE堵头DN16","个",{"v":11316,"d":"11316.00"}]
[25,"支墩","个",{"v":126,"d":"126.00"}]
[26,"镇墩","个",{"v":126,"d":"126.00"}]
[27,"过路","处",{"v":84,"d":"84.00"}]
[28,"过沟","处",{"v":50,"d":"50.00"}]
[29,"主管道试压","项",{"v":1,"d":"1.00"},null,null,"总价"]
["四","混凝土工程"]
["（一）","深水井（新打14眼）"]
[1,"DN30cm灌溉井成井","m",{"v":1120,"d":"1120.00"}]
[2,"井房","m2",{"v":168,"d":"168.00"}]
["五","机电设备及安装工程"]
["（一）","深水井（21眼）"]
[1,"深井潜水泵（含配套电机、防水电缆）","台套",{"v":21,"d":"21.00"}]
[2,"液位传感器","台套",{"v":21,"d":"21.00"}]
[3,"扬水管","m",{"v":1470,"d":"1470.00"}]
[4,"4吋离心式过滤器+4吋网式过滤器","台套",{"v":21,"d":"21.00"}]
[5,"一体化钢制施肥罐(100L)","台套",{"v":21,"d":"21.00"}]
[6,"变频恒压开关控制柜COCON-PU 5.5 DV","台套",{"v":12,"d":"12.00"}]
[7,"变频恒压开关控制柜COCON-PU 7.5 DV","台套",{"v":9,"d":"9.00"}]
[8,"低压电缆YJV-0.6/1KV 1(5×6)MM2 SC40","m",{"v":420,"d":"420.00"}]
[9,"控制电缆KVVR-450/750-8×1 SC40","m",{"v":1470,"d":"1470.00"}]
[10,"其他辅助配材费用","项",{"v":1,"d":"1.00"},null,null,"总价，见井房布置图"]
["六","临时工程"]
["1","施工房屋工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["2","其他临时工程","项",{"v":1,"d":"1.00"},null,null,"总价"]
["合计"]
[]
["投标人：",{"$nulls":5},"(盖章)"]
["法定代表人或委托代理人：",{"$nulls":5},"(签字)"]
[{"$nulls":3},"             年             月             日"]