{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["2-2建筑工程分类分项工程量清单计价表","2-4措施项目清单计价表","2-5其他项目清单计价表","安全文明措施费分解表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"2-2建筑工程分类分项工程量清单计价表","index":0,"n_rows":71,"n_cols":8,"rows_kept":71,"merged":[[0,0,1,7],[2,0,2,7],[3,0,3,7],[4,0,4,5],[4,6,4,7],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7]],"flags":["formulas_cached_only"]}
["建筑工程分类分项工程量清单计价表"]
[]
[]
["合同编号:XY-MLQ、YHQ-FHYX-SG"]
["工程名称:新沂市合沟沂河大桥防洪影响补偿工程",{"$nulls":5},"第1页 共2页"]
["序号","项目编码","项目名称","计量单位","工程数量","单价（元）","合价（元）","主要技术条款编码"]
[]
["1","5001","水利建筑工程",null,0]
["1.1","500101","土方开挖工程",null,0]
["1.1.1","500101001","场地平整",null,0]
["1.1.1.1","500101001001","场地平整","m2",{"v":4800,"d":"4800.000"}]
["1.1.2","500101002","一般土方开挖",null,0]
["1.1.2.1","500101002001","一般土方开挖\r\n（东侧滩地岸坡土方）","m3",{"v":1000,"d":"1000.000"}]
["1.1.3","500101004","沟、槽土方开挖",null,0]
["1.1.3.1","500101004001","沟、槽土方开挖","m3",{"v":690.9,"d":"690.900"}]
["1.2","500103","土石方填筑工程",null,0]
["1.2.1","500103010","石料抛投",null,0]
["1.2.1.1","500103010003","石料抛投","m3",{"v":700,"d":"700.000"}]
["1.2.2","500103014","土工合成材料铺设",null,0]
["1.2.2.1","500103014001","土工合成材料铺设\r\n土工布，300g/m2","m2",{"v":4920,"d":"4920.000"}]
["1.3","500104","疏浚和吹填工程",null,0]
["1.3.1","500104001002","船舶疏浚","m3",{"v":60100,"d":"60100.000"}]
["1.3.2","500101002002","一般土方开挖（疏浚土方）\n装车、运输5km","m3",{"v":60100,"d":"60100.000"}]
["1.4","500105","砌筑工程",null,0]
["1.4.1","500103007","垫层料填筑",null,0]
["1.4.1.1","500103007001","垫层料填筑\r\n碎石","m3",{"v":352,"d":"352.000"}]
["1.4.1.2","500103007002","垫层料填筑\r\n粗砂","m3",{"v":352,"d":"352.000"}]
["1.4.2","500105003","浆砌块石",null,0]
["1.4.2.1","500105003001","浆砌块石\r\n2.砂浆强度等级及配合比:M10水泥砂浆","m3",{"v":636,"d":"636.000"}]
["1.4.3","500105007","干砌混凝土预制块",null,0]
["1.4.3.1","500105007001","干砌混凝土预制块\r\n12cm自锁式生态砖","m2",{"v":4920,"d":"4920.000"}]
["1.5","500109","混凝土工程",null,0]
["1.5.1","500109001","普通混凝土",null,0]
["1.5.1.1","500109001001","普通混凝土（格埂）\r\n4.级配、拌制要求:C25商品砼","m3",{"v":408.96,"d":"408.960"}]
["1.6","500110","模板工程",null,0]
["1.6.1","500110001","普通模板",null,0]
["1.6.1.1","500110001001","普通模板（格梗木模板）","m2",{"v":500,"d":"500.000"}]
["1.7","500114","植草护坡",null,0]
["1.7.1","500114001","护坡","m2",0]
["1.7.1.1","500114001001","坡面播撒狗牙根草籽","m2",{"v":7100,"d":"7100.000"}]
{"$rows_empty":30}
[null,null,"合计",null,0,0]

{"sheet":"2-4措施项目清单计价表","index":1,"n_rows":43,"n_cols":3,"rows_kept":43,"merged":[[0,0,1,2],[2,0,2,2],[3,0,3,2],[4,0,4,1],[5,0,6,0],[5,1,6,1],[5,2,6,2]],"flags":["formulas_cached_only"]}
["措施项目清单计价表"]
[]
[]
["合同编号:XY-MLQ、YHQ-FHYX-SG"]
["工程名称:新沂市合沟沂河大桥防洪影响补偿工程",null,"第1页 共1页"]
["序号","项目名称","金额（元）"]
[]
["1","环境保护措施"]
["2","安全文明措施",30290.43]
["3","临时工程",0]
["4","交通工程",0]
["5","保险费"]
["6","大型施工机械安拆"]
["7","施工场外交通"]
["8","施工场外供电及通信"]
["9","施工房屋"]
["10","其他临时工程（疏浚土方堆放）"]
{"$rows_empty":25}
[null,"合计"]

{"sheet":"2-5其他项目清单计价表","index":2,"n_rows":44,"n_cols":4,"rows_kept":44,"merged":[[0,0,1,3],[2,0,2,3],[3,0,3,3],[4,0,4,2],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3]],"flags":["formulas_cached_only"]}
["其他项目清单计价表"]
[]
[]
["合同编号:XY-MLQ、YHQ-FHYX-SG"]
["工程名称:新沂市合沟沂河大桥防洪影响补偿工程",null,null,"第1页 共1页"]
["序号","项目名称","金额（元）","备注"]
[]
["1","预留金",{"v":100762.927,"d":"100762.93"}]
{"$rows_empty":35}
[null,"合  计"]

{"sheet":"安全文明措施费分解表","index":3,"n_rows":54,"n_cols":9,"rows_kept":54,"merged":[[0,0,0,8],[1,0,1,7],[2,0,2,7],[3,5,3,6],[3,7,3,8],[4,5,4,6],[4,7,4,8],[5,5,5,6],[5,7,5,8],[6,5,6,6],[6,7,6,8],[7,5,7,6],[7,7,7,8],[8,5,8,6],[8,7,8,8],[9,5,9,6],[9,7,9,8],[10,5,10,6],[10,7,10,8],[11,5,11,6],[11,7,11,8],[12,5,12,6],[12,7,12,8],[13,5,13,6],[13,7,13,8],[14,5,14,6],[14,7,14,8],[15,5,15,6],[15,7,15,8],[16,5,16,6],[16,7,16,8],[17,5,17,6],[17,7,17,8],[18,5,18,6],[18,7,18,8],[19,5,19,6],[19,7,19,8],[20,5,20,6],[20,7,20,8],[21,5,21,6],[21,7,21,8],[22,5,22,6],[22,7,22,8],[23,6,23,8],[24,0,24,8],[25,0,25,7],[26,0,26,7],[27,5,27,6],[27,7,27,8],[28,5,28,6],[28,7,28,8],[29,5,29,6],[29,7,29,8],[30,5,30,6],[30,7,30,8],[31,5,31,6],[31,7,31,8],[32,5,32,6],[32,7,32,8],[33,5,33,6],[33,7,33,8],[34,5,34,6],[34,7,34,8],[35,5,35,6],[35,7,35,8],[36,5,36,6],[36,7,36,8],[37,5,37,6],[37,7,37,8],[38,5,38,6],[38,7,38,8],[39,5,39,6],[39,7,39,8],[40,5,40,6],[40,7,40,8],[41,5,41,6],[41,7,41,8],[42,5,42,6],[42,7,42,8],[43,5,43,6],[43,7,43,8],[44,5,44,6],[44,7,44,8],[45,5,45,6],[45,7,45,8],[46,5,46,6],[46,7,46,8],[47,5,47,6],[47,7,47,8],[48,5,48,6],[48,7,48,8],[49,5,49,6],[49,7,49,8],[50,5,50,6],[50,7,50,8],[51,5,51,6],[51,7,51,8],[52,0,52,8],[53,6,53,8]],"flags":["formulas_cached_only"]}
["安全文明措施费分解表"]
["合同编号:XY-MLQ、YHQ-FHYX-SG"]
["工程名称:新沂市合沟沂河大桥防洪影响补偿工程",{"$nulls":7},"第1页 共2页"]
["一","完善、改造和维护安全防护设施设备","元",""]
["1","现场临时用电防护","元","",{"$nulls":3},"用电保护；高压区和用电危险区防护和围挡"]
["2","洞口、临边防护","元","",{"$nulls":3},"洞口、临边等危险部位防坠、防滑设施；临时防护盖板或围栏和隔离防护层"]
["3","机械设备防护","元","",{"$nulls":3},"钢防护网罩、防护挡板、防护栏杆等安全防护"]
["4","高处作业防护","元","",{"$nulls":3},"防止物体、人员坠落而设置的安全网、防护棚、防护栏杆、警戒线"]
["5","交叉作业防护","元","",{"$nulls":3},"平面、立面交叉作业时的防护"]
["6","防火、防爆、防尘、防毒","元",""]
["7","防雷、防台风、防地质灾害","元",""]
["8","地下工程有害气体监测、通风","元",""]
["9","临时安全防护","元","",{"$nulls":3},"围堰安全监测、防护，高脚手、高立模安全防护"]
["10","安全警示标志","元","",{"$nulls":3},"警告、提醒、指令、指示等标志、标牌；示警灯、报警闪光灯、夜间警示灯、照明灯"]
["二","配备、维护、保养应急救援器材、设备和应急演练","元",""]
["1","配备、维护、保养应急救援器材、设备","元","",{"$nulls":3},"应急救援器材、设备的配备、维护、保养和更新"]
["2","应急演练","元",""]
["三","重大危险源和事故隐患评估、监控和整改","元",""]
["1","重大危险源评估、监控与管理","元",""]
["2","事故隐患排查、评估和整改","元",""]
["四","安全文明生产检查、评价、咨询和标准化建设","元","",{"$nulls":3},"安全文明生产检查、评价、咨询和标准化建设持续改进等。不含企业安全生产标准化等级创建过程中给予咨询评价机构的评价咨询费用"]
["五","配备和更新现场作业人员安全防护用品","元","",{"$nulls":3},"必须配备的安全防护用品及对安全防护用品的正常损耗进行必要补充"]
["六","安全文明生产宣传、教育、培训","元","",{"$nulls":3},"安全文明宣传活动、标语、展板、音像、图片资料等；安全技术交底、安全操作规程培训、安全知识教育；知识竞赛、技能竞赛、专题会议；经验交流、现场观摩"]
[{"$nulls":6},"【新点水利软件江苏版 V10.3.4】"]
["安全文明措施费分解表"]
["合同编号:XY-MLQ、YHQ-FHYX-SG"]
["工程名称:新沂市合沟沂河大桥防洪影响补偿工程",{"$nulls":7},"第2页 共2页"]
["序号","项目名称","计量单位","数量","单价（元）","合价（元）",null,"备注"]
["七","安全文明生产适用的新技术、新标准、新工艺、新装备的推广应用","元"]
["八","安全设施及特种设备检测检验","元",""]
["九","文明施工、生活设施和环境的改善、运行和维护","元",""]
["1","现场布置","元","",{"$nulls":3},"现场围挡、五板一图、企业标志"]
["2","办公和生活设施","元","",{"$nulls":3},"施工现场办公、生活区与作业区分开设置，保持安全距离；设施符合卫生和安全要求；文体卫生设施配备"]
["3","现场管理","元","",{"$nulls":3},"场容场貌；工地地面硬化处理等；材料堆放；扬尘控制；垃圾清运；环境美化、绿化；现场保洁"]
["十","其他与安全文明施工直接相关的内容","元","",{"$nulls":3},"含廉政建设费用"]
[null,"总计",null,""]
{"$rows_empty":17}
[{"$nulls":6},"【新点水利软件江苏版 V10.3.4】"]